Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
00B5 | Error/Warning |
Description:
CPU: Inputparameter out of range in syntax. Leads to a hang-up in combination with CU release 3.x if FU_HI (Human Interface) firmware < 4512-113-20524. Causes a warning entry with CU release 2,but does not disturb application.
Possible Causes / Advice:
Fixed with FU_HI firmware 4512-113-20524 for release 2 + 3 generators. If CU release is still at 3.2 and FU_HI (Human Interface) firmware is still at 4512-113-20523 a PREP wakes up the generator. Check if FCO 00 135 006 has been carried out. This error is solved in R3.5 SW with FCO 74200002 and includes the latest FU_HI firmware. This FCO is "Retrofit on Failure" so it will not automatically come to the site.