Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
00L2 | Error/Warning |
Description:
GC: data access error Tube calculation data might have changed during start-up or service work online with the PC. Parts of the tube data might be missing after tube data loading process to the generator.
Possible Causes / Advice:
A defective filament (data corruption) will be taken from the APR data at Duo Diagnost systems with Optimus C, the remaining filament is automatically set for all APR in ADAM,after tube load and adaptation the assignment filament<>APR is back to normal. CAN connected systems: EZX42+EZX43 must be removed during the loading process. Thoravision and Digital Diagnost: signal bus EZX23 must also be removed to avoid reset commands of the SUN. Signal bus EZX23 must be removed anyhow for adaptation. Such measures are not required for Optimus C and non-system-CAN systems. If this error occurs during APR programming then install R3.5 SW with FCO 74200002. This FCO is "Retrofit on Failure" so it will not automatically come to the site.