Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
DS_BV_SG
Dose signal ramp of image intensifier signal EZX61:7 - EZ139X2:A17 backpanel version 4512 108 05983/4 (II/TV_adapter_PCB_X1:R-X2:2)-EZX61:2 - EZ139X2:A17 backpanel version 4512 108 09361/2 0...10V, polarity positive differential signal with DS_BV_NG release 3 generators only release 2 generators: not used, no function part of: dose rate control