Important!

In case of downgrading MRC type to e.g. MRM type:

1. First deselect the MRC tube type by selecting: empty string

2. Disconnect the tube physically

3. Install the new MRM tube

4. Configure the required MRM tube in this menu

Film Screen Combination adjustment:

Select the Film; Screen; Cassette; and Chamber-type from the selection menu.

If you cannot select the right FSC get the lateset information from the "Intranet"

http:// technet.best.ms.philips.com/

and select the page: Radiography/ Documents/ image performance and select Radiographic screens and films (pdf file)

and carry out the manual FSC programming.