## FU - mA read status trace

##### table (focus number FU-mA)

|  | filament converter PCB | focus number
| focus number FU-mA | FU-mA EZ119 | CU EZ139 (0...8 = max 9)
1 | large focus tube 1 | filament circuit 2 | focus number 2
2 | small focus tube 1 | filament circuit 1 | focus number 0
3 | large focus tube 2 | filament circuit 2 | focus number 5
4 | small focus tube 2 | filament circuit 1 | focus number 3
5 | large focus tube 3 | filament circuit 2 | focus number 8
6 | small focus tube 3 | filament circuit 1 | focus number 6

##### Read status Trace |  | Displays the last 10 activities with FU_mA. All fields have several entries possible. details to be continued
time |  | relative time [ms] of the last 10 status changes
foc |  | see table (‘focus number FU-mA’)
old sta |  | old static condition before status change
old dyn. |  | old dynamic condition before status change
signal |  | status change command
new sta |  | new static condition after status change
new dyn. |  | new dynamic condition after status change