Explanation:

With this function user can switch on/off three different types

of monitoring of the generator. They are: TTS monitoring,

Interface monitoring and CU Process monitoring. There are

also two checkboxes, that are used to enable/disable writting

of incoming data into the trace log and their their presentation

in separate window. By default, trace log is deactivated, and

presentation in window is activated.