Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
00E0 | Error/Warning |
Description:
iRMX exception #2#1H occurred. Appears if a desk key has been pushed after erasing APR data without a reset afterwards, might appear if data sets can not be downloaded due to unknown data mismatch.
Possible Causes / Advice:
If 00E0 appears during APR loading erase CU memory by setting the battery jumper to the off position for at least 5 minutes, put it back to ON, then start programming from scratch, better not use existing CU Complete download file, it might carry the problem. Memory Quick Erase Procedure