### Internal CAN Configuration

This screen displays the actual status of the assigned members on the internal generator CAN. The CU as main controller of the generator is not part of this list.

b = basic unit, must be in

o = option

FU kV: | [ | ] | b | kV_control EZ130
FU mA a: | [ | ] | b | mA_control EZ119
FU mA b: | [ | ] | o | 2nd mA_control, not available
FU mA c: | [ | ] | o | 3rd mA_control, not available
FU mA d: | [ | ] | o | 4th mA_control, not available
FU CIE: | [ | ] | b | C entral Interface Extension = Basic interface EZ150
FU HI a: | [ | ] | o | H uman Interface = operating desk CPU C300
FU HI b: | [ | ] | o | 2nd operating panel, not available
FU RC a: | [ | ] | o | high speed Rotor Control EY100
FU RC b: | [ | ] | o | 2nd high speed rotor control, not available
FU RC c: | [ | ] | o | 3rd high speed rotor control, not available
FU AD a(1WA): | [ | ] | o | adapter for 4 aux. units WA (Bucky/Tomo) 1WA102
FU AD b(2WA): | [ | ] | o | adapter for 4 aux. units WA (Bucky/Tomo) 2WA102
FU AD c(1WB): | [ | ] | o | adapter for 4 aux. units WB (R/F and Bucky) 1WB102
FU AD d(2WB): | [ | ] | o | adapter for 4 aux. units WB (R/F and Bucky), not available
FU MDO: | [ | ] | o | monitor data overlay, not available
| [01] | = | no response from basic unit
| [ 2] | = | unit (basic and optional) on CAN member list and ok
| [F0] | = | optional unit in CAN member list, but no response during turn-on
| [FF] | = | optional unit not present, FF also appears if a unit is physically installed but has not yet been assigned