Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
02HE | Warning |
Description:
kV actual value too large during transition standby to exposure > 3kV at > 400ms after PREP
Possible Causes / Advice:
With a PC and XRGSCOPE: select error # from error log index list, select error details and read screen Error: Specific Information to get the faulty value. Monitor with an oscilloscope at: EZ130 X3 AVHT 20kV/V trigger: EN_X/ EZX82 Check signal connections EZ130 to HT measuring circuit EG100. HT_AN & HT_AN_GND HT_CA & HT_CA_GND Check supply voltages EZ130 + 5V X2:AC1 X2:AC2 +15V X2:AC11 - 15V X2:AC12 +26V X2:AC14 against ground X2:AC15 If values indicated at the detail screens do not match the externally measured ones exchange PCB.