Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
10LH | Error / Warning |
Description:
intermediate current too high FU_RC 4512 104 71401...6 with Firmware 4512-113-22311/12 stator phase current too high FU_RC 4512 104 71421/61 with Firmware 4512-113-22322
Possible Causes / Advice:
Check system with High Speed RoCo Replacement procedure. With Rotor Control FU_RC 4512-104-71421/61: Compare stator currents with the High Speed RoCo waveforms page.