Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
02HL | Error |
Description:
E value (converter DC) during high tension out of range: <350 V or >800 V 3 detections within 30 ms
Possible Causes / Advice:
With a PC and XRGSCOPE: select error # from error log index list, select screen Error: HW Read Values to get the faulty value. Monitor with oscilloscope at - EZ130 X1:A5 & X1:C5 24V = 750V (E value) frontal converter EQ (measuring point for all release 2 generators and all 50kW generators with one converter only) OR Monitor with oscilloscope at - EZ130 X1:A26 & X1:C26 24V = 750V (E value) rear converter E2Q (all release 3 generators with 2 converters) Check supply voltages EZ130 + 5V X2:AC1 X2:AC2 +15V X2:AC11 - 15V X2:AC12 +26V X2:AC14 against ground X2:AC15 If values indicated at the detail screens do not match the externally measured ones exchange PCB.