Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
02HC | Warning |
Description:
Z nominal value out of range +/- 1% +/- 0.2 3 measurements within 30ms duty cycle range Z = 3...30%
Possible Causes / Advice:
With a PC and XRGSCOPE: select error # from error log index list, select error details and read screen Error: HW Set Values to get Z nominal, then read Error: Specific Information to get the faulty value. Check supply voltages EZ130 + 5V X2:AC1 X2:AC2 +15V X2:AC11 - 15V X2:AC12 +26V X2:AC14 against ground X2:AC15 If all supplies OK replace PCB