Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
E_NG_CV2
E value converter DC supply negative converter 2 (rear 65/80kW): E2Q100X1:5 - EZX34:5 - EZ130X1:C26 no input to EZ130 release 2 generators release 3 generators only with 2 converters 0...-12V = 0...-375V if converter is stand-alone (E2Q X1 not connected) if in normal operation: E_PO + E_NG >> 445VDC = 10V measuring input EZ130 X1:A26 - X1:C26