Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
CAN_H
Generator CAN high active. EZ119X2:C3 - EZ130X2:C3 - EZ139X2:C3 - EZ150X2:C3 - EZX44:10 - EZX45:10 - EZX46:10 -- C300X1:10 - EZX51:3 - EZX151:3 - EZX52:7 - EZX72 --EWAX51:10 - EWAX52:10 - EWA100X2:C3 - EWBX51:10 - EWBX52:10-EWB100X2:C3- +2.5VDC standby, +3.2VDC during communication EZX72 for communication of generator function units only part of: XRG bus.