### Tube Temperature Supervision Temperature Log

The tube temperatures are supervised by the TTS calculation model.

Every second the temperatures are re-calculated and updated in this table.

Overload flags (see part: 23456) are tube and housing type dependent.

Tables disappear with switch off, but actual temperatures will be calculated and updated during switch on or warm start.

All temperatures should be at 20ºC (basic value) after a long switch-off period.

04/ X-SEGMENT: Tube Temperature Table

temperature in degrees centigrade overload at

time tube T(2) T(3) T(4) T(5) T(6) part: 23456

8193 1 20.0 20.0 20.0 20.0 20.0 0 0 1 0 0 0 0 0 (see table (Overload Bit) below)

(condition after turn-on, long time no working)

time time table in seconds

tube tube number (1...3)

T(2) focal spot temperature

T(3) focal track temperature (outer anode circuit)

T(4) anode disk temperature (inner anode circuit)

T(5) rotor temperature

T(6) oil temperature

Table (Overload Bit)

0 | 0 | 1 | 0 | 0 | 0 | 0 | 0
yellow | red | 1 = standby 0 = exposure | T(2) | T(3) | T(4) | T(5) | T(6)
traffic light condition: | 0 = temperature value within the max limit
green | = | 0 0
green + yellow | = | 0 0
yellow | = | 1 0 | 1 = temperature value increased max limit
yellow + red | = | 1 1
red | = | 1 1