External APR Assignments

Device Interface 1 only possible, if 'Release circuit adaptation unit' is programmed as

1WA unit (jumper W1/W2/W3 open at WA backpanel)

RGDV key 1: position 1 RGDV key 2: position 2 APR key 1...6 (0 = no APR): positions 3...8 | 1 | 2
3 | 4
5 | 6
7 | 8

The 'RGDV key 1/2' positions can be programmed with any of the active RGDV's. Six
APR of every active RGDV can be assigned to the six buttons 3...8. To get the 'APR
key' numbers use 'Select APR'.
The APR numbers must be entered at the RGDV # where they are assigned to. The two programmed RGDV keys appear at all RGDV screens.
If an assigned RGDV and/or an assigned APR is selected at the control desk, the
RGDV/APR button will light up at the external APR module and vice versa.

Device Interface 2 only possible, if 'Release circuit adaptation unit' is programmed as

2WA unit (jumper W1closed, W2/W3 open at WA backpanel)

APR key 1...8 (0 no APR): positions 1..8 = keys 1..8

8 APR of each active RGDV can be assigned to the 8 APR keys ( >> max 64 !!).
It is recommended to use one RGDV only.
If an assigned APR is selected at the control desk, the APR button will light up at the
external APR module and vice versa.

Note: Device Interface 3 not existing for Rel. 2.x OPTIMUS generators

Device Interface 3 only possible, if 'Release circuit adaptation unit' is programmed as

1WB unit (jumpers W1/W3 open, W2 closed at WB backpanel)

With the RGDV key 1 and RGDV key 2 assignment the RGDV remote switch over
inputs WB X21 pin 1 and 2 will be activated. The selected RGDV must get a low signal
from the R/F controller, while the other RGDV signal must go high.

!! Both keys must be programmed.

8 APR of each activated RGDV can be assigned to the 8 APR keys (e.g. SCOPO)

(max 64 !!).

It is recommended to use one RGDV only.

If an assigned APR is selected at the control desk, the APR button will light up in the

external APR module and vice versa.