Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
DR_TV_NG
Dose rate of TV chain signal negative, fluoro control (II/TV_adapter_PCB_X3:1 - X2:8) - EZX61:8 - EZ139X2:C19 backpanel version 4512 108 09361/2 +/-12V minus polarity dual voltage differential signal typically +6V in standby coming from TV chain +V for more dose, -V for less dose, 0V stable image part of: dose rate control