Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
00TH | Warning |
Description:
TTS (Tube Temperature Supervision): Load Data Supply inconsistent
Possible Causes / Advice:
If this error occurrs in during tube adaption see Service Recommedation 00 135 016 If this error only occurs during fluoro it can be ignored. This will be fixed in R3.5.