Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
02WJ | Error |
Description:
kV over voltage detected
Possible Causes / Advice:
With a PC and XRGSCOPE: select error # from error log index list, select error details and read screen Error: HW Set Values to get KV nominal, then read Error: Read HW Values to get the faulty value. Connect an oscilloscope to EZ130 X1:C17 (HT_AN ) and EZ130 X1:C16 (HT_CA) (10KV/V)and monitor the KV waveform at the input to the EZ130. Trigger = EZX74 (CTRL_X_C) OR Connect an oscilloscope to EZ130:X3 (AV_HT_AN ) and EZ130:X4 (AV_HT_CA) (20KV/V)and monitor the KV waveform at the output of the EZ130.Trigger = EZX74 (CTRL_X_C)