Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
03HG | Warning |
Description:
Filament current (If) actual out of tolerance
Possible Causes / Advice:
Check high tension cable cathode plug pins at generator and tube side. With a PC and XRGSCOPE: Select error # from error log index list, select error details, and read screen Error: Read HW Values to get the setpoint and the faulty value. fil. circuit 1 = small focus fil. circuit 2 = large focus Monitor with oscilloscope at: EZ119 X5 = small focus EZ119 X7 = large focus 1V = 2.5A filament current Mains phase 2 present? Try HT cable exchange if the actual ones very old / suspicious. Check supply voltages EZ119 + 5V X2:AC1 X2:AC2 +15V X2:AC11 - 15V X2:AC12 +26V X2:AC14 against ground X2:AC15 If values indicated at the detail screens do not match the externally measured ones exchange PC