Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Error Code: | Type: | Segment:
02WH | Error |
Description:
tube arcing detected
Possible Causes / Advice:
With a PC and XRGSCOPE: select error # from error log index list, select screen Error: HW Set Values to get KV nominal. Switch an exposure with this value and monitor kV actual value signal at EZ130 X5 and compare waveform against the arcing waveforms. Carry out tube conditioning procedure to improve tube behavior.