### Tube Statistic

#### Optimus RAD/RF Rel. ≥ 3.5 & Optimus C Rel. ≥ 1.2

#### Reset Tube Statistic

A screen "Start function: reset tube statistic" comes up. Hit <ENTER> to reset the tube statistic data table.

# Note

# This “reset tube statistic” procedure should be carried out after tube exchange.

#### Type of Tube 1...3

Tube name + housing type as programmed from the tube data file.

Empty field: no tube programmed.

#### Tube 1...3 Statistic

reset date: | [ DD.MM.YY | ]
= date of the last reset (initial, tube exchange) |  |
last update: | [ DD.MM.YY | ]
= date of the last table entry |  |
preparation time large focus [s]: | [ | ]
preparation time small focus [s]: | [ | ]
preparation time vario focus [s]: | [ | ]
preparation counter large focus: | [ | ]
preparation counter small focus: | [ | ]
preparation counter vario focus: | [ | ]
fluoro time [min]: | [ | ]
fluoro counter: | [ | ]
exposure counter large focus: | [ | ]
exposure counter small focus: | [ | ]
exposure counter vario focus: | [ | ]
overload exposure counter large focus: | [ | ]
overload exposure counter small focus: | [ | ]
overload exposure counter vario focus: | [ | ]

#### Optimus RAD/RF Rel. ≤ 3.3 & Optimus C Rel. ≤ 1.

#### Tube 1...3

for Optimus C only tube 1 applicable

exposure counter: displays the number of exposures

fluoro counter : displays the number of fluoro requests

#### Type of Tube 1...3

Tube name + housing type as programmed from the tube data file.

Empty field: no tube programmed.