Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
Fuctional Units
HEX | Mnemonic | Description
00 | CU | Central Unit -EZ139
01 | FU_DRC | The Dose Rate Control (fluoro) is physically located on the EZ139. For amplimat exposures the EZ139 and parts of the EZ150 (basic interface) are involved.
02 | FU_KV | KV Control - EZ130
03 | FU_mA | mA Control - EZ119 Handles 2 filaments for up to 3 tubes.
07 | FU_CIE | Central Unit Extension - EZ150 Basic Interface, also drives low speed rotor control
08 | FU_HI | Human Interface - C300 Control Desk
0A | FU_RC | Rotor Control (High Speed / Dual Speed) EY100
0D | FU_ADAPT_a | Adapter decade cables for 4 aux units RAD = WA102 or 1WA102
0E | FU_ADAPT_b | Adapter decade cables for 4 aux units RAD = 2WA102
0F | FU_ADAPT_c | Adapter decade cables for 4 aux units RF = WB102