Home Bucky Controller EZ Diagnost Duo Diagnost Omni Diagnost D76 / D76+ Optimus SCP Medio DSI CPE PFCo |
Optimus
EN_X_C/
Enable X-ray, internal generator signal preparation or fluoro request if confirmed by CAN message (RAD-R/F) or hardware requests (Optimus C) EZ119X2:C7 - EZ130X1:C7 - EZ130X2:C7 - EZ139X2:C7 - EZ150X2:C7 - EZX52:9 - EZX76 0V/+5V low active measuring point EZX76 driven by CU if EN_X/ active (low) part of: XS/XRG bus