;语言文件格式为: 名称|中文|英文，竖线分割，逗号与分号为注释，///为换行，空行自动忽略
;Language file format: Name|Chinese|English，vertical is delimiter， comma or semicolon is Comments，///is newline，Empty lines automatically ignored
 
lang_Main_Title|USR-M0 系列|USR-M0 Series
lang_Main_AppTitle|USR-M0 系列|USR-M0 Series
lang_Menu_File|文件|File
lang_Menu_Pswd|用户名密码设置|User config
lang_Menu_Quit|退出|Quit
lang_Menu_Lang|Language|Language
lang_Menu_Cn|简体中文|简体中文
lang_Menu_En|English|English
lang_Menu_Diy|DiyLang|DiyLang
lang_Menu_Help|帮助|Help
lang_Menu_About|关于...|About...
lang_Menu_Hint|实时帮助|Real-time Help
lang_Menu_Version|检查更新|Latest version
lang_Menu_WorkOrder|提交问题|Work Order
lang_Menu_DownUrl|http://www.usr.cn/Download/230.html|http://www.usriot.com/Download/237.html
lang_Lv_DevIP|设备IP|Device IP
lang_Lv_DevName|设备名称|Device Name
lang_Lv_MAC|MAC地址|MAC
lang_Lv_Version|版本|Version
lang_lblKNum|请选择设备型号|Select Model Type
lang_lbl_SelectCom|请选择串口|Select serial port
lang_NoCom|没有串口|No serial port
lang_mni_CopeAllMac|复制所有MAC|Cope All Mac
lang_mni_CopyTheMac|复制选中MAC|Copy The Mac
lang_mni_FirmwareUp|固件升级|Firmware upgrade
lang_mni_OpenWeb|打开网页|OpenWeb
lang_mni_Reset|恢复出厂设置|Reset
lang_mni_Restart|重启设备|Restart
lang_btn_Search|搜索设备|Search Device
lang_btn_ComSet|保存参数|Save Config
lang_btn_ComRead|读取参数|Read Config
lang_rztbsht_Net|通过网络操作|Operate Via LAN
lang_rztbsht_Com|通过串口操作|Operate Via COM
lang_rztbsht_Log|操作日志|Operation Log
lang_rztbsht_Hex|数据流|Hex Streams
lang_grp_Param|常规功能|General functions
lang_grp_Special|扩展功能|Expand functions
lang_grp_BaseSave|基础设置 (不带★的一般保持默认)|Base Param (which is without ★,usually keep default)
lang_grp_ComParam|端口设置|Port Param
lang_InputBdTitle|自定义波特率|Diy Baud Rate
lang_PlsInputBd|请输入波特率：|Please Input your Baud Rate :
lang_BaudRate_Custom|自定义|Custom
lang_Lbl_UPNPPort|UPNP端口|UPNP Port
lang_Lbl_HTTPPort|HTTP服务端口|HTTP Port
lang_Lbl_DevID|设备ID|Device ID
lang_Lbl_DevIDType|设备ID类型|Device ID Type
lang_Lbl_UserName|用户名|User Name
lang_Lbl_Password|密码|Password
lang_Lbl_DevName|设备名称|Device Name
lang_Lbl_MAC|用户MAC地址|User MAC
lang_Lbl_IPType|IP地址类型|IP Type
lang_Lbl_StaticIP|模块静态IP|ModuleStaticIP
lang_Lbl_Gateway|网关|Gateway
lang_Lbl_SubnetMask|子网掩码|SubnetMask
lang_Lbl_Baudrate|串口波特率|Baudrate
lang_Lbl_PDS|校验/数据/停止|Parity/Data/Stop
lang_Lbl_FlowControl|串口流控制|FlowControl
lang_Lbl_LocalPort|本地端口|Local Port
lang_Lbl_RemotePort|远程端口|Remote Port
lang_Lbl_WorkMode|模块工作方式|Module work mode
lang_Lbl_TCPSvrCount|TCP Server 连接数|Tcp connect num
lang_Lbl_TCPStyle|TCP Server 样式|TCP Server style
lang_Lbl_ModbusTCP|ModbusTCP|ModbusTCP
lang_Lbl_RemoteIP|目标IP/域名|RemoteIP
lang_Lbl_TelnetTimeout|网络重连时间|Telnet Timeout
lang_Lbl_PackTime|串口打包时间|PackTime
lang_Lbl_PackLen|串口打包长度|PackLen
lang_Chkbox_RFC22170|同步波特率(类RFC2217)|Synchronize baudrate(RFC2217 similar)
lang_Lbl_InfoTimeOut|秒     (<256, 0为不使用)|s  (<256, 0 for no uses)
lang_Lbl_InfoPackTime|毫秒 (0~255)|ms (0~255)
lang_Lbl_InfoPackLen|字节 (0~1023)|byte (0~1023)
lang_Cbb_DHCP|DHCP/动态IP|DHCP/Auto IP
lang_Cbb_StaticIP|静态IP|Static IP
lang_Cbb_Transparent|透明传输|Transparent transmission
lang_Cbb_NoIDDiscard|按ID发送-无ID则丢弃|As ID(No ID discard)
lang_Cbb_NoIDBroadcast|按ID发送-无ID则群发|As ID(No ID Broadcast)
lang_rzgrpbxCloudEn|启用透传云|Enable USR Cloud
lang_lblCloudId|设备编号|Device ID
lang_lblCloudPswd|通讯密码|Communication code
lang_lbl_ModuleIP|本模块IP地址|Module IP
lang_lbl_DeIP|连接目标IP|Destination IP
lang_chk_ConnSendId|建立连接后发送ID号|Send device ID when connected
lang_chk_DataWithId|发送数据时携带ID号|Send data with device ID
lang_H_btn_Search|搜索局域网内的设备,需要将CFG引脚悬空|Search device in LAN, please leave CFG pin free
lang_H_btn_ComRead|通过串口读取设备配置,需要将CFG引脚接地|Read device param via COM, please connect CFG to GND
lang_H_lv_Dev|点击搜到的设备可读取参数，右键点击设备列表显示更多功能|Click device can read the parameters, right-click Device list show more
lang_lbl_H_LocationURLPort| UPNP端口，一般用不着 | LocationURLPort /// In general ，it's useless 
lang_lbl_H_HTTPServerPort| 网页端口 | Webpage Port 
lang_lbl_H_Id| 设备ID必须与设备ID类型配合使用 | Device ID must be used with Device ID Type 
lang_lbl_H_IdType| 设备ID类型必须与设备ID配合使用 | Device ID Type must be used with Device ID 
lang_lbl_H_username| 网页登录与本软件配置的用户名与密码 | The user name and password for webpage login and the software configuration 
lang_lbl_H_password| 网页登录与本软件配置的用户名与密码 | The user name and password for webpage login and the software configuration 
lang_lbl_H_ModName| 设备名称，可修改 | Device Name ,it's revisable 
lang_lbl_H_UserMAC| MAC地址，可修改 | MAC address ,it's revisable 
lang_lbl_H_AddrType| 静态IP是使用固定IP地址，DHCP是由路由器分配动态的IP地址 | Static IP :  set a fixed IP address /// DHCP    :  get a dynamic IP address from router 
lang_lbl_H_StaticIP| 本模块静态IP地址可在指定网段内任意分配，但网内不允许重复 | Assign any IP address  for the module in the network , but the IP address isn't allowed to repeat
lang_lbl_H_GatewayIP| 网关，可以参看你电脑的网关IP，///一般是192.168.0.1，192.168.1.1，192.168.0.254这类。 | Default Gateway in your lan,/// you can look at pc‘s default getway,///it should be like 192.168.0.1 
lang_lbl_H_SubnetMask| 子网掩码：通常是255.255.255.0 | Subnet mask, the default is 255.255.255.0 
lang_lbl_H_BaudRate| 请选择或自定义波特率。我们确保每个模块都工作OK的波特率是115200///（我们的测试波特率和默认波特率）| Please select standard bandrate number or custom any bandrate. 
lang_lbl_H_PDS| 校验/数据/停止| Parity bits / data bits / stop bits  
lang_lbl_H_FlowControl| 默认为none，/// RS485代表开启485功能（RTS脚做收发控制），/// Hardware代表使用RTS/CTS硬件流控  | The default is none /// RS485 :use 485(RTS transceiver control) /// Hardware : use RTS/CTS hardware flow control
lang_lbl_H_LocalPort| 模块工作于UDP或TCPServer模式时将监听此端口 | When work at UDP mod or TCP Server mode, module will listen this port. 
lang_lbl_H_RemotePort| 服务器上的应用程序监听的端口号 | The port be listen at server software. 
lang_lbl_H_WorkMode| 模块工作方式选择：///UDP server 是指不验证来源IP地址，///收到UDP数据包后将目标IP改为数据来源IP，///类似TCP server的功能。 | module work mode: ///UDP server is like TCP server,when receive a UDP packet,///change target IP to sorce IP of the received UDP packet ///Does not verify the source IP. 
lang_lbl_H_TCPSvrCount| TCP Server下允许的最大客户端数量 | The number of allowed client when device is working at ' TCP Server ' WorkMode 
lang_lbl_H_TCPStyle| 一般选择透明传输 | Generally , please select transparent transmission 
lang_lbl_H_ModbusTCP| 请选择none，除非使用了Modbus TCP协议 |  , Please select 'none' , unless Modbus TCP is used 
lang_lbl_H_RemoteIP| 服务器的IP或者你要连接的计算机的IP | RemoteIP is the Server Ip or the PC ip which you want to link. 
lang_lbl_H_UARTTime| 当串口持续一定时间没有接到数据之后，当前的数据就会被打包发送出去。/// 打包时间跟打包长度共同作用，详见 http://www.usr.cn/Faq/6.html /// ★想禁用此功能，请将该值设为0★| When the serial port has not received a data for a certain time , /// the data will be packed and sent. /// PackTime and PackLen will working together./// More information is on http://www.usr.cn/Faq/6.html ///★ Want the feature disable , set it 0 ★
lang_lbl_H_UARTLength| 当串口收到的数据长度达到一定数量后，当前的数据就会被打包发送出去。/// 打包时间跟打包长度共同作用，详见 http://www.usr.cn/Faq/6.html /// ★想禁用此功能，请将该值设为0★ | When the data length of received through the serial port achieve the certain value , /// the data will be packed and sent. /// PackLen and PackTime will working together./// More information is on http://www.usr.cn/Faq/6.html ///★ Want the feature disable , set it 0 ★
lang_chk_H_RFC2217| 默认勾选，配合虚拟串口软件使用，/// 根据您的应用软件，动态改变串口服务器的串口参数。 | Ticked default , use it with 'USR-VCOM Virtual Serial Port Server'  /// Change the configure of Serial server dynamically based on your software 
lang_Hint_ModuleWork|模块工作方式选择：///UDP server 是指不验证来源IP地址，收到UDP数据包后将目标IP改为数据来源IP，类似TCP server的功能。|module work mode: ///UDP server is like TCP server,when receive a UDP packet,change target IP to sorce IP of the received UDP packet,Does not verify the source IP.
lang_Hint_ModuleIP|本模块IP地址可在指定网段内任意分配，但网内不允许重复。|Module IP can fill any ip in LAN, ///just remeber do not repeat.
lang_Hint_Mask|子网掩码：通常是255.255.255.0|Subnet mask, the default is 255.255.255.0
lang_Hint_Gateway|模块默认网关，可以参看你电脑的网关IP，///一般是192.168.0.1，192.168.1.1，192.168.0.254这类。|Default Gateway in your lan, ///you can look at pc's default getway, ///it should be like 192.168.0.1
lang_Hint_BaudRate|模块默认波特率为115200.波特率应该与串口服务器连接的串口设备波特率一致。选择第一项可弹出自定义波特率|The default baudRate is 115200,it should be same as baudRate of device which communicate with the module.You can select the first line to diy bandrate.
lang_Hint_PDS|校验位 / 数据位 / 停止位|Parity bits / Data bits / Stop bits
lang_Hint_ModulePort|模块工作于UDP或TCP Server模式时将监听此端口|When work at UDP mod or TCP Server mode,/// module will listen this port.
lang_Hint_DeIP|服务器的IP或者模块要连接计算机的IP，目标IP只对TCP client和UDP模式起作用。///发UDP广播时，将其设置为255.255.255.255，其广播端口在下面的【远程端口】处设置。|Destination IP is the Server Ip or the PC ip which you want to link.It only work in TCP client or UDP mod.///If you want to Broadcast,set it 255.255.255.255,and set the broadcast port in 【RemotePort】
lang_Hint_DePort|服务器上的应用程序监听的端口号|The port be listen at server software.
lang_Hint_NetDev|点击搜到的设备可读取参数，右键点击设备列表显示更多功能|Click device can read the parameters, right-click Device list show more
lang_Hint_ID|设备的ID，十进制表示，范围0~65535|Device ID in decimal, from 0 to 65535.
lang_Hint_RS485|开启485功能，默认勾选。不会对232通信造成影响|Use 485
lang_Hint_RS422|开启422功能|Use 422
lang_Hint_Reset|做TCP Client时，尝试30次连接Tcp Server失败，自动重启|The Device as a TCP Client, try to connect the TCP Server 30 times failure, automatic restart
lang_Hint_Link|开启Link脚指示TCP连接是否建立的功能，连接建立则输出低电平|Pin link to show if tcp has connected or not,f the connection is established, then the output low level
lang_Hint_Index|模块做TCP server时，使用index来区分多个tcp连接|TCP Server index,4.12 or above support this function
lang_Hint_RFC2217|类RFC2217功能，在网络端动态修改模块的串口工作参数，默认勾选|RFC2217 change baudrate in socket,4.13 support this function
lang_Hint_ComF5|点击可刷新显示本机所有串口|Click to refresh and show all serial port in the machine
lang_Hint_HexCopy|复制数据流|Copy Hex
lang_About_Title|关于|About
lang_About_Version|版本：|Version:
lang_About_OK|确 认|OK
lang_About_SoftName|名称：USR-M0 系列|Name:  USR-M0 Series
lang_About_Description|说明：本程序由济南有人物联网技术有限公司设计提供，用于对USR-TCP232-310产品的设置，本软件使用免费。|Instruction:  This software is design by Jinan usr IOT Technology Co., Ltd.Apply to USR-TCP232-310 product model.
lang_About_Contact|联系我们：|Contact Us:
lang_About_Website|http://www.usr.cn|http://www.usriot.com
lang_About_Tel|0531-88822739|0531-88822739
lang_About_Email|tec@usr.cn|tec@usr.cn
lang_Log_Title|用户名密码设置|User config
lang_Log_OK|确定|OK
lang_Log_Cancel|取消|Cancel
lang_Upgrade_Title|固件升级|Firmware Upgrade
lang_Upgrade_grpClnt| 目标选择 |Select Client
lang_Upgrade_grpFileName| 固件选择 |Select .bin file
lang_Upgrade_btnProgram|升 级|Program
lang_Upgrade_btnExit|退 出|Exit
lang_Upgrade_lblClientIP|目标IP地址：|Client IP Address:
lang_Upgrade_lblClientMAC|目标MAC地址：|Client MAC Address:
lang_ts_OK|完成| OK 
lang_ts_Send|发送|send
lang_ts_Read|读取|Read
lang_Hint_DevNum| 在线设备数：| On-line Device NUM:
lang_Hint_ACK| 正确执行。| ACK.
lang_Hint_CheckErr| 校验错误,正确的校验值为: | Check Error: it should be: 
lang_Hint_ReceiveOther| 接收未知数据,长度为: | Receive unknown,length is: 
lang_Hint_PswdErr| 用户名密码错误！请重新输入。| UsrName or Password Error!
lang_Hint_OtherErr| 其他错误。| Other Error.
lang_Hint_OverTime| 接收超时！| Receive over time.
lang_Hint_Sending|数据已发送| Data has been sent
lang_Hint_BeenRead| 数据读取完毕。| Data has been read.
lang_Hint_Searching| 搜索在线设备...| Search online Device...
lang_Hint_UDPPortChange| 搜索端口：| Search Port:
lang_Hint_UDPPortInUse| 端口被占用！| Port In Use!
lang_Hint_NoTarget| 请在搜索列表中选择模块。| Please select the module in the search list.
lang_Hint_UpSearching| 搜索可升级设备...| Searching device...
lang_Hint_UpReady| 已搜索到设备，发送升级请求...| Find Device,Ready to upgrade...
lang_Hint_UpProgress| 升级进度...| Upgrade progress...
lang_Hint_UpSuccess| 升级已完成，请恢复出厂默认。| Upgrade successful.please restore factory default.
lang_Hint_UpNoClient| 未选择升级目标。| Please Select Client first.
lang_Hint_UpNoFileName| 未选择升级文件。| Please Select .bin file first.
lang_Hint_Upfailed| 固件升级失败，请联系厂家！| Upgrade failed!
lang_Hint_UpTimeOut| 升级超时！| Upgrade time out!
lang_Hint_BinNotMatch| 固件与硬件不匹配！| Firmware does not match with hardware!
lang_Hint_UpPleaseUpgrade|本程序支持2002或更高版本，请先升级：设备->固件升级|This program supports version 2002 or higher, please upgrade first:Device->Firmware upgrade
lang_Hint_UpNoSamNetwork|请先设置模块与计算机在同一网段，否则无法升级。|Please set the module and the computer on the same network segment, otherwise unable to upgrade.
lang_Hint_VerIncompatible|本程序仅支持M0系列|This program is only used for M0 Series
lang_ts_CfgFree|CFG引脚需悬空|please leave CFG pin free
lang_ts_CfgGnd|CFG引脚需接地|please connect CFG to GND
lang_ComIsNo|串口不存在或被占用|Serial is Occupied
lang_ComIsOpen|串口已打开|Serial is Open
lang_ComIsClose|串口已关闭|Serial is Close
lang_Ts_ComSendFailure|串口发送失败，请重试|Serial Send Failure，please try again
lang_DataHeadOrChkErr|包头或校验错误|Packet Header error or check sum is not correct
lang_Ts_ComSetOk|设置成功|setup success
