display_name = "The 3DO Company - 3DO (4DO)"
authors = "JohnnyDude|FreeDO team|trapexit"
supported_extensions = "iso|bin|chd|cue"
corename = "4DO"
manufacturer = "Various"
categories = "Emulator"
systemname = "3DO"
systemid = "3do"
database = "The 3DO Company - 3DO"
license = "LGPL/Non-commercial"
permissions = ""
display_version = "v1.3.2.4+"
supports_no_game = "true"
firmware_count = 10

firmware0_desc = "panafz1.bin (Panasonic FZ-1 BIOS)"
firmware0_path = "panafz1.bin"
firmware0_opt = "true"
notes = "(!) panafz1.bin (md5): f47264dd47fe30f73ab3c010015c155b"

firmware1_desc = "panafz10.bin (Panasonic FZ-10 BIOS)"
firmware1_path = "panafz10.bin"
firmware1_opt = "true"
notes = "(!) panafz10.bin (md5): 51f2f43ae2f3508a14d9f56597e2d3ce"

firmware2_desc = "panafz10-patched.bin (Panasonic FZ-10 BIOS [RSA Patch])"
firmware2_path = "panafz10-patched.bin"
firmware2_opt = "true"
notes = "(!) panafz10-patched.bin (md5): 1477bda80dc33731a65468c1f5bcbee9"

firmware3_desc = "panafz10e-anvil.bin (Panasonic FZ-10E BIOS [Anvil])"
firmware3_path = "panafz10e-anvil.bin"
firmware3_opt = "true"
notes = "(!) panafz10e-anvil.bin (md5): a48e6746bd7edec0f40cff078f0bb19f"

firmware4_desc = "panafz10e-anvil-patched.bin (Panasonic FZ-10E BIOS [Anvil RSA Patch])"
firmware4_path = "panafz10e-anvil-patched.bin"
firmware4_opt = "true"
notes = "(!) panafz10e-anvil-patched.bin (md5): cf11bbb5a16d7af9875cca9de9a15e09"

firmware5_desc = "goldstar.bin (Goldstar GDO-101M BIOS)"
firmware5_path = "goldstar.bin"
firmware5_opt = "true"
notes = "(!) goldstar.bin (md5): 8639fd5e549bd6238cfee79e3e749114"

firmware6_desc = "sanyotry.bin (Sanyo Try IMP-21J BIOS)"
firmware6_path = "sanyotry.bin"
firmware6_opt = "true"
notes = "(!) sanyotry.bin (md5): 35fa1a1ebaaeea286dc5cd15487c13ea"

firmware7_desc = "3do_arcade_saot.bin (Shootout At Old Tucson BIOS)"
firmware7_path = "3do_arcade_saot.bin"
firmware7_opt = "true"
notes = "(!) 3do_arcade_saot.bin (md5): 8970fc987ab89a7f64da9f8a8c4333ff"

firmware8_desc = "panafz1-kanji.bin (Panasonic FZ-1 Kanji Font ROM)"
firmware8_path = "panafz1-kanji.bin"
firmware8_opt = "true"
notes = "(!) panafz1-kanji.bin (md5): b8dc97f778a6245c58e064b0312e8281"

firmware9_desc = "panafz10ja-anvil-kanji.bin (Panasonic FZ-10JA Kanji Font ROM)"
firmware9_path = "panafz10ja-anvil-kanji.bin"
firmware9_opt = "true"
notes = "(!) panafz10ja-anvil-kanji.bin (md5): 428577250f43edc902ea239c50d2240d"
