display_name = " 世嘉MS/GG/MD/CD模拟器 (Genesis Plus GX)"
authors = "Charles McDonald|Eke-Eke"
supported_extensions = "mdx|md|smd|gen|bin|cue|iso|sms|gg|sg|68k|chd"
corename = "Genesis Plus GX"
manufacturer = "Sega"
categories = "Emulator"
systemname = "Sega 8/16-bit (Various)"
systemid = "mega_drive"
database = "Sega - Game Gear|Sega - Master System - Mark III|Sega - Mega-CD - Sega CD|Sega - Mega Drive - Genesis|Sega - PICO|Sega - SG-1000"
license = "Non-commercial"
permissions = ""
display_version = "v1.7.4"
supports_no_game = "false"
firmware_count = 12
firmware0_desc = "bios_MD.bin (Mega Drive startup ROM)"
firmware0_path = "bios_MD.bin"
firmware0_opt = "true"
firmware1_desc = "bios_CD_E.bin (MegaCD EU BIOS)"
firmware1_path = "bios_CD_E.bin"
firmware1_opt = "true"
firmware2_desc = "bios_CD_U.bin (SegaCD US BIOS)"
firmware2_path = "bios_CD_U.bin"
firmware2_opt = "true"
firmware3_desc = "bios_CD_J.bin (MegaCD JP BIOS)"
firmware3_path = "bios_CD_J.bin"
firmware3_opt = "true"
firmware4_desc = "bios_E.sms (MasterSystem EU BIOS)"
firmware4_path = "bios_E.sms"
firmware4_opt = "true"
firmware5_desc = "bios_U.sms (MasterSystem US BIOS)"
firmware5_path = "bios_U.sms"
firmware5_opt = "true"
firmware6_desc = "bios_J.sms (MasterSystem JP BIOS)"
firmware6_path = "bios_J.sms"
firmware6_opt = "true"
firmware7_desc = "bios.gg (GameGear BIOS)"
firmware7_path = "bios.gg"
firmware7_opt = "true"
firmware8_desc = "sk.bin (Sonic & Knuckles ROM)"
firmware8_path = "sk.bin"
firmware8_opt = "true"
firmware9_desc = "sk2chip.bin (Sonic & Knuckles UPMEM ROM)"
firmware9_path = "sk2chip.bin"
firmware9_opt = "true"
firmware10_desc = "areplay.bin (Action Replay ROM)"
firmware10_path = "areplay.bin"
firmware10_opt = "true"
firmware11_desc = "ggenie.bin (Game Genie ROM)"
firmware11_path = "ggenie.bin"
firmware11_opt = "true"
notes = "(!) sk2chip.bin (md5): b4e76e416b887f4e7413ba76fa735f16|(!) sk.bin (md5): 4ea493ea4e9f6c9ebfccbdb15110367e"
