Sections
{$ read} | Section code is executed when the read memory button is pressed.
{$ write} | The section code is executed when the memory record button is pressed.
{$ erase} | The section code is executed when the memory erase button is pressed.
{$ verify} | Section code is executed when the memory comparison button is pressed.
{$ unlock} | Section code is executed when the unprotect button is pressed.
Predefined variables
_IC_Name | The name of the currently selected chip
_IC_Size | Size, in bytes, of the currently selected chip
_IC_Spare | Spare area size, in bytes, of the currently selected SPI NAND chip
_IC_Page | Page size, in bytes, of the currently selected chip
_SPI_SPEED_MAX | The highest possible frequency for SPISetSpeed
Main functions
ShowMessage ( text+'\n'+text ); | Analogue ShowMessage (use '\n' string for multi line)
LogPrint ( text ); | Print a message to the log Parameters: text message text
IntToHex ( value , digits ): string; | Analog IntToHex
ProgressBar ( inc , max , pos ); | Sets the status of the ProgressBar Parameters: inc how much the position is increased Optional parameters: max maximum position ProgressBar pos sets the specific position of the ProgressBar
CreateByteArray ( size ): variant; | Creates an array with varbyte element type
CreateStringArray ( size ): variant; | Creates an array of string
GetArrayItem ( array , index ): variant; | Returns the value of an array element
SetArrayItem ( array , index , value ); | Sets the value of an array element
ReadToEditor ( size , position , buffer, ... ); | Writes data from the buffer to the size editor at position
WriteFromEditor ( size , position , buffer, ... ); | Writes data from size editor from position
GetEditorDataSize: longword; | Returns data size in editor
Work with SPI
SPIEnterProgMode ( speed ): boolean; | Initializes the pin state for SPI and sets the SPI frequency Parameters: speed _SPI_SPEED_MAX = AvrIsp 8 (4) MHz / USbAsp 3 MHz If the frequency is not set, returns false Ignored for devices with a fixed frequency
SPIExitProgMode (); | Disables SPI pins
SPIRead ( cs , size , buffer , ... ): integer; | Reads data to buffer Parameters: cs if cs = 1 release Chip Select after reading data size data size in bytes buffer variables for storing data or an array created by CreateByteArray Returns the number of bytes read
SPIWrite ( cs , size , buffer , ... ): integer; | Writes data from the buffer Parameters: cs if cs = 1 release Chip Select after writing data size data size in bytes buffer data variables or array created CreateByteArray Returns the number of written bytes
SPIReadToEditor ( cs , size ): integer; | Reads data to the editor Parameters: cs if cs = 1 release Chip Select after reading data size data size in bytes Returns the number of bytes read
SPIWriteFromEditor ( cs , size , position ): integer; | From Writes data size editor size from the standpoint position parameters: Cs if Cs = 1 release, after Chip Select data record size data size in bytes of the position the position in the editor returns the number of bytes written
Work with I2C
I2CEnterProgMode (); | Initializes the state of the pins
I2cExitProgMode (); | Disables pins
I2CReadWrite ( DevAddr , wsize , rsize , wbuffer , rbuffer ): integer; | Writes / reads data from buffers Parameters: DevAddr device address size data size in bytes buffer variable data or array created CreateByteArray Returns the number of recorded bytes read + * If rsize = 0 can omit the parameter rbuffer
I2CStart (); | Used with I2CReadByte and I2CWriteByte
I2CStop (); | Used with I2CReadByte and I2CWriteByte
I2CReadByte ( ack : boolean): byte; | Reads a data byte and sends ack / nack
I2CWriteByte ( data ): boolean; | Writes a data byte and returns ack / nack