display_name = "Commodore - PET (VICE xpet)"
authors = "VICE Core Team Members"
supported_extensions = "d64|d71|d80|d81|d82|g64||g41|x64|t64|tap|prg|p00|crt|bin|zip|gz|d6z|d7z|d8z|g6z|g4z|x6z|m3u"
corename = "VICE"
manufacturer = "Commodore"
categories = "Emulator"
systemname = "PET"
systemid = "commodore_pet"
database = "Commodore - PET"
license = "GPLv2"
permissions = ""
display_version = "v3.3"
supports_no_game = "false"
firmware_count = 7
firmware0_desc = "chargen (PET BIOS)"
firmware0_path = "vice/PET/chargen"
firmware0_opt = "false"
firmware1_desc = "edit1g (PET BIOS)"
firmware1_path = "vice/PET/edit1g"
firmware1_opt = "false"
firmware2_desc = "edit2b (PET BIOS)"
firmware2_path = "vice/PET/edit2b"
firmware2_opt = "false"
firmware3_desc = "edit2g (PET BIOS)"
firmware3_path = "vice/PET/edit2g"
firmware3_opt = "false"
firmware4_desc = "edit4b40 (PET BIOS)"
firmware4_path = "vice/PET/edit4b40"
firmware4_opt = "false"
firmware5_desc = "edit4b80 (PET BIOS)"
firmware5_path = "vice/PET/edit4b80"
firmware5_opt = "false"
firmware6_desc = "edit4g40 (PET BIOS)"
firmware6_path = "vice/PET/edit4g40"
firmware6_opt = "false"
notes = "(i) Place BIOS files in system/vice/PET folder."
