| Home > Control Panel # Using the Control Panel Control Panel Buttons and Lights You can control simple printer operations—such as line feeding, form feeding, and loading and ejecting paper. The control panel lights show the printer’s status. ## Control Panel Buttons and Lights 1. LF/FF button Feeds paper line by line when pressed shortly. Ejects a single sheet or advances continuous paper to the next top-of-form position when held down for a few seconds. 2. Micro Adjust When you hold down the Pause button for three seconds, the printer enters the Micro Adjust mode. In this mode, you can adjust the top-of-form and tear-off positions by pressing the LF/FF and Load/Eject buttons. See Using the Micro Adjust Function. 3. Load/Eject button Loads a single sheet of paper. Ejects a single sheet of paper if a sheet is loaded. Loads continuous paper from the standby position. Feeds continuous paper backward to the standby position if a sheet is loaded. 4. Pause button Stops printing temporarily, and resumes printing when pressed again. When held down for three seconds, enters the Micro Adjust mode. When pressed again, exits the Micro Adjust mode. 5. Pause light On when the printer is paused. Flashes when the printer is in the Micro Adjust mode. 6. Paper Out light On when no paper is loaded in the selected paper source or paper is not loaded correctly. Flashes when paper has not been fully ejected. 7. Power light On when the printer turns on. Flashes when a fatal error occurs. Top |