Thank you for purchasing this Jolimark FP-530K+ Printer. The detailed instruction of driver installation is shown as below. If you have any question, please consult our website: http://www.jolimark.com.cn or contact us directly. 

กมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกม
กม        Driver CD content          กม
กมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกม
This driver CD contains the Jolimark FP-530K+ printer operation systems for Windows 98/ME, Windows2000/XP: 

Driver list   	             Suitable operation system 
WIN98(WINME)	            Windows 98/ME
WIN2000(XP-Vista)	    Windows 2000/XP/2003/Vista/Windows 7

กมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกม
กม    Install driver in WINDOWS98/WINDOWSME/WINDOWSNT operation system กม
กมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกม
|
|---- 1. If printing with USB interface, first, please install USB driver solely. Or else, install the driver as shown below. 

    2. Click กฐStartกฑ --- กฐSettingsกฑ --- กฐPrinterกฑ. 

    3. Double click กฐAdd Printerกฑ, and click กฐNextกฑ, then please read the select guide carefully, such as, select กฐLocal printerกฑ in the กฐAdd Printer Wizardกฑ window, then click กฐNextกฑ.

     4. After reading the select guide, Click กฐHave Diskกญกฑ. Please according to the operating system environment, such as Windows 98 system, you should select the path as follow: WIN98 (WINME), click กฐOKกฑ, a file named: FP530KP.inf appears, and then click กฐOKกฑ. 

     5. A window of กฐInstall From Diskกฑ appears, make sure the selected path is correct, then click กฐOKกฑ to enter the window of กฐAdd Printer Wizardกฑ, please ensure the printer name is correct or not, If you are sure, please click กฐNextกฑ; Else if not sure, please reinstall it from step 1. 

     6. Enter the window of กฐAdd Printer Wizardกฑ, select the usable port, such as, select: กฐLPT1:กฑ, and then click กฐNextกฑ, and it would show the printer name. Then Otherwise according to prompt, choose the printer is default: กฐYesกฑ, click กฐNextกฑ. Choose กฐYes-(recommended)กฑ, if it prints correctly, click กฐFinishกฑ. Thus, you have finished installation of printer driver. 
       (The Windows 2000 version of this driver may be unable to find the driver digital signature during installation, and it would ask if going on installing, at that time, please click กฐOKกฑ to ignore that signature. This would not affect the driver installation.) 
     
|
|---- Information: In WIN98/ME system, if you need to use USB interface for printing, please install USB driver separately, and then install the graph printing driver! After installation, please click กฐStartกชSettingsกชPrintersกฑ again to select FP-530K+ driver and select USB port. 
  *****************************    
    USB driver installation
  *****************************    
  
     1. In the operating system of Windows 2000/XP, use a USB cable to connect the printer with the computer, after turning on the printer, the system would identify the printer driver in accordance with installation automatically. 
     
     2. In the operating system of Windows 98/ME, use a USB cable to connect the printer with the computer, after turning on the printer, the computer would pop up a window of กฐAdd new hardware wizardกฑ, please install it according to the information.
     
     3. Click กฐNextกฑ, select กฐBrowseกฑ, and select the corresponding driver in กฐWIN98(WINME)กฑกชกฐUSBdriverกฑ, click กฐOKกฑ and click กฐNextกฑ. 
     
     4. System would install USB driver automatically, clickกฑOKกฑ, installation is finished. 
  
     5. In the system of WIN98/ME, if you need to use USB interface for printing, after installing USB driver, you need to install FP-530K+ printer driver again. Please select the FP-530K+ driver from กฐStartกชSettingsกชPrintersกฑ, and then select USB port. 


กมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกม
กม Install driver in the system of WINDOWS2000/WINDOWSXP//2003/Vista/Windows 7: กม
กมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกม
|
|---- 1. Connect the printer and power on the printer. 

     2. Open the installation file in the driver CD, double click the file named กฐSetup.exe.กฑ, then it would pop up an installation window. 

     3. Please select the printer driver in the popping window. 
     
     4. Click the กฐInstallกฑ button in the bottom right of the window, the system would install automatically; (If the computer pops up a window of กฐHardware Installationกฑ, please select กฐContinue Anywayกฑ to go on installing!) 
     
     
     5. After installation, a window of กฐFinish installationกฑ will pop up, click กฐOKกฑ and กฐExit installationกฑ to exit the installation. Then you could set the printing parameters and start to use the driver for printing. 

|
|---- Information:
     1. In the system of Windows 2000/XP/2003/Vista/Windows 7, when using USB interface for printing, please using the same USB interface of computer to connect with the printer (do no change the USB port optionally), so that to avoid the system automatically producing the driver copy of the same model. 
     
     2. When installing the USB driver, please connect the printer and the computer with USB cable and install the driver while the printer is turned on. 
     If you install the driver when the printer is turned off, after turning on the printer, the computer may still detect new hardware and would appear the same driver copy as information1 shown above. 

     3. When using auto-install of Setup, only connect parallel interface when using parallel interface for printing; only connect USB interface when using USB interface for printing. 


กมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกม
กม  Additional instruction with respect to the driver      กม
กมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกมกม
1. When there is no your required setting in the predetermined page of the printer page setting, we recommend to use กฑMetricกฑ (centimeter or millimeter) as the unit during setting user-defined unnormalized page length to ensure the paper feeding more precisely. 

2. Before installing new driver, please make sure the old driver has been deleted to avoid installation error! 
