# Send / Reception Settings
Device Management > Configuration > Fax > Send / Reception Settings

Configure settings for Internet Fax transmission and Fax reception.

Note

- Settings on this page can be changed by the following administrators and users:
  - Network Administrator (Transmission Settings)
  - Machine Administrator (Reception Settings)
  - Users logged in to a device that is set to perform user authentication
    Users must have normal fax operation rights and permission to change settings that usually only administrators can change.
- Some items may not appear depending on machine type or configuration.

## Transmission Settings

### Maximum Email Size

Specify whether to limit Internet Fax transmissions according to maximum email size.
When On is selected, specify the maximum email size in Email Size below.

#### Email Size

Enter the maximum email size in kilobytes (128 to 102400 KB).

## Reception Settings

### Switch Reception Mode

Select the reception mode if using standard G3 line.

Note

- The optional handset or an external telephone is required to use Manual Reception.

#### Auto Reception

When a call comes in, the device automatically receives it as a fax. Use this setting for dedicated fax lines. If the call is voice, you must manually switch to telephone mode.

#### Manual Reception

When a call comes in, the device rings. If the call is a fax, you must manually switch to facsimile mode.

### SMTP RX File Delivery Settings

Specify whether to deliver files received on an SMTP server using a fax line.
When On is selected, specify the authorized email address in Authorized Email Address below.

Note

- SMTP server settings can be configured on the Configuration: Device Settings: Email page.

#### Authorized Email Address

Enter an email address. Up to 128 alphanumeric characters can be entered.
Files sent from the email address entered here are delivered.
For example, if you specify "@xyz.co.jp", email sent from addresses such as "abc@xyz.co.jp" or "def@xyz.co.jp" will be delivered. Email sent from addresses that do not match the setting, for example "abc@xyz2.co.jp", will not be delivered.

Note

- When email is received from an email address that does not match the email addresses specified here, the email is deleted and an error message returned to the SMTP server. An error report is not produced even if the email is deleted.

#### Encryption

Specify whether or not to encrypt fax-received data when sending it to an email address.

#### Signature

Specify whether or not to apply a digital signature when sending fax-received data to an email address.

### 2 Sided Print

Specify whether to duplex print fax-received data.

Note

- To initiate duplex printing, all pages of received data must be the same size. Also, paper of the same size as the received data must be loaded in the machine.

### Checkered Mark

Specify whether to print a checkered mark on the first page of fax messages to help you separate multiple jobs.

### Center Mark

Specify whether to print a center mark on fax messages, lists, and reports. The center mark position can be Center of Left Edge or Center of Top Edge of the paper.

### Print Reception Time

Specify whether to print the time of receipt on fax messages. The print position is the bottom edge of the paper.

### Reception File Print Quantity

Enter the number of copies you want to print. You can enter a number between 1 and 10 (copies).

### Paper Tray

Select a paper tray for printing fax-received data.

### Fax Print Color

Select a color for printing fax-received data.

Note

- This setting item may not be displayed depending on machine type.

### 2nd Color

Select an alternative color when toner of the color selected in Fax Print Color runs out.

Note

- The color selected in Fax Print Color cannot be selected.
- This setting item may not be displayed depending on machine type.

### Memory Lock Reception

Specify whether to use memory lock reception.
If memory lock reception is enabled, incoming faxes are stored in memory and do not print automatically. You need to enter a memory lock ID to print them.
To enable memory lock reception, you must first enter the ID in the Program Memory Lock ID box on the Configuration: Fax: Initial Settings page.

## Buttons

### Refresh

Click to update the currently displayed information.

Note

- Before making the settings, click Refresh to obtain the machine's current status.

### OK

Click to apply the settings.

### Cancel

Click to cancel the settings.

##