# Change Phase 2 User Name
Device Management > Configuration > Security > IEEE 802.1X > Change Phase 2 User Name

Use this page to set or change the user name used for phase 2.

Note

- If EAP Type is set to EAP-TTLS or PEAP for IEEE 802.1X, the user name is required.
- Settings on this page can be changed by the following administrator:
  - Network Administrator

### New Phase 2 User Name

Enter the user name you want to set or change, using up to 31 alphanumeric characters. The "@" (at-sign) character cannot be used.

### Confirm Phase 2 User Name

Enter the new user name again to confirm it.
The user name entered here must be the same as that entered earlier in New Phase 2 User Name.

## Buttons

### OK

Click to save the settings and return to the IEEE 802.1X page. The settings are applied when you click OK on the IEEE 802.1X page.

### Cancel

Click to cancel the settings.

##