# LDAP Server (Setup)
Device Management > Configuration > Device Settings > LDAP Server > LDAP Server (Setup)

Register and update LDAP servers.

### Identification Name

Enter the LDAP server's name using up to 20 characters.

### Server Name

Enter the LDAP server's host name or IP address using up to 128 characters.

### Search Base

Enter the position within the LDAP directory's structure from which to start user searches. Use up to 128 alphanumeric characters.
Example: dc=my-domain.com

### Port Number

Enter the port number used to connect to the LDAP server. Use a number from 1 to 65535. The default is 389.

### SSL

Specify whether or not to use SSL to communicate with the LDAP server. If you select On, communication between machine and LDAP server is SSL encrypted. If you select Off, communication is not encrypted.

Note

- To apply SSL encryption, a device certificate must be installed in the device.
- This setting is reflected in the Port Number box. When On is selected, Port Number is set to "636", and when Off is selected, Port Number is set to "389".

### Authentication

Select to perform authentication when the machine connects to the LDAP server.

#### Off

No authentication.

#### Cleartext Authentication

User name and password authentication.

#### Digest Authentication

User name, password, and device certification authentication.

#### Kerberos Authentication

User name, password, and device certification authentication.

Note

- Set your user name and password using User Name and Password on this page.

### User Name

Enter your LDAP server login user name. Use up to 128 alphanumeric characters.

Note

- If Authentication is set to Digest Authentication or Kerberos Authentication, a user name must be set.

### Password

Click Change to update the logged-in user's password.

Note

- If Authentication is set to Digest Authentication or Kerberos Authentication, a password must be set.

For details about the Change Password page

### Realm Name

If you selected Kerberos Authentication for Authentication, you must specify the Kerberos realm for user authentication.

Note

- The realm name must be preset on the Device Management - Configuration - Device Settings - Kerberos Authentication page.

### Japanese Character Code Set

Select a character code set for the LDAP server to use.

### Connection Test

Click Start to see whether or not connection to the LDAP server is possible using the settings configured.

## Search Conditions

Specify which items of user information to search for via LDAP search.

### Identification Name

Enter an attribute type by which the user name can be distinguished. Use up to 64 alphanumeric characters.
Default: "cn".

### Email Address

Enter an attribute type by which the user email address can be distinguished. Use up to 64 alphanumeric characters.
Default: "mail".

### Fax Number

Enter an attribute type by which the user fax number can be distinguished. Use up to 64 alphanumeric characters.
Default: "facsimileTelephoneNumber".

### Company Name

Enter an attribute type by which the user's company (or organization) name can be distinguished. Use up to 64 alphanumeric characters.
Default: "o".

### Department Name

Enter an attribute type by which the user's department name can be distinguished. Use up to 64 alphanumeric characters.
Default: "ou".

## Search Options

Specify other condition for LDAP search, if required. For example, to search for information based on user's employee number, enter "employeeNo" in the Attribute box, and then enter "Employee No." in the Key Display box.

### Attribute

Enter an attribute type by which the user can be distinguished. Use up to 64 alphanumeric characters.

### Key Display

Enter the name shown on the machine's control panel, which is used for LDAP search to search a user based on the attribute type specified in the Attribute box. Use up to 20 alphanumeric characters.

## Buttons

### OK

Click to apply the settings.

### Cancel

Click to cancel the settings and return to the LDAP Server page.

##