# User Authentication Management (User Code)
Device Management > Configuration > Device Settings > User Authentication Management > User Authentication Management (User Code)

Specify whether to enable user code management (limit functions or count total pages by user code) for each function available on the device.

Note

- To enable user code management, a user code must be registered to the Address Book. Click Address Book in the menu area to display the Address Book.
- Some items may not appear depending on machine type or configuration.

## Printer Job Authentication Settings

Configure settings for processing printer jobs under each authentication method.

Note

- The setting configured here is for User Code Authentication, Basic Authentication, Windows Authentication, and LDAP Authentication.

### Printer Job Authentication

Specify whether to print a job if the printer driver sending the job contains no authentication information (i.e. no user name or password).

#### Entire

The job is not printed if it has no authentication information.

#### Simple (Limitation)

Authentication-based print is determined by settings configured under the following: Limitation Range (IPv4), Limitation Range (IPv6), Parallel Interface (Simple), and USB (Simple).

#### Simple (All)

The job is printed even if it has no authentication information.

### Limitation Range (IPv4)

Enter a range for limiting unauthenticated print jobs from IPv4 addresses. You can set up to five ranges.
Any job sent from an IPv4 address within the range entered here is printed, regardless of whether or not it is authenticated. Any unauthenticated job sent from an IPv4 address outside the entered range is not printed.

Note

- This setting is only possible if Printer Job Authentication is set to Simple (Limitation).

### Limitation Range (IPv6)

Enter a range for limiting unauthenticated print jobs from IPv6 addresses. Enter the range using a combination of start and end addresses, or a combination of base address and mask. You can set up to five ranges.
Any job sent from an IPv6 address within the range entered here is printed, regardless of whether or not it is authenticated. Any unauthenticated job sent from an IPv6 address outside the entered range is not printed.

Note

- Use one of the following procedures to specify the range:
  - Select Range, and then enter the start and end addresses.
  - Select Mask, enter the base address, and then enter the mask between 1 and 128 in the Mask Length.
- This setting is only possible if Printer Job Authentication is set to Simple (Limitation).

### Parallel Interface (Simple)

Specify whether or not to apply authentication-based print to jobs sent using the parallel interface.
Apply: unauthenticated jobs are not printed.
Do not Apply: unauthenticated jobs are printed.

Note

- This setting is only possible if Printer Job Authentication is set to Simple (Limitation).

### USB (Simple)

Specify whether or not to apply authentication-based print to jobs sent using the USB interface.
Apply: unauthenticated jobs are not printed.
Do not Apply: unauthenticated jobs are printed.

Note

- This setting is only possible if Printer Job Authentication is set to Simple (Limitation).

## User Code Authentication Settings

### Functions to Restrict

Select the function(s) for which you want to enable user code management.

Note

- If Printer: PC Control is selected, user code management by printer color mode (Color and Black & White) is disabled.
- Some items may not appear depending on machine type or configuration.

#### Copier: Black & White

Enable or disable user code management for black and white copying.

#### Copier: Single Color

Enable or disable user code management for single color copying.

#### Copier: Two-color

Enable or disable user code management for two-color copying.

#### Copier: Full Color

Enable or disable user code management for full color copying.

#### Printer: Black & White

Enable or disable user code management for black and white printing.

#### Printer: Color

Enable or disable user code management for color printing.

#### Printer: PC Control

Enable or disable automatically registering user codes to the Address Book.
If the check box is selected, the user code assigned in the printer driver is automatically registered to the Address Book on the device when a job is sent by the driver.

#### Other Function(s): Document Server

Enable or disable user code management for operations of the Document Server.

#### Other Function(s): Fax

Enable or disable user code management for fax functions.

#### Other Function(s): Scanner

Enable or disable user code management for scanner functions.

#### Other Function(s): Browser

Enable or disable user code management for browser functions on the machine's control panel.

#### Extended Features

Enable or disable user code management for the extended features application.

## Buttons

### Refresh

Click to update the currently displayed information.

Note

- Before making the settings, click Refresh to obtain the machine's current status.

### OK

Click to apply the settings.

### Cancel

Click to cancel the settings.

##