# AirPrint
Device Management > Configuration > Network > AirPrint

Configure settings related to AirPrint.

Note

- Settings configured here relate to the following interfaces:
  Ethernet and wireless LAN.
- Settings on this page can be changed by the following administrators and users:
  - Network Administrator
  - Login users
    User authentication is enabled on the device and users are permitted to make changes to administrator's setting items.
- AirPrint is a trademark of Apple Inc.

### AirPrint

Specify whether AirPrint for the device's interface boards is active or inactive.

### Bonjour Service Name

Enter a name to identify the device using Bonjour, using up to 63 characters.
The default is the manufacturer's name followed by the device model.
This item is linked to Computer Name on the Device Management - Configuration - Network - Bonjour page.

## Location

Enter the device location, using up to 32 characters.
This item is linked to Location on the Device Management - Configuration - Device Settings - System page.

### Latitude/Longitude

Enter the latitude and longitude of the device location, using the ranges (to the 14th decimal place) specified below.
Latitude: -90.00000000000000 to 90.00000000000000
Longitude: -180.00000000000000 to 180.00000000000000

## Device Certificate

The Device Certificate page appears.
If you transfer data via AirPrint (IPP), you need to apply SSL/TLS in advance. Set "Certificate 1" on the Device Certificate page. Confirm the certificate status of "Certificate 1". Change the settings or upload a certificate file as necessary.

Note

- Changes in the Device Certificate settings are also applied to other communication methods.

## IPP Authentication

The IPP Authentication page appears.
To require authentication by password and user name in print form, set the IPP Authentication.

Note

- IPP Authentication settings are applied to all device settings.

## Buttons

### Refresh

Click to update the currently displayed information.

Note

- Before making the settings, click Refresh to obtain the machine's current status.

### OK

Click to apply the settings.

### Cancel

Click to cancel the settings.

##