# Change Password
Device Management > Configuration > Security > IEEE 802.1X > Change Password

Use this page to set or change the password for logging in to the authentication server.

Note

- If EAP Type is set to LEAP, EAP-TTLS, or PEAP for IEEE 802.1X, the password is required.
- Settings on this page can be changed by the following administrator:
  - Network Administrator

### New Password

Enter the password to set or change, using up to 128 alphanumeric characters.

### Confirm Password

Enter the new password again to confirm it.
The password entered here must be the same as that entered earlier in New Password. If it is not, the password cannot be changed.

## Buttons

### OK

Click to save the settings and return to the IEEE 802.1X page. The settings are applied when you click OK on the IEEE 802.1X page.

### Cancel

Click to cancel the settings.

##