# Printer Basic Settings
Device Management > Configuration > Printer > Printer Basic Settings

Use this page to make changes to the printer function settings.

Note

- Settings on this page can be changed by the following administrators and users:
  - Machine Administrator
  - Login users
    User authentication is enabled on the device and users are permitted to make changes to administrator's setting items.
- Some items may not appear depending on machine type or configuration.

## System

Configure settings for the machine's basic operations.

### Print Error Report

Select to have an error report printed if an error occurs during print data processing.
This setting is available when you use a PCL 6 or PS3 printer driver, or when you select PDF printing.

### Auto Continue

Select the printer response when the appropriate paper tray matching paper size and type specified in the job, is not equipped with the printer.

#### Off

The printer stops operation until the correct paper is loaded.

#### Immediate, 1 minute, 5 minutes, 10 minutes, 15 minutes

When the specified period of time elapses, the printer does the following:
When Auto Select is specified, the printer checks trays in the order of Paper Tray Priority, Tray 1, Tray 2, Tray 3, and Bypass Tray, for trays with paper loaded. When the printer detects a tray with paper loaded, it begins printing.
When Auto Select is not specified and the paper tray is specified by the job, the printer begins printing using the tray, regardless of size and type of paper loaded in the tray. If the specified tray has no paper loaded, the printer stops operation until the correct paper is loaded.

### Memory Overflow

Select the printer response if the job is too large.

#### Do not Print

Resets the job at the error page. Subsequent pages following the error page are not printed.

#### Error Information

For the error page, job data before the error is processed and printed. Subsequent pages are printed normally, and the error sheet is printed at the end. When this happens, the electronic collation is canceled.

### Error Display Setting

Select the format of error message that appears on the device's control panel when an error occurs during print data processing.

#### Only Important Ones

Displays simplified error information.

#### All

Displays detailed error information.

### Auto Cancel Confirmation for PDL Error Job

Specify whether or not to stop printing and display a confirmation page when auto job reset occurs.
When Display is selected, subsequent jobs following the error job will not be received unless you close the confirmation page.

### Auto Cancel for Print Job(s) on Error

Specify whether or not to reset the print job where the print error occurred and reset the jobs received before the error.

### Job Separation

Completes sets of copies and shifts the output position of each. When printing large numbers of multiple-sheet jobs, the output can be automatically separated.

### Rotate Sort: Auto Paper Continue

Specify whether to print continually or cancel the print job if either of the trays where paper is loaded for landscape and portrait is empty when the rotate collate function is used for printing.

### Auto Delete Temporary Print Jobs

Specify whether to automatically delete Locked, Sample, and Hold print jobs stored on the machine.
When On is selected, enter a time after which jobs stored on the machine are deleted. Enter from 1 to 200 hours.

### Auto Delete Stored Print Jobs

Specify whether to automatically delete Stored Print jobs stored on the machine.
When On is selected, enter a time after which jobs stored on the machine are deleted. You can enter a value between 1 and 180 (days).

### Print Job Function

Specify whether to enable or disable the print job settings such as Sample Print, Locked Print, Hold Print, and Stored Print.

#### Same as System Settings

Follows the setting of Document Server Function in System Settings on the control panel. The print job setting is enabled if Document Server Function is selected.

#### On

Enables the print job settings.

### Stapleless Stapler and Staple Display Setting

Specify whether or not to display only the stapleless stapler as the top slant stapling option.

#### Stapleless Only Available

Enables to select only stapleless stapling as the top slant stapling option.

#### Stapleless & Staple Available

Enables to select either stapleless or regular stapling as the top slant stapling option.

### Jobs Not Printed As Machine Was Off

Specify how the machine responds when the Hold Print (Print at Set Time) jobs are not printed because the main power of the machine is turned off.

#### Print When Machine On

Prints the jobs automatically when the main power is turned on.

#### Do not Print

Does not print the jobs even when the main power is turned on. The status changes to Hold Print (Incomplete: Print at Set Time). If you want to print them, go to the Print Job List page where you can print it.

For details about the Print Job List page

### Rotate by 180 Degrees

Specify whether to rotate images by 180 degrees before printing.

### Print Compressed Data

Specify whether to print incoming compressed job data after decompressing it on the printer.

Note

- The only supported compression format is GZIP.

### Memory Usage

Select memory usage priority.
Select an option according to paper size, print resolution, and printer language used.

#### Font Priority

This setting uses memory for registering fonts and foreign characters.

#### Frame Priority

This setting uses memory for high speed printing.

### Duplex

Specify whether or not to print on both sides of each page, and then select the binding orientation.
This setting is available when you use a PCL, PS3, or XPS printer driver, or when you select PDF printing.

### Copies

Enter the default number of copies. Available values are between 1 and 999.
This setting is available when you use a PCL, PS3, or XPS printer driver, or when you select PDF printing.

### Blank Page Print

Specify whether to print blank pages.

### Reserved Job Waiting Time

Select the timeout period to elapse before beginning the next job.

Note

- This setting is enabled only when Job Order is selected for Interleave Priority. You can configure settings for Interleave Priority on the Configuration: Device Settings: System page.

### Printer Language

Select the printer language to be used.
When Auto is selected, the printer automatically switches between the available printer languages according to job data format.

### Sub Paper Size

Specify whether or not the paper size switches automatically when paper of the specified size is not loaded in the tray. This feature supports automatic switching between A4 and Letter (8 ½ x 11) size paper only.

Note

- A4 and Letter (8 ½ x 11) have different maximum printable areas. Therefore, if you enable the switching option, images that extend beyond the printable area may be cropped.

### Page Size

Select the default paper size.
This setting is available when you use a PCL printer driver.

### Letterhead Setting

Select to have the letterhead printed.

#### Off

Does not perform letterhead printing.

#### Auto Detect

Perform letterhead printing only when letterhead paper is specified.

#### On (Always)

Always perform letterhead printing.

### Tray Setting Priority

When using input trays, specify whether to give priority to the device's paper settings or to the job's paper settings.

Note

- Driver / Command (Size Discord) is available for the bypass tray only.

#### Driver/Command

Jobs are printed using the paper settings (such as paper size and type) configured for the job.

#### Machine Setting(s)

Jobs are printed using the paper settings (such as paper size and type) configured on the machine.

#### Driver / Command (Size Discord)

You can set this option only for the bypass tray. If the paper size specified in the printer driver or by a command is different from the paper size detected by the machine, a paper mismatch error occurs.

### Paper Confirmation for Bypass Tray

Specify whether or not to display the confirmation page for checking the paper size, type and direction on the bypass tray before the paper is fed from the tray.

### Paper Mismatch Alert for Bypass Tray

Specify whether or not to display an alert page if the paper size, or paper type settings configured for the job does not match the paper loaded in the bypass tray or paper is running out.

Note

- This function is available only if Machine Setting(s) or Driver / Command (Size Discord) is selected in Tray Setting Priority.

### Store and Skip Errored Job

Specify whether or not to store the print job on the machine when the job is stopped because of the print error. By storing and skipping jobs with errors, a print job after the job with the error is processed and printed. To print the stored print job, go to the Print Job List page.

For details about the Print Job List page

Note

- You cannot skip the job that was stopped after the machine started feeding one single paper from the input tray.

#### No. of Pages to Judge if a Job has Error

After the function checked through the specified pages for errors, the print job is processed. The machine does not feed a paper until the error check is finished. You can avoid the situation described above in the note.

### Edge to Edge Print

Select to print over the whole sheet area, leaving no edge borders.
Selecting On results in output leaving no borders.
This setting is available when you use a PCL, PS3, or XPS printer driver, or when you select PDF printing.

### Default Printer Language

Select the default printer language to be activated when the printer is turned on.

### Tray Switching

Specify whether or not to switch to the alternate tray when paper size or type specified in the job data does not match paper loaded in the specified tray.
This setting is available when you use a PCL, PS3, or XPS printer driver, or when you select PDF printing.

#### On

Outputs the job using the paper tray having the correct paper, if available.

#### Off

Do not make switching. The job will result in an error.

### Collate Settings

Specify whether or not to collate multiple printed sets.

#### Collate

Outputs each set in page order.

#### Rotating Collate

Outputs each set in page order, rotating every other set by 90 degrees.

#### Shift Collate

Outputs each set in page order, staggering every other set.

### Staple Settings

Specify whether or not to staple each copy, and if yes, select the staple position.

#### Off

Do not staple.

#### Top Left Slant (Stapleless)

Apply stapleless stapling to the top left of the paper in one position. Staple orientation is slanted.

#### Top Right Slant (Stapleless)

Apply stapleless stapling to the top right of the paper in one position. Staple orientation is slanted.

#### Top 2

Staple the top of the paper in two positions.

#### Top Left

Staple the top left of the paper in one position. Staple orientation is vertical.

#### Top Left Slant

Staple the top left of the paper in one position. Staple orientation is slanted.

#### Top Right

Staple the top right of the paper in one position. Staple orientation is vertical.

#### Top Right Slant

Staple the top right of the paper in one position. Staple orientation is slanted.

#### Left 2

Staple the left side of the paper in two positions.

#### Right 2

Staple the right side of the paper in two positions.

#### Center

Staple the center of the paper in two positions.

### Punch Settings

Specify whether or not to punch the printed paper, and if yes, select the punch position.

#### Off

Do not punch.

#### Top 2, Top 3, Top 4, Left 2, Left 3, Left 4, Right 2, Right 3, Right 4

The above are the number of punch holes and their positions.

### List/Test Print Lock

Specify whether to disable test print.
If On is selected, the printer cannot print test pages even if it receives the test print command.

### Extended Auto Tray Switching

Specify whether or not the machine automatically switches to another tray containing paper of the required size, orientation, and type if the specified tray runs out of paper during a job.

### Virtual Printer

Specify whether to enable or disable the virtual printer function.

Note

- You can create a virtual printer using the Virtual Printer Settings page (accessed from Device Management - Configuration - Printer).

### Restrict Direct Print Jobs

Specify whether or not to store print jobs on the machine's hard disk without printing out them to the output tray.

#### Off

Prints out the jobs.

#### Automatically Store Jobs

Does not print out the jobs and stores them on the machine's hard disk. If you want to print them, go to the Print Job List page where you can print it.

For details about the Print Job List page

#### Cancel All Direct Print Jobs

Cancels all jobs to be printed out to the output tray.

### Auto Store Jobs without User Authentication Information

Specify whether or not to forcibly store print jobs without user authentication information on the machine's hard disk. If Off is selected, print jobs without user authentication information will be cancelled.

Note

- This function is available only when the following settings are configured:
  - If user authentication other than User Code Authentication is enabled.
  - Automatically Store Jobs is selected for Restrict Direct Print Jobs.

### Initial screen switch setting

Specify an initial screen to be displayed when the printer function is selected on the device control panel.

### Auto Cancel Print Job if Key Card Removed or No Units

Specify whether or not to cancel the job if no units remain on the key card or the key card is removed while printing is performed.

### When Exceeded Max. Number of Sheets for Stapling

Select an option to specify how jobs are handled after the maximum number of sheets are stapled.

Note

- For details about the maximum number of sheets for stapling, see the operating instructions provided with the machine.
- Depending on the finisher installed, the output mode to staple sheets whose number exceeds the maximum number varies.

#### Continue Printing

Continues printing.

#### Cancel Printing

Stops printing, and cancels the job.

#### Suspend (Display Alert Screen)

Suspends printing, and displays a message on the device control panel. Check the message to select Continue Printing or Cancel Printing.

### When Exceeded Max. Number of Sheets for Booklet

Select an option to specify how jobs are handled after the maximum number of sheets are stapled for a booklet.

Note

- For details about the maximum number of sheets for stapling, see the operating instructions provided with the machine.
- Depending on the finisher installed, the output mode to staple sheets whose number exceeds the maximum number varies.

#### Continue Printing

Continues printing.

#### Cancel Printing

Stops printing, and cancels the job.

#### Suspend (Display Alert Screen)

Suspends printing, and displays a message on the device control panel. Check the message to select Continue Printing or Cancel Printing.

## Host Interface

Configure the network connection-related settings.

### I/O Buffer

Set the I/O Buffer's memory size.

Note

- Normally it is not necessary to change this setting.

### I/O Timeout

Set the number of seconds the printer waits before ending a print job if more data is not received through parallel interface or USB. When the specified period elapses, data reception through other interfaces is possible.

Note

- If the value specified is too small, a timeout may occur in the middle of a print job.

## PCL Menu

Configure settings for PCL printing.

Note

- Each of values set in the PCL Menu area may be reset to default by the validity test, performed when PCL is started.

### Orientation

Select the page orientation.

### Form Lines

Enter the number of lines per page. You can enter between 5 and 128 lines.

### Font Source

Set the default font location.

### Font Number

Set the ID of the default font you want to use.

### Point Size

Set the point size you want for the default font. You can enter between 4 and 999.75, in increments of 0.25.

### Font Pitch

Set the number of characters per inch you want for the default font. You can enter between 0.44 and 99.99, in increments of 0.01.

### Symbol Set

Specify the default font character set.

### Nimbus Mono Font

Select the Nimbus Mono font type.

### Extend A4 Width

Select to increase the width of the printable area for A4 paper, leaving narrow side margins.

### Append CR to LF

Select to add a CR code to each LF code.

### Resolution

Set the print resolution in dots per inch.

### Toner Saving

Reduces the amount of toner used when printing. While this increases the life of the toner cartridge, the output appears slightly lighter.

## PS Menu

Configure settings for PS printing.

### Job Timeout

Specify whether or not to apply a timeout limit if the machine takes longer than a specified time to process a job.
To apply a timeout limit, select Use Machine Setting(s), and then specify the time that must elapse (up to 999 seconds) before the timeout is applied. If you enter "0", the machine does not apply a timeout limit.

### Wait Timeout

Specify whether or not to apply a timeout limit if the machine waits longer than a specified time for job data.
To apply a timeout limit, select Use Machine Setting(s), and then specify the time that must elapse (up to 999 seconds) before the timeout is applied. If you enter "0", the machine does not apply a timeout limit.

### Paper Selection Method

Select the default method for paper selection.

### Switching between 1 & 2 Sided Print Functions

Specify whether or not to continue the 2-sided print when a specific command is inserted between the front and back sides of the job in the 2-sided print process.

### Data Format

Select the data format.

### Resolution

Set the print resolution in dots per inch.

### Toner Saving

Reduces the amount of toner used when printing. While this increases the life of the toner cartridge, the output appears slightly lighter.

### Color Setting

Specify whether to apply color correction when converting an RGB color image into a CMYK color image, and if yes, select the correction level.

### Color Profile

Select the color profile you want to use.

#### Auto

The printer automatically selects an appropriate color profile according to the job data.

#### Presentation

Text color reproduction is improved.

#### Solid Color

Solid color area reproduction is improved (optimal for artwork and graphics).

#### Photographic

Gray scale image reproduction is improved.

#### User Setting

The color profile embedded in the job data is used.

### Process Color Model

Select the process color model that you want to apply.

### Orientation Auto Detect

Specify whether or not the machine automatically detects the image orientation (Portrait/Landscape) of the job data it receives.
To enable auto detection of orientation, select On.

### Gray Reproduction

Select the printing method appropriate for black and gray areas of documents.

#### Black/Gray by K (Black)

Prints black and gray using black toner only. Compared to the black printed with CMYK toner, this results in a black that is relatively flatter and purer.

Note:

- Depending on the application you are using, black and gray images may print with CMYK toner even if Black/Gray by K (Black) is selected.

#### Black by K (Black)

Prints black text and graphics using black toner only.

#### CMY + K

Prints black and gray on all pages using four colors: CMY (Cyan, Magenta, and Yellow) and K (Black).

#### Black/Gray by K (Black) -Text Only

Prints black and gray text using black toner only.

#### Black by K (Black) -Text Only

Prints black text using black toner only.

#### Black/Gray by K-Strong UCR

Prints all black and gray objects using black toner only regardless of whether the document is in color or black and white. This is useful when a black and gray image or scanned black text might print with CMYK toner even if Black/Gray by K (Black) is selected.

### Font Change Confirmation

Specify whether or not to display the confirmation window when the Adobe fonts are specified in the printer driver.

Note

- This item does not appear if optional Adobe PostScript3 is installed.

#### Display

A confirmation window will appear. You can specify whether to replace Adobe fonts with substitutes and print a job or to cancel it. You can also check more details of information.

#### Do not Display

A job is printed replacing Adobe fonts with substitutes without the confirmation window.

## PDF Menu

Configure settings for PDF printing.

### Reverse Order Printing

Specify whether to start printing from the last page.

### Resolution

Set the print resolution in dots per inch.

### Toner Saving

Reduces the amount of toner used when printing. While this increases the life of the toner cartridge, the output appears slightly lighter.

### Color Setting

Specify whether to apply color correction when converting an RGB color image into a CMYK color image, and if yes, select the correction level.

### Color Profile

Select the color profile you want to use.

#### Auto

The printer automatically selects an appropriate color profile according to the job data.

#### Presentation

Text color reproduction is improved.

#### Solid Color

Solid color area reproduction is improved (optimal for artwork and graphics).

#### Photographic

Gray scale image reproduction is improved.

#### User Setting

The color profile embedded in the job data is used.

### Process Color Model

Select the process color model that you want to apply.

### Orientation Auto Detect

Specify whether or not the machine automatically detects the image orientation (Portrait/Landscape) of the job data it receives.
To enable auto detection of orientation, select On.

## XPS Menu

Configure settings for XPS printing.

### Resolution

Set the print resolution in dots per inch.

### Toner Saving

Reduces the amount of toner used when printing. While this increases the life of the toner cartridge, the output appears slightly lighter.

### Color Profile

Select the color profile you want to use.

#### Auto

The printer automatically selects an appropriate color profile according to the job data.

#### Text

Text color reproduction is improved.

#### Photo

Gray scale image reproduction is improved.

#### Graphics

Solid color area reproduction is improved (optimal for artwork and graphics).

### Process Color Model

Select the process color model that you want to apply.

### Gray Reproduction

Select the printing method appropriate for black and gray areas of documents.

#### Black/Gray by K (Black)

Prints black and gray using black toner only. Compared to the black printed with CMYK toner, this results in a black that is relatively flatter and purer.

Note:

- Depending on the application you are using, black and gray images may print with CMYK toner even if Black/Gray by K (Black) is selected.

#### Black by K (Black)

Prints black text and graphics using black toner only.

#### CMY + K

Prints black and gray on all pages using four colors: CMY (Cyan, Magenta, and Yellow) and K (Black).

#### Black/Gray by K (Black) -Text Only

Prints black and gray text using black toner only.

#### Black by K (Black) -Text Only

Prints black text using black toner only.

#### Black/Gray by K-Strong UCR

Prints all black and gray objects using black toner only regardless of whether the document is in color or black and white. This is useful when a black and gray image or scanned black text might print with CMYK toner even if Black/Gray by K (Black) is selected.

## IPDS Menu

Configure settings for IPDS.

### Tray Form

Allocate an IPDS form to each paper tray.
For each paper tray, select the form you want to allocate to it.

### Emulation Mode

Select the emulation mode.

### Print Mode

Select the print resolution in dots per inch.

### Default Code Page

Specify the default code page.

### Default FGID

Specify the default FGID (Font Typeface Global Identifier), which identifies the default resident font.

### Characters Per Inch

Select the pitch (in characters per inch) of the default font.

### Valid Printable Area Check

Specify whether or not to enable valid printable area checking.

### Edge to Edge

Specify whether or not to enable edge-to-edge printing.

### Font Substitution

Specify whether or not to enable font substitution.

### Resource Capture

Specify whether or not to enable the resource capture.

### Resolution

Specify the resolution reported to the host in the IPDS XOA-OPC command for raster coded fonts and IM1 images support.

### Graphic Character String

Select the Graphic Character String (Graphic Character Sizing) processing method.

### Bar Code

Specify the bar code level.

### Box Draw

Select the box draw processing method.

### Color Simulation

Select the color simulation.

### Text Color Simulation

Specify whether or not to enable the text color simulation.

### Suppress Staple Count Nacks

Specify whether or not to notify the host of stapling errors.

### Suppress Punch Nacks

Specify whether or not to notify the host of punching errors.

### Tray Mapping

Configure settings for the tray mapping.
If you select Auto, the default host media source ID is automatically selected for the media source (input tray).
If you select IPDS Tray, manually enter the ID number (between 0 and 254) the host uses for the media source.

### Corner Staple Angle

Select the angle of the corner staple.

### Offset

Specify whether or not the output is offset (jogged).
On - Default setting. Output is offset if the job's settings specify offset output.
Off - Output is not offset, even if the job's settings specify offset output.

### Default Punch Pattern

Select the default number of holes to punch if the punch unit provides a selection (for example, two or four holes).

### Color Management

Configure settings for the color management.

#### Input Profile: CMYK

Specify the input profile to use for CMYK objects.

#### Input Profile: RGB

Specify the input profile to use for RGB objects.

#### Input Profile: Gray

Specify the input profile to use for gray objects.

#### Rendering Intent

Specify the rendering intent you want to use.

#### Preserve K for Black/Gray

You can maintain K only black/gray in the same amount as the source document. This K black is 100% black (flat black or standard black) with no other toner in the mix. It prevents colors specified as K-only from being converted to process black (CMY).

#### Black and White Printing

Specify whether or not to print color print jobs in black and white.

## Buttons

### Refresh

Click to update the currently displayed information.

Note

- Before making the settings, click Refresh to obtain the machine's current status.

### OK

Click to apply the settings.

### Cancel

Click to cancel the settings.

##