# Folder Destination
Device Management > Address Book > Add User (Easy Input) > Folder Destination

By creating a shared folder on the network, you can transfer a file scanned by the scanner function to this folder.

### Protocol

Select the protocol for file transfer.

### Port No.

Enter the port number used when transferring a file by FTP. You can enter a value between 1 and 65535. The default is 21.

### Server Name

Enter the name of the connected server used when transferring a file by FTP. You can enter up to 64 characters.

### Path

Enter the shared folder path. You can enter up to 256 characters.

Note

- When a file is transferred by SMB, an error will occur if the strings of the server name and/or the shared folder name in the path exceed 128 characters.

### Login User Name

Enter the name of a user who has write privileges to the shared folder. If you are using FTP, you can enter up to 64 alphanumeric characters. If you are using SMB, you can enter up to 64 characters.

### Login Password

Enter the password of the user entered in the Login User Name box. You can enter up to 64 alphanumeric characters.

### Confirm Login Password

Enter the password again to confirm it.
The password entered here must be the same as that entered earlier in Login Password. If it is not, the password cannot be changed.

## Buttons

### Back

Click to return to the previous page.

### Go to Next

Click to save the settings and go to the next page.

### Cancel

Click to return to the Address List (Display All Items) page.

##