| Network Key (Password) Configuration
| Enter the appropriate network key and click "Next". There are some rules for each authentication method.
| Open System/Shared Key with WEP This key is a 64-bit or 128-bit value that must be entered in an ASCII or hexadecimal format. 64 (40) bit ASCII: Uses 5 text characters, for example "WSLAN" (case-sensitive). 64 (40) bit hexadecimal: Uses 10 digits of hexadecimal data, for example "71f2234aba". 128 (104) bit ASCII: Uses 13 text characters, for example "Wirelesscomms" (case-sensitive). 128 (104) bit hexadecimal: Uses 26 digits of hexadecimal data, for example "71f2234ab56cd709e5412aa2ba". WPA-PSK/WPA2-PSK and TKIP or AES Uses a Pre-Shared Key (PSK) between 8 and 63 characters in length.