;*****************************************************************************
;*
;*  l1e51x64.INF  -   Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller
;*  Copyright 2005-, Atheros Technology.
;*
;*****************************************************************************
[Version]
Signature   = "$WINDOWS NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %Atheros%
CatalogFile = l1e51x64.cat
Compatible  = 1
DriverVer   = 12/02/2009,1.0.0.41

[Manufacturer]
%Atheros% = Atheros,NTamd64

[Atheros.NTamd64]
; DisplayName           Section         	DeviceID
; -----------           -------         	--------
%Atheros.L1e%   =       L1e.ndi,        	PCI\VEN_1969&DEV_1026
%Atheros.L1e%   =       L2eRB.ndi,      	PCI\VEN_1969&DEV_1026&REV_F0
%Atheros.L1e%   =       L1e.ndi,        	PCI\VEN_1969&DEV_1026&SUBSYS_10261969&REV_B0
%Atheros.L1e%   =       L2eRB.ndi,      	PCI\VEN_1969&DEV_1026&SUBSYS_10261969&REV_F0
%Atheros.L1e%   =       L1e.ndi,       		PCI\VEN_1969&DEV_1026&SUBSYS_83041043&REV_B0
%Atheros.L1e%   =       L1e.ndi,       		PCI\VEN_1969&DEV_1026&SUBSYS_83391043&REV_B0
%Atheros.L1e%   =       L1e.ndi,       		PCI\VEN_1969&DEV_1026&SUBSYS_831C1043&REV_B0
%Atheros.L1e%   =       L1e.ECS.ndi,    	PCI\VEN_1969&DEV_1026&SUBSYS_10261019&REV_B0
%Atheros.L1e%   =       L1e.ECS.ndi,    	PCI\VEN_1969&DEV_1026&SUBSYS_00501B0A&REV_B0  ; Pegatron
%Atheros.L1e%   =       L1e.ECS.ndi,    	PCI\VEN_1969&DEV_1026&SUBSYS_00681B0A&REV_B0  ; Pegatron
%Atheros.L1e%   =       L1e.PEGA.ndi, 	        PCI\VEN_1969&DEV_1026&SUBSYS_00821B0A&REV_B0  ; Pegatron
%Atheros.L1e%   =       L1e.PEGA.ndi, 	        PCI\VEN_1969&DEV_1026&SUBSYS_00BE1B0A&REV_B0  ; Pegatron
%Atheros.L1e%   =       L1e.WOLMagic.ndi,    	PCI\VEN_1969&DEV_1026&SUBSYS_00631B0A&REV_B0  ; Pegatron
%Atheros.L1e%   =       L1e.WOLMagic.ndi,    	PCI\VEN_1969&DEV_1026&SUBSYS_00871B0A&REV_B0  ; Pegatron
%Atheros.L1e%   =       L1e.PEGA.ndi,    	PCI\VEN_1969&DEV_1026&SUBSYS_00911B0A&REV_B0  ; Pegatron
%Atheros.L1e%   =       L1e.PEGA.ndi,    	PCI\VEN_1969&DEV_1026&SUBSYS_00A51B0A&REV_B0  ; Pegatron
%Atheros.L1e%   =       L1e.DisS5.ndi,    	PCI\VEN_1969&DEV_1026&SUBSYS_15051043&REV_B0  ; ASUS
%Atheros.L1e%   =       L1e.DisS5.ndi,    	PCI\VEN_1969&DEV_1026&SUBSYS_14F51043&REV_B0  ; ASUS
%Atheros.L1e%   =       L1e.DisS5.ndi,    	PCI\VEN_1969&DEV_1026&SUBSYS_18211043&REV_B0  ; ASUS
%Atheros.L1e%   =       L1e.DisS5.ndi,    	PCI\VEN_1969&DEV_1026&SUBSYS_18221043&REV_B0  ; ASUS
%Atheros.L1e%   =       L1e.ndi,       		PCI\VEN_1969&DEV_1026&SUBSYS_202A1B0A&REV_B0  ; Pegatron_Colt
%Atheros.L1e%   =       L1e.ndi,       		PCI\VEN_1969&DEV_1026&SUBSYS_00B91B0A&REV_B0  ; Pegatron_Spring_Peak

%Atheros.L1e%   =       L1e.zk.ndi,             PCI\VEN_1969&DEV_1026&SUBSYS_002F1B0A&REV_B0  ; Unihan

%Atheros.L1e%   =       L1e.kili.ndi,        	PCI\VEN_1969&DEV_1026&SUBSYS_01461025&REV_B0  ; Kili
%Atheros.L1e%   =       L2eRB.kili.ndi,      	PCI\VEN_1969&DEV_1026&SUBSYS_01461025&REV_F0
%Atheros.L1e%   =       L1e.kili.ndi,        	PCI\VEN_1969&DEV_1026&SUBSYS_01451025&REV_B0  ; Teton
%Atheros.L1e%   =       L2eRB.kili.ndi,      	PCI\VEN_1969&DEV_1026&SUBSYS_01451025&REV_F0

%Atheros.L1e%   =       L1e.zk.ndi,             PCI\VEN_1969&DEV_1026&SUBSYS_01671025&REV_B0  ; KAL90
%Atheros.L1e%   =       L1e.zk.ndi,             PCI\VEN_1969&DEV_1026&SUBSYS_01281025&REV_B0  ; KAVH0
%Atheros.L1e%   =       L1e.zk.ndi,             PCI\VEN_1969&DEV_1026&SUBSYS_019C1025&REV_B0  ; KAV10
%Atheros.L1e%   =       L1e.zk.ndi,             PCI\VEN_1969&DEV_1026&SUBSYS_02101025&REV_B0  ; KAWH0
%Atheros.L1e%   =       L1e.zk.ndi,             PCI\VEN_1969&DEV_1026&SUBSYS_02111025&REV_B0  ; KBWH0
%Atheros.L1e%   =       L1e.zk.ndi,             PCI\VEN_1969&DEV_1026&SUBSYS_02121025&REV_B0  ; KAWF0
%Atheros.L1e%   =       L1e.zk.ndi,             PCI\VEN_1969&DEV_1026&SUBSYS_02131025&REV_B0  ; KAWG0
%Atheros.L1e%   =       L1e.zk.ndi,             PCI\VEN_1969&DEV_1026&SUBSYS_022C1025&REV_B0  ; ZG8
%Atheros.L1e%   =       L1e.zk.ndi,             PCI\VEN_1969&DEV_1026&SUBSYS_021B1025&REV_B0  ; KBLG0
%Atheros.L1e%   =       L1e.zk.ndi,             PCI\VEN_1969&DEV_1026&SUBSYS_02601025&REV_B0  ; KALG0
%Atheros.L1e%   =       L1e.zk.ndi,             PCI\VEN_1969&DEV_1026&SUBSYS_022E1025&REV_B0  ; KAW10
%Atheros.L1e%   =       L1e.zk.ndi,             PCI\VEN_1969&DEV_1026&SUBSYS_028D1025&REV_B0  ; HM50/70-PU

%Atheros.L1e%   =       L1e.zk.ndi,             PCI\VEN_1969&DEV_1026&SUBSYS_015E1025&REV_B0  ; ZK2
%Atheros.L1e%   =       L1e.zk.ndi,             PCI\VEN_1969&DEV_1026&SUBSYS_01661025&REV_B0  ; ZK3
%Atheros.L1e%   =       L1e.zk.ndi,             PCI\VEN_1969&DEV_1026&SUBSYS_02161025&REV_B0  ; HM20-YK

%Atheros.L1e%   =       L1e.zk.ndi,             PCI\VEN_1969&DEV_1026&SUBSYS_02141025&REV_B0  ; HM40-MV
%Atheros.L1e%   =       L1e.zk.ndi,             PCI\VEN_1969&DEV_1026&SUBSYS_019D1025&REV_B0  ; 
%Atheros.L1e%   =       L1e.zk.ndi,             PCI\VEN_1969&DEV_1026&SUBSYS_02151025&REV_B0  ; HM40-YK
%Atheros.L1e%   =       L1e.zk.ndi,             PCI\VEN_1969&DEV_1026&SUBSYS_030D1025&REV_B0  ; HM41

%Atheros.L1e%   =       L1e.zk.ndi,             PCI\VEN_1969&DEV_1026&SUBSYS_0CD9105B&REV_B0  ; SZ902

; Windows NT specific entry
[L1e.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1e.reg, L1e.params, L1e.Params.WinNT, Common.Params, ShutOff.params, WOLDefault.params
CopyFiles       = L1e.CopyFiles

[L1e.ndi.NT.Services]
AddService = L1e, 2, L1e.Service, Common.EventLog

[L1e.ShutOn.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1e.reg, L1e.pega.params, L1e.params, L1e.Params.WinNT, Common.Params, ShutOn.params, WOLDefault.params
CopyFiles       = L1e.CopyFiles

[L1e.ShutOn.ndi.NT.Services]
AddService = L1e, 2, L1e.Service, Common.EventLog

[L1e.DisS5.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1e.reg, L1e.ecs.params, L1e.params, L1e.Params.WinNT, Common.Params, WOLDefault.params
CopyFiles       = L1e.CopyFiles

[L1e.DisS5.ndi.NT.Services]
AddService = L1e, 2, L1e.Service, Common.EventLog

[L1e.WOLMagic.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1e.reg, L1e.pega.params, L1e.params, L1e.Params.WinNT, Common.Params, ShutOn.params, WOLMagic.params
CopyFiles       = L1e.CopyFiles

[L1e.WOLMagic.ndi.NT.Services]
AddService = L1e, 2, L1e.Service, Common.EventLog

; L1e for ECS
[L1e.ECS.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1e.reg, L1e.ecs.params, L1e.params, L1e.Params.WinNT, Common.Params, ShutOff.params, WOLDefault.params
CopyFiles       = L1e.CopyFiles

[L1e.ECS.ndi.NT.Services]
AddService = L1e, 2, L1e.Service, Common.EventLog

[L1e.kili.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1e.reg, L1e.kili.params, L1e.params, L1e.Params.WinNT, Common.Params, ShutOff.params, WOLDefault.params
CopyFiles       = L1e.CopyFiles

[L1e.kili.ndi.NT.Services]
AddService = L1e, 2, L1e.Service, Common.EventLog

[L1e.zk.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1e.reg, L1e.zk.params, L1e.params, L1e.Params.WinNT, Common.Params, ShutOff.params, WOLDefault.params
CopyFiles       = L1e.CopyFiles

[L1e.zk.ndi.NT.Services]
AddService = L1e, 2, L1e.Service, Common.EventLog

[L1e.PEGA.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1e.reg, L1e.pega.params, L1e.params, L1e.Params.WinNT, Common.Params, ShutOff.params, WOLDefault.params
CopyFiles       = L1e.CopyFiles

[L1e.PEGA.ndi.NT.Services]
AddService = L1e, 2, L1e.Service, Common.EventLog

; L2e reversion B.
[L2eRB.kili.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1e.reg, L1e.kili.params, L2eRB.params, L1e.Params.WinNT, Common.Params, ShutOff.params, WOLDefault.params
CopyFiles       = L1e.CopyFiles

[L2eRB.kili.ndi.NT.Services]
AddService = L1e, 2, L1e.Service, Common.EventLog

[L2eRB.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1e.reg, L2eRB.params, L1e.Params.WinNT, Common.Params, ShutOff.params, WOLDefault.params
CopyFiles       = L1e.CopyFiles

[L2eRB.ndi.NT.Services]
AddService = L1e, 2, L1e.Service, Common.EventLog

;-----------------------------------------------------------------------------
; L1e NT specific
;
[L1e.reg]
HKR, Ndi, HelpText,, %HelpText%
HKR, Ndi, Service,    0, "L1e"
; use ndis5 as the upper bound because NT supports it
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

[L1e.Service]
DisplayName     = %L1e.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\l1e51x64.sys
LoadOrderGroup  = NDIS

[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR,, EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\Drivers\l1e51x64.sys"
HKR,, TypesSupported,   0x00010001, 7

[L1e.ecs.params]
HKR,, LedMode,	0x00010001,	1

[L1e.kili.params]
HKR,, LedMode,	0x00010001,	2 ; for Kili, Teton.

[L1e.zk.params]
HKR,, LedMode,	0x00010001,	3 ; for zk2, zk3.

[L1e.pega.params]
HKR,, LedMode,	0x00010001,	4 ;for Pegatron

[L2eRB.params]
HKR,, IsL2eRB,	0x00010001,	1

HKR, Ndi\Params\MaxFrameSize,   ParamDesc,, %MTU%
HKR, Ndi\Params\MaxFrameSize,   Type,,      "int"
HKR, Ndi\Params\MaxFrameSize,   Base,,      "10"
HKR, Ndi\Params\MaxFrameSize,   Min,,       "500"
HKR, Ndi\Params\MaxFrameSize,   Max,,       "1514"
HKR, Ndi\Params\MaxFrameSize,   Step,,      "1"
HKR, Ndi\Params\MaxFrameSize,   Default,,   "1514"


[L1e.params]
HKR, Ndi\Params\MaxFrameSize,   ParamDesc,, %MTU%
HKR, Ndi\Params\MaxFrameSize,   Type,,      "int"
HKR, Ndi\Params\MaxFrameSize,   Base,,      "10"
HKR, Ndi\Params\MaxFrameSize,   Min,,       "500"
HKR, Ndi\Params\MaxFrameSize,   Max,,       "7168"
HKR, Ndi\Params\MaxFrameSize,   Step,,      "1"
HKR, Ndi\Params\MaxFrameSize,   Default,,   "1514"


[Common.Params]
HKR, Ndi\Params\APSmode,    	ParamDesc,,  %APSmode%
HKR, Ndi\Params\APSmode,    	Type,,       "enum"
HKR, Ndi\Params\APSmode,    	Default,,    "0"
HKR, Ndi\Params\APSmode\enum, 	"1",,        %On%
HKR, Ndi\Params\APSmode\enum, 	"0",,        %Off%

HKR, Ndi\Params\NetworkAddress, ParamDesc,, %NetAddr%
HKR, Ndi\Params\NetworkAddress, Type,,      "edit"
HKR, Ndi\Params\NetworkAddress, LimitText,, "18"
HKR, Ndi\Params\NetworkAddress, UpperCase,, "1"
HKR, Ndi\Params\NetworkAddress, Default,,   ""
HKR, Ndi\Params\NetworkAddress, Optional,,  "1"

HKR, Ndi\Params\MaxInterrupt,   ParamDesc,, %MaxIrq%
HKR, Ndi\Params\MaxInterrupt,   Type,,      "int"
HKR, Ndi\Params\MaxInterrupt,   Base,,      "10"
HKR, Ndi\Params\MaxInterrupt,   Min,,       "1000"
HKR, Ndi\Params\MaxInterrupt,   Max,,       "30000"
HKR, Ndi\Params\MaxInterrupt,   Step,,      "200"
HKR, Ndi\Params\MaxInterrupt,   Default,,   "5000"

HKR, Ndi\Params\MediaType,  ParamDesc,,     %MediaType%
HKR, Ndi\Params\MediaType,  Type,,          "enum"
HKR, Ndi\Params\MediaType,  Default,,       "0"
HKR, Ndi\Params\MediaType\enum,     "0",,   %Auto%
HKR, Ndi\Params\MediaType\enum,     "1",,   %100MFD%
HKR, Ndi\Params\MediaType\enum,     "2",,   %100MHD%
HKR, Ndi\Params\MediaType\enum,     "3",,   %10MFD%
HKR, Ndi\Params\MediaType\enum,     "4",,   %10MHD%

HKR, Ndi\Params\FlowControl,    ParamDesc,,  %FlowCtrl%
HKR, Ndi\Params\FlowControl,    Type,,       "enum"
HKR, Ndi\Params\FlowControl,    Default,,    "1"
HKR, Ndi\Params\FlowControl\enum, "1",,      %On%
HKR, Ndi\Params\FlowControl\enum, "0",,      %Off%

[WOLDefault.params]
HKR, Ndi\Params\WakeUpCapability,   ParamDesc,,     %WakeUpCapabilities%
HKR, Ndi\Params\WakeUpCapability,   Type,,          "enum"
HKR, Ndi\Params\WakeUpCapability,   Default,,       "6"
HKR, Ndi\Params\WakeUpCapability\enum, "0",,         %None%
HKR, Ndi\Params\WakeUpCapability\enum, "1",,         %LinkChange%
HKR, Ndi\Params\WakeUpCapability\enum, "2",,         %MagicPacket%
HKR, Ndi\Params\WakeUpCapability\enum, "4",,         %PatternMatch%
HKR, Ndi\Params\WakeUpCapability\enum, "3",,         %Link_Magic%
HKR, Ndi\Params\WakeUpCapability\enum, "5",,         %Link_Pattern%
HKR, Ndi\Params\WakeUpCapability\enum, "6",,         %Magic_Pattern%
HKR, Ndi\Params\WakeUpCapability\enum, "7",,         %All%

[WOLMagic.params]
HKR, Ndi\Params\WakeUpCapability,   ParamDesc,,     %WakeUpCapabilities%
HKR, Ndi\Params\WakeUpCapability,   Type,,          "enum"
HKR, Ndi\Params\WakeUpCapability,   Default,,       "2"
HKR, Ndi\Params\WakeUpCapability\enum, "0",,         %None%
HKR, Ndi\Params\WakeUpCapability\enum, "1",,         %LinkChange%
HKR, Ndi\Params\WakeUpCapability\enum, "2",,         %MagicPacket%
HKR, Ndi\Params\WakeUpCapability\enum, "4",,         %PatternMatch%
HKR, Ndi\Params\WakeUpCapability\enum, "3",,         %Link_Magic%
HKR, Ndi\Params\WakeUpCapability\enum, "5",,         %Link_Pattern%
HKR, Ndi\Params\WakeUpCapability\enum, "6",,         %Magic_Pattern%
HKR, Ndi\Params\WakeUpCapability\enum, "7",,         %All%

[ShutOn.params]
HKR, Ndi\Params\ShutdownWake,   ParamDesc,, %ShutDW%
HKR, Ndi\Params\ShutdownWake,   Type,,      "enum"
HKR, Ndi\Params\ShutdownWake\enum,1,,       %On%
HKR, Ndi\Params\ShutdownWake\enum,0,,       %Off%
HKR, Ndi\Params\ShutdownWake,   Default,,   "1"

[ShutOff.params]
HKR, Ndi\Params\ShutdownWake,   ParamDesc,, %ShutDW%
HKR, Ndi\Params\ShutdownWake,   Type,,      "enum"
HKR, Ndi\Params\ShutdownWake\enum,1,,       %On%
HKR, Ndi\Params\ShutdownWake\enum,0,,       %Off%
HKR, Ndi\Params\ShutdownWake,   Default,,   "0"

[L1e.Params.WinNT]
HKR, Ndi\Params\TaskOffload,    ParamDesc,, %TOff%
HKR, Ndi\Params\TaskOffload,    Type,,      "enum"
HKR, Ndi\Params\TaskOffload\enum,1,,        %On%
HKR, Ndi\Params\TaskOffload\enum,0,,        %Off%
HKR, Ndi\Params\TaskOffload,    Default,,   "1"

HKR, Ndi\Params\MaxRxBuffer,    ParamDesc,, %NumRx%
HKR, Ndi\Params\MaxRxBuffer,    Type,,      "int"
HKR, Ndi\Params\MaxRxBuffer,    Base,,      "10"
HKR, Ndi\Params\MaxRxBuffer,    Min,,       "3"
HKR, Ndi\Params\MaxRxBuffer,    Max,,       "64"
HKR, Ndi\Params\MaxRxBuffer,    Step,,      "1"
HKR, Ndi\Params\MaxRxBuffer,    Default,,   "6"

HKR, Ndi\Params\MaxTxBuffer,    ParamDesc,, %NumTx%
HKR, Ndi\Params\MaxTxBuffer,    Type,,      "int"
HKR, Ndi\Params\MaxTxBuffer,    Base,,      "10"
HKR, Ndi\Params\MaxTxBuffer,    Min,,       "1"
HKR, Ndi\Params\MaxTxBuffer,    Max,,       "32"
HKR, Ndi\Params\MaxTxBuffer,    Step,,      "1"
HKR, Ndi\Params\MaxTxBuffer,    Default,,   "2"

;-----------------------------------------------------------------------------
; DestinationDirs
;
[L1e.CopyFiles]
l1e51x64.sys,,,2

[SourceDisksNames]
;
; diskid = description[, [tagfile] [, <unused>, subdir]]
;
1 = %DriverDisk%,,,

[SourceDisksFiles]
;
; filename_on_source = diskID[, [subdir][, size]]
;
l1e51x64.sys = 1

[DestinationDirs]
L1e.CopyFiles   = 12
DefaultDestDir  = 11

[Strings]
Atheros                 = "Atheros"
APSmode			= "APS mode"
NetAddr         	= "Network Address"
MTU             	= "Maximum Frame Size"
TOff            	= "Task Offload"
MaxIrq          	= "Max IRQ per Second"
NumRx           	= "Number of Rx Buffers"
NumTx           	= "Number of Tx Buffers"
FlowCtrl        	= "Flow Control"
ShutDW          	= "Shutdown Wakeup"
MediaType       	= "MediaType"
Auto            	= "Auto"
10MHD           	= "10Mbps Half Duplex"
10MFD           	= "10Mbps Full Duplex"
100MHD          	= "100Mbps Half Duplex"
100MFD          	= "100Mbps Full Duplex"
WakeUpCapabilities      = "WakeUp Capabilities"
None            	= "None"
LinkChange      	= "Link Change"
MagicPacket     	= "Magic Packet"
PatternMatch    	= "Pattern Match"
Link_Magic      	= "LinkChange & MagicPacket"
Link_Pattern    	= "LinkChange & PatternMatch"
Magic_Pattern   	= "MagicPacket & PatternMatch"
All             	= "All"
On              	= "On"
Off             	= "Off"

Atheros.L1e          = "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
L1e.Service.DispName = "Miniport Driver for Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
DriverDisk           = "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller Installation Disk"
HelpText             = "This Atheros network Controller connects you to the network."
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Chinese (Taiwan)
[Strings.0404]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
APSmode			= "APS 模式"
NetAddr         	= "網路位址"
MTU             	= "框架大小上限"
TOff            	= "作業卸載"
MaxIrq          	= "每秒 IRQ 上限"
NumRx           	= "接收緩衝數量"
NumTx           	= "傳輸緩衝數量"
FlowCtrl        	= "流量控制"
ShutDW          	= "關閉狀態喚醒"
MediaType       	= "MediaType"
Auto            	= "自動"
10MHD           	= "10Mbps 半雙工"
10MFD           	= "10Mbps 全雙工"
100MHD          	= "100Mbps 半雙工"
100MFD          	= "100Mbps 全雙工"
WakeUpCapabilities      = "喚醒功能"
None            	= "無"
LinkChange      	= "Link Change"
MagicPacket     	= "Magic Packet"
PatternMatch    	= "Pattern Match"
Link_Magic      	= "LinkChange & MagicPacket"
Link_Pattern    	= "LinkChange & PatternMatch"
Magic_Pattern   	= "MagicPacket & PatternMatch"
All             	= "全部"
On              	= "開啟"
Off             	= "關閉"

Atheros.L1e          = "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
L1e.Service.DispName = "Miniport Driver for Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
DriverDisk           = "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller Installation Disk"
HelpText             = "This Atheros network Controller connects you to the network."
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; German (Standard)
[Strings.0407]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
APSmode			= "APS-Modus"
NetAddr         	= "Netzwerkadresse"
MTU             	= "Maximale Framegröße"
TOff            	= "Task-Offload"
MaxIrq          	= "Max. IRQ pro Sekunde"
NumRx           	= "Anzahl Rx-Puffer"
NumTx           	= "Anzahl Tx-Puffer"
FlowCtrl        	= "Flusssteuerung"
ShutDW          	= "Shutdown/Wakeup"
MediaType       	= "MediaType"
Auto            	= "Automatisch"
10MHD           	= "10 Mbit/s Halbduplex"
10MFD           	= "10 Mbit/s Vollduplex"
100MHD          	= "100 Mbit/s Halbduplex"
100MFD          	= "100 Mbit/s Vollduplex"
WakeUpCapabilities      = "WakeUp-Eigenschaften"
None            	= "Keine"
LinkChange      	= "Link Change"
MagicPacket     	= "Magic Packet"
PatternMatch    	= "Pattern Match"
Link_Magic      	= "LinkChange & MagicPacket"
Link_Pattern    	= "LinkChange & PatternMatch"
Magic_Pattern   	= "MagicPacket & PatternMatch"
All             	= "Alle"
On              	= "An"
Off             	= "Aus"

Atheros.L1e          = "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
L1e.Service.DispName = "Miniport Driver for Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
DriverDisk           = "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller Installation Disk"
HelpText             = "This Atheros network Controller connects you to the network."
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Spanish (Spain, Traditional Sort)
[Strings.040A]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
APSmode			= "Modo APS"
NetAddr         	= "Dirección de red"
MTU             	= "Tamaño máximo de trama"
TOff            	= "Descarga de tarea"
MaxIrq          	= "IRQ máx por segundo"
NumRx           	= "Número de búfers de recepción"
NumTx           	= "Número de búfers de transmisión"
FlowCtrl        	= "Control de flujo"
ShutDW          	= "Reactivar cierre"
MediaType       	= "MediaType"
Auto            	= "Automático"
10MHD           	= "Dúplex medio 10Mbps"
10MFD           	= "Dúplex completo 10Mbps"
100MHD          	= "Dúplex medio 100Mbps"
100MFD          	= "Dúplex completo 100Mbps"
WakeUpCapabilities      = "Capacidades de reactivación"
None            	= "Ninguno"
LinkChange      	= "Link Change"
MagicPacket     	= "Magic Packet"
PatternMatch    	= "Pattern Match"
Link_Magic      	= "LinkChange & MagicPacket"
Link_Pattern    	= "LinkChange & PatternMatch"
Magic_Pattern   	= "MagicPacket & PatternMatch"
All             	= "Todo"
On              	= "Activado"
Off             	= "Desactivado"

Atheros.L1e          = "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
L1e.Service.DispName = "Miniport Driver for Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
DriverDisk           = "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller Installation Disk"
HelpText             = "This Atheros network Controller connects you to the network."
; French (Standard)
[Strings.040C]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
APSmode			= "Mode APS"
NetAddr         	= "Adresse réseau"
MTU             	= "Taille maximale de la trame "
TOff            	= "Déchargement de tâche"
MaxIrq          	= "IRQ maxi. par seconde"
NumRx           	= "Nombre de tampons rx"
NumTx           	= "Nombre de tampons Tx"
FlowCtrl        	= "Contrôle de flux"
ShutDW          	= "Sortie de veille à l'arrêt"
MediaType       	= "MediaType"
Auto            	= "Automatique"
10MHD           	= "10 Mbits/s Semi-duplex"
10MFD           	= "10 Mbits/s Duplex intégral"
100MHD          	= "100 Mbits/s Semi-duplex"
100MFD          	= "100 Mbits/s Duplex intégral"
WakeUpCapabilities      = "Capacités de mise en éveil"
None            	= "Aucune"
LinkChange      	= "Changement de liaison"
MagicPacket     	= "Paquet magique"
PatternMatch    	= "Correspondance au modèle"
Link_Magic      	= "LinkChange et MagicPacket"
Link_Pattern    	= "LinkChange et PatternMatch"
Magic_Pattern   	= "MagicPack et PatternMatch"
All             	= "Tous"
On              	= "Activé"
Off             	= "Désactivé"

Atheros.L1e          = "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
L1e.Service.DispName = "Miniport Driver for Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
DriverDisk           = "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller Installation Disk"
HelpText             = "This Atheros network Controller connects you to the network."
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Italian (Standard)
[Strings.0410]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
APSmode			= "Modalità APS"
NetAddr         	= "Indirizzo di rete"
MTU             	= "Dimensioni massime frame"
TOff            	= "Offload attività"
MaxIrq          	= "Numero massimo di IRQ per secondo"
NumRx           	= "Numero di buffer Rx"
NumTx           	= "Numero di buffer Tx"
FlowCtrl        	= "Controllo di flusso"
ShutDW          	= "Attivazione arresto"
MediaType       	= "MediaType"
Auto            	= "Automatica"
10MHD           	= "Half Duplex 10 Mbps"
10MFD           	= "Full Duplex 10 Mbps"
100MHD          	= "Half Duplex 100 Mbps"
100MFD          	= "Full Duplex 100 Mbps"
WakeUpCapabilities      = "Capacità di attivazione"
None            	= "Nessuno"
LinkChange      	= "Modifica collegamento"
MagicPacket     	= "Magic Packet"
PatternMatch    	= "Corrispondenza motivo"
Link_Magic      	= "LinkChange e MagicPacket"
Link_Pattern    	= "LinkChange e PatternMatch"
Magic_Pattern   	= "MagicPacket e PatternMatch"
All             	= "Tutti"
On              	= "On"
Off             	= "Off"

Atheros.L1e          = "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
L1e.Service.DispName = "Miniport Driver for Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
DriverDisk           = "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller Installation Disk"
HelpText             = "This Atheros network Controller connects you to the network."
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Japanese
[Strings.0411]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
APSmode			= "APS モード"
NetAddr         	= "ネットワーク アドレス"
MTU             	= "最大フレーム サイズ"
TOff            	= "タスク オフロード"
MaxIrq          	= "最大 IRQ/秒"
NumRx           	= "Rx バッファ数"
NumTx           	= "Tx バッファ数"
FlowCtrl        	= "フロー制御"
ShutDW          	= "シャットダウン ウェークアップ"
MediaType       	= "MediaType"
Auto            	= "自動"
10MHD           	= "10 Mbps 半二重"
10MFD           	= "10 Mbps 全二重"
100MHD          	= "100 Mbps 半二重"
100MFD          	= "100 Mbps 全二重"
WakeUpCapabilities      = "ウェークアップ機能"
None            	= "なし"
LinkChange      	= "リンク変更"
MagicPacket     	= "マジック パケット"
PatternMatch    	= "パターン マッチ"
Link_Magic      	= "LinkChange と MagicPacket"
Link_Pattern    	= "LinkChange と PatternMatch"
Magic_Pattern   	= "MagicPacket と PatternMatch"
All             	= "すべて"
On              	= "オン"
Off             	= "オフ"

Atheros.L1e          = "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
L1e.Service.DispName = "Miniport Driver for Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
DriverDisk           = "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller Installation Disk"
HelpText             = "This Atheros network Controller connects you to the network."
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Dutch (Netherlands)
[Strings.0413]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
APSmode			= "APS-modus"
NetAddr         	= "Netwerkadres"
MTU             	= "Maximale framegrootte"
TOff            	= "Offload van taken"
MaxIrq          	= "Max. IRQ per seconde"
NumRx           	= "Aantal Rx-buffers"
NumTx           	= "Aantal Tx-buffers"
FlowCtrl        	= "Datatransportbesturing"
ShutDW          	= "Afsluiten Ontwaken"
MediaType       	= "MediaType"
Auto            	= "Automatisch"
10MHD           	= "10 Mbps half-duplex"
10MFD           	= "10 Mbps volledige duplex"
100MHD          	= "100 Mbps half-duplex"
100MFD          	= "100 Mbps volledige duplex"
WakeUpCapabilities      = "Mogelijkheden voor ontwaken"
None            	= "Geen"
LinkChange      	= "Wijziging koppeling"
MagicPacket     	= "Magic-pakket"
PatternMatch    	= "Patroonovereenkomst"
Link_Magic      	= "Wijziging koppeling en Magic-pakket"
Link_Pattern    	= "Wijziging koppeling en Patroonovereenkomst"
Magic_Pattern   	= "Magic-pakket en Patroonovereenkomst"
All             	= "Alles"
On              	= "Aan"
Off             	= "Uit"

Atheros.L1e          = "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
L1e.Service.DispName = "Miniport Driver for Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
DriverDisk           = "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller Installation Disk"
HelpText             = "This Atheros network Controller connects you to the network."
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Portuguese (Brazil)
[Strings.0416]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
APSmode			= "Modo APS"
NetAddr         	= "Endereço de Rede"
MTU             	= "Tamanho Máximo do Pacote"
TOff            	= "Descarga de Tarefas"
MaxIrq          	= "Max IRQ por Segundo"
NumRx           	= "Número de Rx Buffers"
NumTx           	= "Número de Tx Buffers"
FlowCtrl        	= "Controlo d Fluxo"
ShutDW          	= "Encerramento Reactivação"
MediaType       	= "MediaType"
Auto            	= "Automático"
10MHD           	= "10Mbps Half Duplex"
10MFD           	= "10Mbps Full Duplex"
100MHD          	= "100Mbps Half Duplex"
100MFD          	= "100Mbps Full Duplex"
WakeUpCapabilities      = "Capacidades de Reactivação"
None            	= "Nenhum"
LinkChange      	= "Alteração de Ligação"
MagicPacket     	= "Magic Packet"
PatternMatch    	= "Correspondência por Padrão"
Link_Magic      	= "Alteração de Ligação e MagicPacket"
Link_Pattern    	= "Alteração de Ligação e Correspondência por Padrão"
Magic_Pattern   	= "MagicPacket e Correspondência por Padrão"
All             	= "Todos"
On              	= "Ligado"
Off             	= "Desligado"

Atheros.L1e          = "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
L1e.Service.DispName = "Miniport Driver for Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
DriverDisk           = "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller Installation Disk"
HelpText             = "This Atheros network Controller connects you to the network."
; Chinese (PRC)
[Strings.0804]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
APSmode			= "APS 模式"
NetAddr         	= "网络地址"
MTU             	= "最大帧大小"
TOff            	= "任务卸载"
MaxIrq          	= "每秒最大 IRQ"
NumRx           	= "Rx 缓冲区数"
NumTx           	= "Tx 缓冲区数"
FlowCtrl        	= "流控制"
ShutDW          	= "关闭状态唤醒"
MediaType       	= "MediaType"
Auto            	= "自动"
10MHD           	= "10Mbps 半双工"
10MFD           	= "10Mbps 全双工"
100MHD          	= "100Mbps 半双工"
100MFD          	= "100Mbps 全双工"
WakeUpCapabilities      = "唤醒功能"
None            	= "无"
LinkChange      	= "链接更改"
MagicPacket     	= "幻数据包"
PatternMatch    	= "模式匹配"
Link_Magic      	= "LinkChange & MagicPacket"
Link_Pattern    	= "LinkChange & PatternMatch"
Magic_Pattern   	= "MagicPacket & PatternMatch"
All             	= "全部"
On              	= "开"
Off             	= "关"

;; Do NOT translate
;---------------------------------------------------------------------------------------------------

;-----------------------------------------------------------------------------

Atheros.L1e          = "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
L1e.Service.DispName = "Miniport Driver for Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller"
DriverDisk           = "Atheros AR8121/AR8113/AR8114 PCI-E Ethernet Controller Installation Disk"
HelpText             = "This Atheros network Controller connects you to the network."
