; Miix86_130.INF  -- WIA Driver setup file, 4800U2L-LL56
; Copyright (c) 2013 Microtek Corporation
; Manufacturer:  Microtek Scanner Driver Team

[Version]
Signature="$WINDOWS NT$"
Class=Image
ClassGUID={6bdd1fc6-810f-11d0-bec7-08002be2092f}
Provider=%Mfg%
DriverVer=04/24/2013,1.02.0003.1
CatalogFile.NTx86=Miix86_130.cat

[SourceDisksNames.x86]
1=%Location%,,,

[SourceDisksFiles.x86]
MSM6012W2.dll=1

[DestinationDirs]
DefaultDestDir=11

[Manufacturer]
%Mfg%=Models, NTx86

; This is the models section for the x86 driver
[Models.NTx86]
%USB\VID_05DA&PID_6012.DeviceDesc% = WIADRIVER.Device, USB\VID_05DA&PID_6012

[WIADRIVER.Device]
DriverVer=04/24/2013,1.02.0003.1
Include=sti.inf
Needs=STI.USBSection
SubClass=StillImage
DeviceType=1
DeviceSubType=0x1
Capabilities=0x10
PortSelect=NO
Events=WIADRIVER.Events
DeviceData=WIADRIVER.DeviceData
AddReg=WIADRIVER.AddReg
CopyFiles=WIADRIVER.CopyFiles
ICMProfiles="sRGB Color Space Profile.icm"

[WIADRIVER.Events]

[WIADRIVER.DeviceData]
UI Class ID={4DB1AD10-3391-11D2-9A33-00C04FA36145}
Server=local
UI DLL=sti.dll
PortType=5

[WIADRIVER.Device.Services]
Include=sti.inf
Needs=STI.USBSection.Services

[WIADRIVER.AddReg]
HKR,,HardwareConfig,1,1
HKR,,USDClass,,"{3AC0C671-51C8-4383-807B-876197D67C4C}"
HKCR,CLSID\{3AC0C671-51C8-4383-807B-876197D67C4C},,,"4800U2L-LL56"
HKCR,CLSID\{3AC0C671-51C8-4383-807B-876197D67C4C}\InProcServer32,,,%11%\MSM6012W2.dll
HKCR,CLSID\{3AC0C671-51C8-4383-807B-876197D67C4C}\InProcServer32,ThreadingModel,,"Both"
; The above GUID must change by different model.

[WIADRIVER.CopyFiles]
MSM6012W2.dll

[Strings]
Mfg="Microtek Driver Team"
Location="Microtek Scanning Software"
USB\VID_05DA&PID_6012.DeviceDesc = "4800U2L-LL56"

