; MiiAMD64_141.INF  -- WIA Driver setup file, 4800U2CScanner
; Copyright (c) 2016 Microtek Corporation
; Manufacturer:  Microtek Scanner Driver Team

[Version]
Signature="$WINDOWS NT$"
Class=Image
ClassGUID={6bdd1fc6-810f-11d0-bec7-08002be2092f}
Provider=%Mfg%
DriverVer=11/18/2016,1.02.0003.1
CatalogFile.ntamd64=MiiAMD64_141.cat

[SourceDisksNames.amd64]
1=%Location%,,,

[SourceDisksFiles.amd64]
MSM603FW2.dll=1

[DestinationDirs]
DefaultDestDir=11

[Manufacturer]
%Mfg%=Models, NTamd64

; This is the models section for the amd64 driver
[Models.NTamd64]
%USB\VID_05DA&PID_603F.DeviceDesc% = WIADRIVER.Device, USB\VID_05DA&PID_603F

[WIADRIVER.Device]
DriverVer=11/18/2016,1.02.0003.1
Include=sti.inf
Needs=STI.USBSection
SubClass=StillImage
DeviceType=1
DeviceSubType=0x1
Capabilities=0x10
PortSelect=NO
Events=WIADRIVER.Events
DeviceData=WIADRIVER.DeviceData
AddReg=WIADRIVER.AddReg
CopyFiles=WIADRIVER.CopyFiles
ICMProfiles="sRGB Color Space Profile.icm"

[WIADRIVER.Events]

[WIADRIVER.DeviceData]
UI Class ID={4DB1AD10-3391-11D2-9A33-00C04FA36145}
Server=local
UI DLL=sti.dll
PortType=5

[WIADRIVER.Device.Services]
Include=sti.inf
Needs=STI.USBSection.Services

[WIADRIVER.AddReg]
HKR,,HardwareConfig,1,1
HKR,,USDClass,,"{4763809C-4BCD-486E-A905-53DE72B4976B}"
HKCR,CLSID\{4763809C-4BCD-486E-A905-53DE72B4976B},,,"4800U2CScanner"
HKCR,CLSID\{4763809C-4BCD-486E-A905-53DE72B4976B}\InProcServer32,,,%11%\MSM603FW2.dll
HKCR,CLSID\{4763809C-4BCD-486E-A905-53DE72B4976B}\InProcServer32,ThreadingModel,,"Both"
; The above GUID must change by different model.

[WIADRIVER.CopyFiles]
MSM603FW2.dll

[Strings]
Mfg="Microtek Driver Team"
Location="Microtek Scanning Software"
USB\VID_05DA&PID_603F.DeviceDesc = "4800U2CScanner"

