; MiiAMD64_086.INF  -- WIA Driver setup file
; Copyright (c) 2011 Microtek Corporation
; Manufacturer:  Microtek Scanner Driver Team

[Version]
Signature="$WINDOWS NT$"
Class=Image
ClassGUID={6bdd1fc6-810f-11d0-bec7-08002be2092f}
Provider=%Mfg%
DriverVer=07/28/2011,1.72.0000.0
CatalogFile=MiiAMD64_086.cat

[SourceDisksNames.AMD64]
1=%Location%,,,

[SourceDisksFiles.AMD64]
MSMB5W2.dll=1

[DestinationDirs]
DefaultDestDir=11

[Manufacturer]
%Mfg%=Models, NTAMD64

; This is the models section for the amd64 driver
[Models.NTAMD64]
%USB\VID_05DA&PID_60B5.DeviceDesc% = USB.Device, USB\VID_05DA&PID_60B5


[USB.Device]
DriverVer=07/28/2011,1.72.0000.0
Include=sti.inf
Needs=STI.USBSection
SubClass=StillImage
DeviceType=1
DeviceSubType=0x1
Capabilities=0x10
PortSelect=NO
Events=WIADRIVER.Events
DeviceData=WIADRIVER.DeviceData
AddReg=WIADRIVER.AddReg
CopyFiles=WIADRIVER.CopyFiles
ICMProfiles="sRGB Color Space Profile.icm"


[WIADRIVER.Events]

[WIADRIVER.DeviceData]
UI Class ID={4DB1AD10-3391-11D2-9A33-00C04FA36145}
Server=local
UI DLL=sti.dll
PortType=5

[USB.Device.Services]
Include=sti.inf
Needs=STI.USBSection.Services

[WIADRIVER.AddReg]
HKR,,HardwareConfig,1,1
HKR,,USDClass,,"{B34B4A72-D539-4582-86C6-1B79AF2B4610}"
HKCR,CLSID\{B34B4A72-D539-4582-86C6-1B79AF2B4610},,,"4800U2L-FB"
HKCR,CLSID\{B34B4A72-D539-4582-86C6-1B79AF2B4610}\InProcServer32,,,%11%\MSMB5W2.dll
HKCR,CLSID\{B34B4A72-D539-4582-86C6-1B79AF2B4610}\InProcServer32,ThreadingModel,,"Both"
; The above GUID must change by different model.

[WIADRIVER.CopyFiles]
MSMB5W2.dll

[Strings]
Mfg="Microtek Driver Team"
Location="Microtek Scanning Software"
USB\VID_05DA&PID_60B5.DeviceDesc = "4800U2L-FB"

