8. Copying

8.1. Copying function

Copy | Instructions
Common copying | Multipage | Print a multi-page document to a piece of paper.
Clone | Print several identical images to a piece of paper.
Poster | Print a one-page original to pieces of paper.
Collated copy | Collate copies of an original.
Duplex copying | Duplex copying of the original can be achieved.
Image quality | Set the definition mode to improve the copying effect.
Intensity | Adjust deep-light copying effect by setting intensity.
Resizing | Reduce or enlarge the size of image copied.
Paper Size | Set the paper size.
Paper type | Set paper type.
ID copy | Arrangement mode | Set the ID copy layout.
Intensity | Adjust deep-light copying effect by setting intensity.
Paper Size | Set the paper size.
Receipt copying | Intensity | Adjust deep-light copying effect by setting intensity.
Paper Size | Set the paper size.

8.2. Copying method

1. Click “Copy” button/“ID copy” button/“Bill copy” button in control panel.

2. Put an original into the ADF with its front upward (only for plain copying) or on the glass platen with its front downward. (For how to put an original, please see Chapter 2.5.)

3. Click “Copy” button to copy.

4. Place the original text in the glass platen, scan this page, then give a prompt of "Scan next page". When there is another page to scan, take away the previous one, put the next one in the glass platen, click “Scan next page”. After scanning all the pages, click “End scan”.

8.3. Copying cancel

To cancel copy job, click “Cancel job” button.

8.4. Common copying setting

Change related setting through setting menu for better copy result.

1. Select “Copy” button in printer control panel;

2. Determine copy setting, click “Copy” button to copy.

| Note: | • The image quality, intensity, resizing and paper setting can keep valid after options are set. • Settings on all-in-one, clone, poster, collated copy and duplex copy will be restored to defaults after completing the copying, switching among panel keys or rebooting the machine.

8.4.1.Image quality

Select corresponding image quality mode for original document used in order to improve copying effect.

There are 4 modes in total:

Auto: default mode, applicable to text and image originals.

Text + image: applicable to originals with mixed text and image.

Image: applicable to original image.

Text: applicable to original text.

| Note: | • The image quality mode supports “automatic” mode only after “poster” and “collated copy” are set.

8.4.2.Intensity

Adjust deep-light copying effect by setting intensity.

8.4.3.Resizing

When original document is copied, resize image copied.

The resizing includes “fixed” and “manual adjustment” and the default value is 100%.

1. Fixed resizing: 100%、141% A5->A4、122% A5->B5、115% B5->A4、97% LTR->A4、94% A4->LTR、86% A4->B5、81% B5->A5、70% A4->A5.

e.g.: 70% A4->A5:

2.“Manual adjustment” applies to copying with glass platform only, the adjustment scope of which is 25%-400% and 5% can be adjusted each time after “direction key” is pressed once.

8.4.4.Multipage

With setting on all-in-one feature, a 2- or 4-page document could be copied to one piece of paper. Copying with the ADF and the glass platen are both supported.

The multipage includes 3 modes:

(1) Two-in-one:

(2) Horizontal four-in-one:

(3)vertical four-in-one:

| Note: | • "Multipage” and “resizing function” cannot be set at the same time.

8.4.5.Clone

Through setting on clone feature, you may print multiple original images on one piece of paper. Copying with the ADF and the glass platen are both supported.

The clone copying includes 3 modes:

2x2： 3x3： 4X4：

| Note: | • The “clone” and “resizing function” cannot be set at the same time.

8.4.6.Poster

Poster setting enables the printing of one piece of original document on several pieces of paper. The "Poster" feature supports only copying with the glass platen.

The poster copying includes 3 modes:

2x2： 3x3：4X4：

| Note: | • The “poster” and “resizing function” cannot be set at the same time.

8.4.7.Collated copy

The "Collated Copies" feature supports only copying with the automatic document feeder (ADF).

The collated copy includes 2 modes:

Startup:

Closed:

8.4.8.Duplex copy

You can use flat plate and ADF for Auto Duplex copy, ADF supports auto duplex copy.

There are 4 modes in total for duplex copying:

1. One-sided → One-sided:

2. One-sided → Two-sided:

3. Two-sided → One-sided:

4. Two-sided → Two-sided:

8.4.9.Paper setting

Select the paper size and paper type of original copying in Paper Settings menu.

Paper dimension: A4, Letter, B5, A5, A6, Executive, Legal and Folio.

Paper type: common paper, thick paper, envelope paper, film paper, card paper, tagboard and thin paper.

| Note: | • After “multipage” and “clone function” are set, “paper dimension” supports “A4” and “Letter” only. • For copying with the ADF, only plain paper is available in "Paper Type".

8.5. ID copy setting

Change related setting through setting menu for better copy result.

1. Select “ID Copy” button in printer control panel;

2. Determine copy setting, click “Copy” button to copy.

8.5.1.Arrangement mode

ID copy supports four layouts:

Whole page up-down | Half page up-down | Half page left-right | A5 left and right

Position:

Half page up-down: default mode; put ID card at “orange left half area” of glass platform.

Half-page up and down, half-page left and right or A5 left and right: put the ID card in the "blue area" in glass platen.

| Note: | • After setting, the arrangement mode can keep valid before startup; after startup, the arrangement mode will recover to default setting.

8.5.2.Intensity

Adjust copy luminosity through “Luminosity” setting.

8.5.3.Paper dimension

If arranged in modes of "Full Page Up and down", "Half-page Up and down" and "Half-page Left and right", the paper size supports "A4" and "Letter" only; if arranged in mode of "A5 Long Edge", the paper size supports "A5" only. Please follow instructions on panel to put the paper vertically for printing.

8.6. Receipt setting

Change related setting through setting menu for better copy result.

1. Select “Bill copy” button in printer control panel;

2. Determine copy setting, click “Copy” button to copy.

8.6.1.Intensity

Adjust copy luminosity through “Luminosity” setting.

8.6.2.Paper setting

The receipt copying supports A4, Letter, B5, A5, A6 and Executive paper dimension.