1.Before Using the Printer

1.1.Product series introduction

Product series parameters | BM4100FDN series | BM4100FDW series
Interface type | USB | ● | ●
NET | ● | ●
Wi-Fi |  | ●
Print Language
PDL | ● | ●
Control Panel | Touch screen | ● | ●
Print Speed | A4
33ppm | ● | ●
Letter
35ppm | ● | ●
Automatic Two-Sided Printing | ● | ●
Auto Duplex Scan | ● | ●
NFC function |  | ●
Mute printing | ● | ●
Copy | ● | ●
Scan | ● | ●
Fax | ● | ●
Scan to U-disk | ● | ●
USB print | ● | ●
Secure printing | ● | ●
ADF | ● | ●

(●: Support; Blank: Unsupport)

| Note: | • This product series is subject to additions or changes without prior notice. • The printer with fax should be set for language, time and fax as per window prompts upon initial starting or restoring factory settings. • For this user manual, the "ADF" is short for automatic document feeder.

1.2.Supplied Accessories

Name | Parts
Toner cartridge |
Drum component |
USB Interface Cable |
Power Cord |
CD |
Quick Setup Guide |
Pantum Warranty |

| Note: | • The Pantum Warranty may not be attached in some regions.

1.3.Product View

Side view

1 | Cover of automatic document feeder | This is used to remove the paper jammed in scanning for the ADF.
2 | Feed tray of automatic document feeder | This is used to place originals scanned from the ADF.
3 | Exit tray of automatic document feeder | Prevent originals scanned from falling off.
4 | Cover of scanner | Open the cover of scanner to place the scanned originals on its glass plate.
5 | Output Bin | For storing the printed paper.
6 | Front USB interface | For USB flash disk printing and scanning into USB flash disk.
7 | Control Panel | Indicate printer status to conduct set operation.
8 | NFC (Near Field Communication) label | Use mobile device to touch the tag to download or start the mobile application and for Wi-Fi Direct.
9 | Glass Platen | To put the original of tablet PC for scan.
10 | Output Tray | To prevent the printed paper from falling.
11 | Front Cover | To open the front cover to take out the laser toner cartridge.
12 | Multipurpose feed tray | For placing media for printing from multipurpose feed tray.
13 | Power switch | Turn the power on or off and press this button under Ready state to enter energy-saving mode. Press and hold this button for more than 2s to turn the printer power off.
14 | Automatic Feeder Tray | For placing mediums that are printed in auto feed tray.
15 | Paper guide of multipurpose feed tray | Slide paper deflector to adapt to paper width. | 16 | Front cover button of printer | For opening the front cover of printer. | 17 | Paper width deflector of auto feed tray | Slide paper width deflector to adapt to paper width. | 18 | Paper length deflector of auto feed tray | Slide paper length deflector to adapt to paper length. | 19 | Clip of extended tray of auto feed tray | For adjustment of length extension of the tray .

Rear View

1 | LINE interface (only for machine with the fax feature.) | Telephone line interface, used for connection of this product to the telephone circuit.
2 | EXT. interface (only for machine with the fax feature.) | Extension interface, used for connection with external extension telephone.
3 | USB Interface | For connecting product to computer with USB cable.
4 | Network Interface | For connecting product to network with network cable.
5 | Power Interface | For connecting product to power with power cord.
6 | Rear Cover | For paper release when it gets jammed.
7 | Duplex Printing Unit | For paper feed at duplex printing and paper release when paper gets jammed at duplex printing.
8 | Rear USB port | For extension of storage capacity of secure printing.

| Note: | • Printer appearance may differ because of various models and functions, so the schematic diagram is only for your reference.

1.4.Laser Toner Cartridge

Laser toner cartridge is composed of drum component and toner cartridge.

Service life of drum component

Type | Average Print Volume
Longevity of drum component | About 12000 Pages A4/LTR-based page (1 page/job).

Service life of toner cartridge

Type | Average Print Volume
Standard-volume toner cartridge | About 1500 Pages(Based on ISO 19752 standard)
High-volume toner cartridge | About 3000 Pages(Based on ISO 19752 standard)
Toner cartridge of super large capacity | About 6000 Pages(Based on ISO 19752 standard)

| Note: | • The model is subject to increase without notice. • Consumables capacity may vary with different using types. • The Company does not recommend using consumables other than the original consumables provided, as any damages caused by non-original consumables are not covered by the scope of warranty. • Toner cartridge appearance may differ because of multiple volume and models, so the schematic diagram is only for your reference.

1.5.Control Panel

1.5.1.Control Panel

The layout of the printer control panel is shown below:

No. | Name | Functions
1 | Color touch screen | • Check printer status and message. • Set and operate printer.
2 | Return button | Return to the previous menu.
3 | Home button | Go to the home screen.
4 | Help button | • Access to Help system of control panel. • It describes how to use each screen and eliminate faults.
5 | Status icon | • View supplies information in ready state. • View printer error status information in error status.
6 | Wi-Fi icon | • View printer Wi-Fi information. • Icon is dimmed when Wi-Fi disconnects.
7 | Wired network status icon | • Check printer wired network information. • Icon is dimmed when wired network disconnects.

1.5.2.Home screen

Use home screen buttons and icons to initialize print, fax or scan. The layout is shown as below:

No. | Name | Functions
1 | Copy | Access to “Copy” menu and make a copy.
2 | Scan | Access to “Scan” menu and scan document.
3 | Fax | Access to “Fax” menu and send a fax.
4 | ID copy | Access to “ID copy” menu and make an ID card copy.
5 | Bill copy | Access to “Bill copy” menu and make a bill copy.
6 | Secure printing | Access to “Secure Print” menu to print with password.
7 | USB print | Access to USB storage job and make a job print.
8 | “Setting” button | Open menu setting interface.
9 | Status message bar | Display the current printer status.

1.5.3.Touch screen button

Layout of touch screen buttons of printer control panel is shown as below:

No. | Name | Functions
1 | Radio button | Select or delete an item.
2 | Up arrow | Scroll up.
3 | Down arrow | Scroll down.
4 | Acceptance button | Save setting.
5 | Cancel button | Cancel selection.

1.5.4. Function of power indicator

No. | Status displayed by power indicator | Status | Status Description
1 |  | Die out | Shutdown status
2 |  | Always on | Booting and ready states
3 |  | Blink | Sleep mode