Language:
Welcome to TESORO World
Congratulations on purchasing your very own TESORO SHRIKE™ Laser Gaming Mouse - a gaming mouse engineered to suit the needs of every gamers. Featuring powerful marco editor function enable users to record the mouse and keyboard actions. It is the mouse of choice for optimizing the gaming experience.
Gaming-grade Laser sensor with 5-level resolution adjustment 800 / 1800 / 4000 / 6400 / 8200 DPI
Ergonomic design with tuning weight-in system
8 macro keys with 5 setting modes
Unique instant lower-DPI function to increase the cursor accuracy
Powerful Script Editor function let users record the mouse and keyboard actions
Polling rate adjustable by software : 125 / 250 / 500 / 1000 Hz
Build-in 128 KB onboard memory, plug and play while switching to different PC
Optical distance technology to freeze the cursor when user lift the mouse
Up to 256 colors to create unique style in different setting
Gold-plated USB connector with braided cable for ensure low latency
Operating System |
The software supports the following operating systems:
| Windows XP
| Windows Vista
| Windows 7
| Windows 8
Registering your TESORO SHRIKE™
Visit www.tesorotec.com for online product registration:
One year limited manufacture warranty
Free online technical support
Instruction |
| Software Overview |
|  | Profile:Profile management |  |  | Apply: Save setting and continue
|  | Button Assignment: scroll menu bar to assign button function |  |  | Cancel: Cancel setting and go back to previous status
|  | Advanced Setting: DPI and Macro setting |  |  | OK: Save settings and exit
|  | Mouse Wheel Options: Scroll menu bar to assign function |  |  | Minimize
|  | Mapping: Five mappings for editing and loading profiles |  |  | About SHRIKE
|  | Reset: Reset to default |  |  | Close the window
Button Assignment Illustration | Mouse Wheel Setting Illustration
|  | Macro | Load configuration Macro up to the driven menu
|  | Single | Define how to activate function of any single key function configuration
|  | Launch | Define how to open any single program launch
|  | Mapping Switch | Define how to switch different mappings. (+ Scroll Up / + Scroll Down)
Macro Function Configuration 1
|  | Edit New Macro Name |  |  | Macro Status Options:
|  | Macro Record Options: |  |  | Select "save as", "cancel" or "OK".
|  | Select "Start Record" to begin recording; select "Stop Record" |  |  | SHRIKE's Macro keys editing window
|  | to finish recording. |  |  | -->area
|  | Setting time delay for specific key: |  |  | List of Macro:
|  | (1) Set selected time delay --> delay time to certain timing (25ms~12751ms) |  |  | Move to specific macro, right click mouse
|  | (2) Set all item delay time to 25ms |  |  | button to edit, rename, or delete.
|  | Setting Macro Repeat type: |  |  | Macro:
|  | (1) Repeat-times |  |  | Create new macro or load existing macro
|  | (2) Repeat while pressed |  |  |
|  | (3) Repeat until next key is pressed |  |  |
Macro Function Configuration 2
|  | Colors Setting: |  |  | Polling Rate Mapping:
|  | (1) Five colors Mapping files can be defined individually |  |  | Four levels polling rate selection: 125HZ, 250HZ, 500HZ and
|  | (2) Activate lighting effect or dimming effect |  |  | 1000HZ
|  | DPI Setting: |  |  | Liftoff Distance Setting:
|  | Set values of X and Y axises from level one to level five |  |  | Five levels liftoff distance setting
|  | Speed Setting: |  |  |
|  | Click on the logo to view current speed setting |  |  |
After you finish all keys' setting. ClickClick to save current profile and continue to set other profiles.
Wait and finish Macro Setting
After click , now you've completed the macro setting, enjoy and have fun ! |