[COMMON]	 	
PRODUCT_LANGUAGE=EN
COMPANY_NAME=Mercury
PROGRAM_FOLDER_NAME=Mercury
BASE_FOLDER_NAME=Program Files\Mercury
;	 	
USBHUB_NAME=Mercury P2760
SCANNER_NAME=Mercury P2760 SCAN
PRINTER_NAME=MP3100CDN_NET
DRV_MDL_NAME=MP3100CDN_NET
PORT_NAME=192.168.1.160
;	 	
VID_PID=VID_0EFD&PID_0045
USB_SERIAL=0000000000000000
PNP_LPT=Mercury_P27600FC9
PNP_USB=Mercury_P2760
PNP_CHECKSUM=0FC9
USB_PARENT_ID=6&26dc5742&0&0001
;	 	
BUTTON_OK=OK
BUTTON_CANCEL=Cancel
MSG_ERR_CAPTION=Error!!!
MSG_FILE_NOT_FOUND=The system cannot find the file specified.
MSG_DIR_NOT_FOUND=The system cannot find the path specified.
MSG_FILE_NOT_OPEN=The system cannot open the file.
MSG_SHARING_VIOLATION=The process cannot access the file because it is being used by another process.
MSG_FILE_SIZE_ZERO=The file size is 0 byte.
MSG_ACCESS_DENIED=Access is denied.
MSG_HANDLE_INVALID=The handle is invalid.
MSG_ERROR_CODE=Error code:
	 	
[WEBSITE]	 	
default=
current=
	 	
[SETMAN]	 	
CAPTION=Reference Guide Setup
PRODUCT_NAME=Mercury P2760 Reference Guide
UNINSTALL_NAME=Mercury P2760 Reference Guide
SHORTCUT_NAME=Mercury P2760 Reference Guide
ICON_NAME=PRIX903.ICO
PRODUCT_KEY_FILE=M1XXE0HL.HLP
UNINSTALL_KEY_FILE=M1SETMAN.EXE
;	 	
MSG_UNINST_CONFIRM=Are you sure you want to completely remove the Reference Guide and all of its components?
BUTTON_DELETE_YES=OK
BUTTON_DELETE_NO=Cancel
	 	
[SETSTM]	 	
CAPTION=Status Monitor Setup
PRODUCT_NAME=Mercury P2760 Status Monitor
UNINSTALL_NAME=Mercury P2760 Status Monitor
SHORTCUT_NAME=Mercury P2760 Status Monitor
ICON_NAME=PRIX902.ICO
PRODUCT_KEY_FILE=M1XXE0SM.EXE
UNINSTALL_KEY_FILE=M1SETSTM.EXE
;	 	
MSG_UNINST_CONFIRM=Are you sure you want to completely remove the Status Monitor and all of its components?
BUTTON_DELETE_YES=OK
BUTTON_DELETE_NO=Cancel
;	 	
TITLE_STM=Mercury Monitor 3
;	 	
InTitle=Mercury Printer Utility Setup
InEND=Mercury Status Monitor Setup is complete.
;	 	
UnTitle=Mercury Printer Utility Uninstall
UnEND=Uninstall complete.
;	 	
URLSET1=Choose the country or region in which you use this printer.
URLSET2=By choosing a country or a region, you will activate the online consumables order function.
URLSET3=Consumables Web Site URL:
;	 	
WEB1=Korea
WEB2=(No Setting)
URL1=http://www.iprix.co.kr/
URL2=
;	 	
msgChange=You have changed the URL. Do you want to keep the new setting?
;	 	
	 	
[SETDRV]
IPHONENUMBER=88165526
TELEPHONENUMBER=1234 	
CAPTION=Printer Driver Setup
GROUP_NAME=Mercury P2760
PRODUCT_NAME=Mercury P2760 Printer Driver
UNINSTALL_NAME=Mercury P2760 Printer Driver
SHORTCUT_NAME=Mercury P2760 Printer Driver
ICON_NAME=PRIX901.ICO
PRODUCT_KEY_FILE=M1XXE0DR.DLL
UNINSTALL_KEY_FILE=M1SETDRV.EXE
;	 	
MSG_UNINST_CONFIRM=Are you sure you want to completely remove the Printer Driver and all of its components?
BUTTON_DELETE_YES=OK
BUTTON_DELETE_NO=Cancel
;	 	
; progress dialog	 	
;	 	
CAPTION_INSTALL=Copying files...
CAPTION_UNINSTALL=Deleting files...
;	 	
INF_OEMx=oem0.inf
INF_SEC_LPT=OEM_LPT
INF_SEC_USB=OEM_USB
INF_SEC_MFG=OEM_MFG
INF_MFG=Mercury
INF_DATE=01-02-2006
LANG_MONITOR=P2760 Language Monitor
PORT_MONITOR=USBMON
DATA_TYPE=RAW
SHARE_NAME=P2760
;	 	
PATH_LANGUAGE=English
PATH_WIN9X=WIN9X
PATH_WINXP_2K=WINXP_2K
;	 	
PAPER_USERDEFINED=User Defined Size
	 	
[MESSAGE]	 	
MSG_REG_UPDATE=<<< Changing Registry ... >>>
;	 	
MSG_FILE_NOT_FOUND=File not found
;	 	
MSG_EXECUTE_ERROR=Execute Error
MSG_WIN_9X=This program requires Windows 98/98SE/ME.
MSG_WIN_NT=This program requires Windows NT 4.0.
MSG_WIN_XP=This program requires Windows 2000/XP/2003.
;	 	
MSG_END_INST=Mercury P2760 software was installed.
MSG_END_UNINST=Mercury P2760 software was uninstalled.
	 	
[FILENAME]	 	
;	 	
; Driver (XP)	 	
;	 	
FN_DRV2K_DLL=M1XXE0DR.DLL
FN_DRV2K_GPD=M1XXE0DR.GPD
FN_DRV2KUI_DLL=M1XXE0UI.DLL
FN_DRV2KHT_DLL=M1XXE0HT.DLL
FN_DPINST_EXE=DPINST.EXE
;	 	
; Uni-Driver (XP)	 	
;	 	
;FN_STDNAMES_GPD=STDNAMES.GPD
;FN_UNIDRV_DLL=UNIDRV.DLL
;FN_UNIDRV_HLP=UNIDRV.HLP
;FN_UNIDRVUI_DLL=UNIDRVUI.DLL
;FN_UNIRES_DLL=UNIRES.DLL
;	 	
; Driver (9x)	 	
;	 	
FN_DRV9X_DRV=M1XXE1DR.DRV
FN_DRV9X_DLL=M1XXE2DR.DLL
;	 	
; Driver (ALL)	 	
;	 	
FN_STMRSP_DAT=M1XXE0SM.DAT
FN_DRV_HLP=M1XXE0HL.HLP
FN_DRVIMAGE_DLL=M1XXE0IP.DLL
FN_DRVPRINT_DLL=M1XXE0PS.DLL
FN_MDLIMAGE_BMP=M1XXE1PS.BMP
FN_LEDLIGHT_BMP=M1XXE2PS.BMP
FN_LANGMON_DLL=M1XXE0LM.DLL
FN_LANGSEND_DLL=M1XXE0SP.DLL
FN_JBIG_EXE=M1XXE0JB.EXE
FN_MSGBOX_DLL=M1XXE0MB.DLL
FN_RUNCHECK_EXE=M1XXE0RC.EXE
FN_DRVRES_DAT=M1XXEDRV.DAT
;	 	
; Status Monitor	 	
;	 	
FN_SETSTM_EXE=M1SETSTM.EXE
FN_SETSTM_DAT=M1SETSTM.DAT
FN_STM_EXE=M1XXE0SM.EXE
;	 	
; CD Run	 	
;	 	
FN_AUTORUN_INF=AUTORUN.INF
FN_CDROM_ICO=CDROMLP.ICO
FN_CDSETUP_EXE=CDSETUP.EXE
;	 	
; Setup (Install, Uninstall)	 	
;	 	
FN_SETDRV_EXE=M1SETDRV.EXE
FN_SETDRV_DAT=M1SETSET.DAT
FN_SETUNE_EXE=M1SETUNE.EXE
FN_SETUNE_EXE=M1XXE0DF.EXE
FN_SETLINK_EXE=M1SETLNK.EXE
;	 	
; Setup (Add Printer)	 	
;	 	
FN_DRV9X_INF=M1XXE0ME.INF
FN_DRV2K_INF=M1XXE0XP.INF
FN_DRV2K_CAT=M1XXE0XP.CAT
FN_DRV2K_INI=M1XXE0DR.INI
FN_SETVENDOR_DLL=M1SETVND.DLL
;	 	
; Setup (PnP)	 	
;	 	
FN_USBHUB_INF=M1XUSBHU.INF
FN_USBHUB_SYS=USBHUB.SYS
FN_USBPRINT_INF=M1XUSBPR.INF
FN_USBPRINT_SYS=USBPRINT.SYS
FN_USBMON_DLL=USBMON.DLL
FN_USBSCAN_INF=M1XUSBSC.INF
FN_USBSCAN_CAT=M1XUSBSC.CAT
FN_USBSCAN_SYS=USBSCAN.SYS
;	 	
; Manual	 	
;	 	
FN_SETMAN_EXE=M1SETMAN.EXE
FN_SETMAN_DAT=M1SETMAN.DAT
	 	
[FW_MSG]	 	
V_INTERNET=打印机连接外网
V_INTERNETi1=打印机已连接外网！为确保打印数据安全，请使用内部网络
V_READY=准备就绪
V_READYi1=可以印刷的待机状态
V_WAIT=请等待
V_WAITi1=记录引擎初始化状态
V_CANCEL=取消打印
V_CANCELi1=PC打印任务取消状态
V_PRINTING=正在打印
V_PRINTINGi1=正在打印状态
V_CONSUM_N_END=硒鼓即将用尽
V_CONSUM_N_ENDi1=硒鼓寿命即将耗尽的状态
V_CONSUM_N_ENDi2=硒鼓组件接近零件寿命。当打印超过规定比例的部件寿命时，发生此错误。
V_N_END_TONER=墨粉不足
;V_N_END_TONER=Toner Kit near end of service life
V_N_END_TONERi1=碳粉较少的状态
V_N_END_TONERi2=墨粉剩余可以打印的数量不多了、警告（可以进行打印）
;V_N_END_TONERi1=Prepare a new Toner Kit.
V_N_END_C_TONER=青色墨粉不足
;V_N_END_C_TONER=Blue Toner Kit near end of service life
V_N_END_C_TONERi1=青色墨盒墨粉即将用完，请更换墨盒
;V_N_END_C_TONERi1=Prepare a new Toner Kit.
V_N_END_M_TONER=品红色墨粉不足
;V_N_END_M_TONER=Red Toner Kit near end of service life
V_N_END_M_TONERi1=品红色墨盒墨粉即将用完，请更换墨盒
;V_N_END_M_TONERi1=Prepare a new Toner Kit.
V_N_END_Y_TONER=黄色墨粉不足
;V_N_END_Y_TONER=Toner Kit near end of service life
V_N_END_Y_TONERi1=黄色墨盒墨粉即将用完，请更换墨盒
;V_N_END_Y_TONERi1=Prepare a new Toner Kit.
V_N_END_BELT=转印带将用尽
;V_N_END_BELT=Process Cartridge Unit near end of service life
V_N_END_BELTi1=转印带组件接近零件寿命，请立刻更换转印带组件
;V_N_END_BELTi1=Prepare a new Process Cartridge Unit.
V_N_END_OPC=更换硒鼓
;V_N_END_OPC=Process Cartridge Unit near end of service life
V_N_END_OPCi1=需要更换硒鼓的状态
V_N_END_OPCi2=到了该更换硒鼓的时候了。
;V_N_END_OPCi1=Prepare a new Process Cartridge Unit.
V_CHANGE_BELT=更换转印带
V_CHANGE_BELTil=转印带组件寿命已经用尽，请立刻更换转印带组件
V_CHANGE_FUSER=更换定影单元
V_CHANGE_FUSERil=需要更换定影单元的状态
V_CHANGE_FUSERi2=定影器的印刷寿命已经到了
V_N_PAPER_T1=纸盒1无纸
V_N_PAPER_T1i1=纸盒1里没有纸的状态
V_N_PAPER_T1i2=
V_N_PAPER_T2=纸盒2无纸
V_N_PAPER_T2i1=纸盒2里没有纸的状态
V_N_PAPER_T2i2=
V_N_PAPER_T3=纸盒3无纸
V_N_PAPER_T3i1=纸盒3里没有纸的状态
V_N_PAPER_T3i2=
V_N_PAPER_T4=纸盒4无纸
V_N_PAPER_T4i1=纸盒4里没有纸的状态
V_N_PAPER_T4i2=
V_N_TRAY_T1=无纸盒1
V_N_TRAY_T1i1=纸盒1被抽出的状态
V_N_TRAY_T1i2=纸盒1被打开并且没有其他进纸方法的情况下发生的故障
V_N_TRAY_T2=无纸盒2
V_N_TRAY_T2i1=纸盒2被抽出的状态
V_N_TRAY_T2i2=纸盒2被打开并且没有其他进纸方法的情况下发生的故障
V_N_TRAY_T3=无纸盒3
V_N_TRAY_T3i1=纸盒3被抽出的状态
V_N_TRAY_T3i2=纸盒3被打开并且没有其他进纸方法的情况下发生的故障
V_N_TRAY_T4=无纸盒4
V_N_TRAY_T4i1=纸盒4被抽出的状态
V_N_TRAY_T4i2=纸盒4被打开并且没有其他进纸方法的情况下发生的故障
V_NO_MEMORY=内存已满
;V_NO_MEMORY=Insufficient memory
V_NO_MEMORYi1=内存已满的状态
;V_NO_MEMORYi1=Click Continue to resume printing.
V_NO_MEMORYi2=在解压PC-Print的Data数据时内存不足的状態
;V_NO_MEMORYi2=Click Cancel Printing to cancel the print job.
V_NO_MEMORYi3=
;V_NO_MEMORYi3=This error might be avoided by selecting Avoid Insufficient Memory Error in Extended Settings on the printer driver's Optional Settings menu.
V_SLEEP=休眠
V_SLEEPi1=打印加热装置关闭的状态（睡眠模式）
V_COVER_OPEN=盖子未合上
;V_COVER_OPEN=Top cover open
V_COVER_OPENi1=前盖（存放碳粉的地方的盖子）被打开的状态
V_COVER_OPENi2=前盖被打开了
;V_COVER_OPENi1=Close the cover.
V_NO_WASTE_TONER=无废粉仓
V_NO_WASTE_TONERi1=没有安装废粉仓，请安装废粉仓
V_BACK_COVER_OPEN=不能双面打印
;V_BACK_COVER_OPEN=Top cover open
V_BACK_COVER_OPENi1=后盖（打印机背面的保护盖）被打开的状态
V_BACK_COVER_OPENi2=试图开始双面打印时，由于后盖打开，不能双面打印时产生的Error。Error发生时，机器会等待后盖关闭。
;V_BACK_COVER_OPENi1=Close the cover.
V_REPLACE__WT_BOX=更换废粉仓
V_REPLACE__WT_BOXi1=废粉仓已满，请立即更换
V_DRUM_STOP=硒鼓停止
V_DRUM_STOPi1=硒鼓故障，请立即更换
V_REPLACE_TONER=更换墨粉盒
V_REPLACE_TONERi1=执行打印动作时，没有碳粉的状态下
V_REPLACE_TONERi2=没有碳粉的状态
V_REPLACE_C_TONER=更换青色墨粉
V_REPLACE_C_TONERi1=接收数据时青色墨粉用尽
V_REPLACE_M_TONER=更换品红色墨粉
V_REPLACE_M_TONERi1=接收数据时品红色墨粉用尽
V_REPLACE_Y_TONER=更换黄色墨粉
V_REPLACE_Y_TONERi1=接收数据时黄色墨粉用尽
V_NO_CARTRIGE=无硒鼓单元
;V_NO_CARTRIGE=Toner Kit not installed
V_NO_CARTRIGEi1=打印机必要零件“硒鼓”没有安装的状态
V_NO_CARTRIGEi2=不存在硒鼓单元。在未安装硒鼓组件的状态下接通电源的情况。
;V_NO_CARTRIGEi1=Open the top cover, then install the Toner Kit.
V_TONER_ID_ERR=无墨粉
;V_TONER_ID_ERR=Incorrect Toner Kit
V_TONER_ID_ERRi1=打印机必要零件“碳粉盒”没有安装的状态
;V_TONER_ID_ERRi1=Open the top cover, then remove and reinstall the Toner Kit.
V_TONER_ID_ERRi2=没有安装碳粉盒
;V_TONER_ID_ERRi2=If this error occurs again, replace the Toner Kit.
V_C_TONER_ID_ERR=未安装青色墨粉单元
;V_C_TONER_ID_ERR=Incorrect Toner Kit
V_C_TONER_ID_ERRi1=请打开盖板并安装青色墨粉单元
;V_C_TONER_ID_ERRi1=Open the top cover, then remove and reinstall the Toner Kit.
V_C_TONER_ID_ERRi2= 
;V_C_TONER_ID_ERRi2=If this error occurs again, replace the Toner Kit.
V_M_TONER_ID_ERR=未安装品红色墨粉单元
;V_M_TONER_ID_ERR=Incorrect Toner Kit
V_M_TONER_ID_ERRi1=请打开盖板并安装品红色墨粉单元
;V_M_TONER_ID_ERRi1=Open the top cover, then remove and reinstall the Toner Kit.
V_M_TONER_ID_ERRi2= 
;V_M_TONER_ID_ERRi2=If this error occurs again, replace the Toner Kit.
V_Y_TONER_ID_ERR=未安装黄色墨粉单元
;V_Y_TONER_ID_ERR=Incorrect Toner Kit
V_Y_TONER_ID_ERRi1=请打开盖板并安装黄色墨粉单元
;V_Y_TONER_ID_ERRi1=Open the top cover, then remove and reinstall the Toner Kit.
V_Y_TONER_ID_ERRi2= 
;V_Y_TONER_ID_ERRi2=If this error occurs again, replace the Toner Kit.
V_BELT_ID_ERR=无转印带单元
V_BELT_ID_ERRi1=请打开盖板并安装转印带单元
V_N_PAPER_MP=多功能进纸板无纸
V_N_PAPER_MPi1=多功能进纸板上没有记录用纸的状态
V_N_PAPER_MPi2=印刷的时候，设定 纸盒用途 为仅多功能进纸板时，检测到多功能进纸板里没有纸的故障
V_NO_PAPER_T1=纸盒1无纸
V_NO_PAPER_T1i1=纸盒1中没有记录用纸的状态
V_NO_PAPER_T1i2=印刷的时候，设定 纸盒用途 为仅纸盒1时，检测到纸盒1里没有纸的故障
V_NO_PAPER_T2=纸盒2无纸
V_NO_PAPER_T2i1=纸盒2中没有记录用纸的状态
V_NO_PAPER_T2i2=印刷的时候，设定 纸盒用途 为仅纸盒2时，检测到纸盒2里没有纸的故障
V_NO_PAPER_T3=纸盒3无纸
V_NO_PAPER_T3i1=纸盒3中没有记录用纸的状态
V_NO_PAPER_T3i2=印刷的时候，设定 纸盒用途 为仅纸盒3时，检测到纸盒3里没有纸的故障
V_NO_PAPER_T4=纸盒4无纸
V_NO_PAPER_T4i1=纸盒4中没有记录用纸的状态
V_NO_PAPER_T4i2=印刷的时候，设定 纸盒用途 为仅纸盒4时，检测到纸盒4里没有纸的故障
V_N_PAPER=无纸
V_N_PAPERi1=当 纸盒用途 设定为 自动选择时，所有进纸槽都没纸的状态
V_N_PAPERi2=印刷的时候存在多个可以使用的纸盒，（有多个纸盒且纸盒用途 设定为 自动选择）但是检测到这些纸盒中都没有纸
V_JAM_OUTPUT=后部卡纸
;V_JAM_OUTPUT=Paper jam - output
V_JAM_OUTPUTi1=打印机卡纸状态
V_JAM_OUTPUTi2=在排纸槽附近发生的卡纸。排纸槽发生用纸堵塞的情况。
;V_JAM_OUTPUTi1=Open the top and output covers, then remove any jammed paper.
V_FEED_JAM=多功能进纸板卡纸
;V_FEED_JAM=Unable to feed paper
V_FEED_JAMi1=打印机卡纸状态
;V_FEED_JAMi1=Reload the paper.
V_FEED_JAMi2=多功能进纸板出现纸张堵塞的情况
;V_FEED_JAMi2=Click Continue or open and close the top cover to resume printing.
V_JAM_TRAY1=纸盒1卡纸
V_JAM_TRAY1i1=打印机卡纸状态
V_JAM_TRAY1i2=纸盒1出现纸张堵塞的情况
V_JAM_INSIDE=内部卡纸
V_JAM_INSIDEi1=打印机卡纸状态
V_JAM_INSIDEi2=打印机内出现纸张堵塞的情况
V_JAM_2SIDED=双面卡纸
V_JAM_2SIDEDi1=打印机卡纸状态
V_JAM_2SIDEDi2=双面进纸槽出现纸张堵塞的情况
V_CALIBRATION=校准失败
V_CALIBRATIONi1=颜色校准过程中故障
V_SELF_DIAGNOSTIC=自我诊断
V_SELF_DIAGNOSTICi1=定影装置异常的状态（警告）
V_SELF_DIAGNOSTICi2=定影单元相关的故障，用户需要重启一下机器
V_PRINT_DATA_FULL=打印数据已满
V_PRINT_DATA_FULLi1=Secure Print数据已经满了的状态
V_PRINT_DATA_FULLi2=为了保存Secure Print的数据，超过了被预先Secure Print用保证的内存大小的时候发生的Error
V_TEMP_ERROR_002=正在冷却
V_TEMP_ERROR_002i1=打印机正在冷却的状态
V_TEMP_ERROR_002i2=Cooling Down（机内冷却中）。装置内的温度上升，无法打印的状态。打印机内温度检测到超过规定温度的情况发生。(直到温度恢复到规定值以下之前都不可打印)
V_DRUM=硒鼓错误
V_DRUMi1=请移动微调器清理硒鼓静电的状态
V_DRUMi2=硒鼓上可能有静电，所以出现了请移动带电微调器（Drum上可以滑动的小型零件）的故障
V_LSU_COVER_OPEN=盖子未合上
V_LSU_COVER_OPENi1=定影单元盖被打印开的状态
V_LSU_COVER_OPENi2=定影单元盖被打开的错误，打开后盖，打开其中的定影单元盖就会发生该错误
V_SIZE_ERR_DX=双面纸张尺寸错误
V_SIZE_ERR_DXi1=双面打印的强制排出状态
V_SIZE_ERR_DXi2=在双面打印时，供纸的记录纸过短或过长，不能双面运送的情况发生。
V_MACHINE_ERR=无法打印
V_MACHINE_ERRi1=机器故障状态
V_MACHINE_ERRi2=机器故障状态
V_INCOR_MEDIA_WR=介质不匹配
V_INCOR_MEDIA_WRi1=纸张类型与设定不符合的状态
V_INCOR_MEDIA_WRi2=设定好的用纸类型和打印数据的用纸类型不一致时发生的故障
V_INCOR_PAPER_WR=尺寸匹配错误
;V_INCOR_PAPER_WR=Printing on incorrect paper size
V_INCOR_PAPER_WRi1=纸张大小与设定不符合的状态
;V_INCOR_PAPER_WRi1=Select the correct size paper.
V_INCOR_PAPER_WRi2=设定好的用纸大小和打印数据的用纸大小不一致时发生的故障
;V_INCOR_PAPER_WRi2=Click Close to close this message.
V_CARTRIDGE_ERR=墨粉盒错误
V_CARTRIDGE_ERRi1=新的墨粉故障的状态
V_CARTRIDGE_ERRi2=检测到新墨粉不正确时出现的故障
V_TRAY2_ERR=纸盒2错误
V_TRAY2_ERRi1=纸盒2故障错误
V_TRAY2_ERRi2=建议更换纸盒2
V_TONER_ERR=墨粉盒错误
V_TONER_ERRi1=检测出墨粉盒故障
V_TONER_ERRi2=建议更换墨粉盒
V_REGISTRATION=配准失败
V_REGISTRATIONi1=颜色校准故障
V_SHORT_PAPER=短纸张错误
V_SHORT_PAPERi1=所选纸张太小，印刷出错
V_SHORT_PAPERi2=建议选择合适纸张大小
V_CONDENSATION=凝露
V_CONDENSATIONi1=发生结露故障
V_CONDENSATIONi2=建议清理机器
V_TRAY3_ERR=纸盒3错误
V_TRAY3_ERRi1=纸盒3故障错误
V_TRAY3_ERRi2=建议更换纸盒3
V_TOO_MANY_TRAYS=纸盒过多
V_TOO_MANY_TRAYSi1=存在太多纸盒的状态
V_TOO_MANY_TRAYSi2=检测到比可连接数目更多的纸盒被连接时发生的错误
V_UNABLE_ZC=无法打印ZC
V_UNABLE_ZCi1=电压不稳定状态
V_UNABLE_ZCi2=检测到输入的电源电压波形异常时发生的故障Zero Cross Error(重启后可能解决故障)。
V_SELF_DIAGNOSTIC2=自我诊断
V_SELF_DIAGNOSTIC2i1=定影单元出现异常超过15分钟的状态
V_SELF_DIAGNOSTIC2i2=中央热敏电阻检测到了已超过后，关闭电源15分钟后开启机器、打印引擎会再次启动。
V_PLACE_LASER=更换激光单元
V_PLACE_LASERi1=更换部件寿命到达的警告状态
V_PLACE_LASERi2=更换激光单元的时候到了
V_WT_BOX_END=废粉仓寿命用尽
V_WT_BOX_ENDi1=打印机废粉仓寿命达到更换状态
V_WT_BOX_ENDi2=打印机废粉仓寿命达到更换状态，请更换废粉仓
V_PLACE_KIT1=更换纸盒1进纸器
V_PLACE_KIT1i1=更换部件寿命到达的警告状态
V_PLACE_KIT1i2=进纸器1的印刷寿命到了
V_PLACE_KIT2=更换纸盒2进纸器
V_PLACE_KIT2i1=更换部件寿命到达的警告状态
V_PLACE_KIT2i2=进纸器2的印刷寿命到了
V_PLACE_KIT3=更换纸盒3进纸器
V_PLACE_KIT3i1=更换部件寿命到达的警告状态
V_PLACE_KIT3i2=进纸器3的印刷寿命到了
V_PLACE_KIT4=更换纸盒4进纸器
V_PLACE_KIT4i1=更换部件寿命到达的警告状态
V_PLACE_KIT4i2=进纸器4的印刷寿命到了
V_PLACE_KITMP=更换MP纸盒进纸器
V_PLACE_KITMPi1=更换部件寿命到达的警告状态
V_PLACE_KITMPi2=多功能进纸器的印刷寿命到了
V_PAPER_T1_LOW=纸盒1纸张少
V_PAPER_T1_LOWi1=打印机纸盒1剩余纸张较少
V_PAPER_T1_LOWi2=打印机纸盒1剩余纸张较少，请向纸盒1中添加纸张
V_PAPER_T2_LOW=纸盒2纸张不足
V_PAPER_T2_LOWi1=纸盒2纸张残量较少的状态（警告）
V_PAPER_T2_LOWi2=
V_PAPER_T3_LOW=纸盒3纸张不足
V_PAPER_T3_LOWi1=纸盒3纸张残量较少的状态（警告）
V_PAPER_T3_LOWi2=
V_PAPER_T4_LOW=纸盒4纸张不足
V_PAPER_T4_LOWi1=纸盒4纸张残量较少的状态（警告）
V_PAPER_T4_LOWi2=
V_N_PAPER_FEED1=纸盒1无进纸
V_N_PAPER_FEED1i1=打印机卡纸状态
V_N_PAPER_FEED1i2=纸盒1出现了吸纸失败的故障
V_JAM_TRAY2=纸盒2卡纸
V_JAM_TRAY2i1=打印机卡纸状态
V_JAM_TRAY2i2=纸盒2出现了卡纸的故障
V_N_PAPER_FEED2=纸盒2无进纸
V_N_PAPER_FEED2i1=打印机卡纸状态
V_N_PAPER_FEED2i2=纸盒2出现了吸纸失败的故障
V_JAM_TRAY3=纸盒3卡纸
V_JAM_TRAY3i1=纸盒3出现了卡纸的故障
V_JAM_TRAY3i2=纸盒3出现了卡纸的故障
V_N_PAPER_FEED3=纸盒3无进纸
V_N_PAPER_FEED3i1=打印机卡纸状态
V_N_PAPER_FEED3i2=纸盒3出现了吸纸失败的故障
V_JAM_TRAY4=纸盒4卡纸
V_JAM_TRAY4i1=纸盒4出现了卡纸的故障
V_JAM_TRAY4i2=纸盒4出现了卡纸的故障
V_N_PAPER_FEED4=纸盒4无进纸
V_N_PAPER_FEED4i1=打印机卡纸状态
V_N_PAPER_FEED4i2=纸盒4出现了吸纸失败的故障
V_DOC_JAM=原稿卡纸
V_DOC_JAMi1=原稿卡纸故障状态
V_DOC_JAMi2=ADF读取原稿的时候出现卡纸的故障
V_WRONG_SIZE=纸张尺寸错误
V_WRONG_SIZEi1=纸张大小错误的状态
V_WRONG_SIZEi2=复印的时候，优先级最高的纸盒里没纸了，使用次级优先级的纸盒，出现了纸张大小不符合的错误
V_ADF_OPEN=盖子未合上
V_ADF_OPENi1=ADF盖子未合上的状态
V_ADF_OPENi2=ADF 盖子被打开
V_UNABLE_AF=无法扫描
V_UNABLE_AFi1=扫面元件的起始位置错误
V_UNABLE_AFi2=
V_UNABLE_A9=无法扫描
V_UNABLE_A9i1=扫描特殊错误
V_UNABLE_A9i2=
V_UNABLE=无法扫描
V_UNABLEi1=ADF双面读取长尺原稿错误
V_UNABLEi2=原稿长度太长，不能ADF双面输送。

V_POWER_SAVE=省电模式
V_POWER_SAVEi1=打印中会自动退出此模式
;V_POWER_SAVEi1=This mode is canceled automatically when printing is performed.
V_PRT_OTHER_PORT=来自其他端口的打印数据
;V_PRT_OTHER_PORT=Printing data from another port
V_PRT_OTHER_PORTi1=请等待...
;V_PRT_OTHER_PORTi1=Please wait.
V_NOT_ALL_PRINT=未完成所有打印
;V_NOT_ALL_PRINT=Not all pages printed
V_NOT_ALL_PRINTi1=
;V_NOT_ALL_PRINTi1=This error might be avoided by selecting Avoid Insufficient Memory Error in Extended Settings on the printer driver's Optional Settings menu.
;V_CONSUM_N_ENDi1=Prepare the following consumables:
V_CONSUM_N_ENDi2=硒鼓
;V_CONSUM_N_ENDi2=Process Cartridge Unit
V_CONSUM_N_ENDi3=墨盒
;V_CONSUM_N_ENDi3=Toner Kit
V_N_GENUINE_INST=使用了伪劣的硒鼓
;V_N_GENUINE_INST=Non-genuine Toner Kit installed
V_N_GENUINE_INSTi1=使用伪劣硒鼓会影响打印质量，推荐使用光电原装硒鼓
;V_N_GENUINE_INSTi1=Using a non-genuine Toner Kit may affect print quality. Installing a genuine Mercury Toner Kit is recommended.
V_CONSUM_WARNING=耗材报警
;V_CONSUM_WARNING=Consumables warning
V_CONSUM_WARNINGi1=准备下列耗材:
;V_CONSUM_WARNINGi1=Prepare the following consumables:
V_CONSUM_WARNINGi2=硒鼓
;V_CONSUM_WARNINGi2=Process Cartridge Unit
V_CONSUM_WARNINGi3=墨盒
;V_CONSUM_WARNINGi3=Toner Kit
V_CONSUM_WARNINGi4=使用伪劣硒鼓会影响打印质量，推荐使用光电原装硒鼓
;V_CONSUM_WARNINGi4=Using a non-genuine Toner Kit may affect print quality. Installing a genuine Mercury Toner Kit is recommended.
V_N_END_NONTONER=墨盒即将用尽
;V_N_END_NONTONER=Toner Kit near end of service life
V_N_END_NONTONERi1=准备一个新硒鼓
;V_N_END_NONTONERi1=Prepare a new Process Cartridge Unit.
V_N_END_NONTONERi2=使用伪劣墨盒会影响打印质量，推荐使用光电原装硒鼓
;V_N_END_NONTONERi2=Using a non-genuine Toner Kit may affect print quality. Installing a genuine Mercury Toner Kit is recommended.
V_TOO_MUCH_DATA=页中包含数据过多
;V_TOO_MUCH_DATA=Page contains too much data to process
V_TOO_MUCH_DATAi1=请单击“继续打印”按钮，继续打印
;V_TOO_MUCH_DATAi1=Click Re-print to print again.
V_TOO_MUCH_DATAi2=请单击“取消打印”按钮，取消打印任务
;V_TOO_MUCH_DATAi2=Click Cancel Printing to cancel the print job.
V_TOO_MUCH_DATAi3=
;V_TOO_MUCH_DATAi3=This error might be avoided by selecting Avoid Page Error in Extended Settings on the printer driver's Optional Settings menu.
V_SIZE_TYPE_ERR=纸张尺寸不正确
;V_SIZE_TYPE_ERR=Incorrect paper size
V_SIZE_TYPE_ERRi1=在打印机驱动中选择的纸张大小与装载的纸张大小不匹配
;V_SIZE_TYPE_ERRi1=The paper size selected in the printer driver does not match the paper size that is loaded.
V_SIZE_TYPE_ERRi2=请单击“继续”按钮，继续打印
;V_SIZE_TYPE_ERRi2=Click Continue to resume printing.
V_SIZE_TYPE_ERRi3=请单击“取消打印”按钮，取消打印任务
;V_SIZE_TYPE_ERRi3=Click Cancel Printing to cancel the print job.
V_PAPER_MISMATCH=纸张尺寸不正确
;V_PAPER_MISMATCH=Incorrect paper size
V_PAPER_MISMATCHi1=在打印机驱动中选择的纸张大小与装载的纸张大小不匹配
;V_PAPER_MISMATCHi1=The paper size selected in the printer driver does not match the paper size that is loaded.
V_PAPER_MISMATCHi2=请单击“确定”按钮，继续打印
;V_PAPER_MISMATCHi2=Click OK to resume printing.
V_PAPER_MISMATCHi3=请单击“取消”按钮，取消打印任务
;V_PAPER_MISMATCHi3=Click Cancel to cancel the print job.
V_JAM_PRINT=打印机卡纸
;V_JAM_PRINT=Paper jam - printer
V_JAM_PRINTi1=打开顶盖移除被卡纸张
;V_JAM_PRINTi1=Open the top and output covers, then remove any jammed paper.
V_FEED_JAM_PAP=搓纸失败
;V_FEED_JAM_PAP=Unable to feed paper
V_FEED_JAM_PAPi1=重新装纸
;V_FEED_JAM_PAPi1=Reload the paper.
V_FEED_JAM_PAPi2=清除错误后请开合顶盖，继续打印
;V_FEED_JAM_PAPi2=Open and close the top cover to resume printing.
V_OUTPUT_C_OPEN=输出盖子打开
;V_OUTPUT_C_OPEN=Output cover open
V_OUTPUT_C_OPENi1=关闭外盖
;V_OUTPUT_C_OPENi1=Close the cover.
V_TONER_OUT_ERR=墨粉溢出
;V_TONER_OUT_ERR=Toner out
V_TONER_OUT_ERRi1=打开顶盖，更换墨盒
;V_TONER_OUT_ERRi1=Open the top cover, then replace the Toner Kit.
V_TONER_OUT_ERRi2=使用伪劣硒鼓会影响打印质量，推荐使用光电原装硒鼓
;V_TONER_OUT_ERRi2=Using a non-genuine Toner Kit may affect print quality. Installing a genuine Mercury Toner Kit is recommended.
V_TONER_RW_ERR=墨盒故障
;V_TONER_RW_ERR=Trouble with Toner Kit
V_TONER_RW_ERRi1=打开顶盖，重新安装或更换墨盒
;V_TONER_RW_ERRi1=Open the top cover, then reinstall or replace the Toner Kit.
V_NGENUINE_TONER=伪劣墨盒
;V_NGENUINE_TONER=Non-genuine toner
V_NGENUINE_TONERi1=使用伪劣硒鼓会影响打印质量，推荐使用光电原装硒鼓
;V_NGENUINE_TONERi1=Using a non-genuine Toner Kit may affect print quality. Installing a genuine Mercury Toner Kit is recommended.
V_GENERAL_ERROR=普通错误
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
V_TEMP_ERROR_001=加热异常
V_TEMP_ERROR_001i1=关闭打印机，等待几分钟，再开启打印机
V_TEMP_ERROR_001i2=如果此错误再次出现，请联系当地经销商

V_BLSU_ERROR_001=红色LSU错误001
V_BLSU_ERROR_001i1=未收到线同步信号。关闭打印机，等待几分钟，再开启打印机
V_BLSU_ERROR_001i2=如果此错误再次出现，请联系当地经销商

V_BLSU_ERROR_002=红色LSU错误002
V_BLSU_ERROR_002i1=未收到ready信号。关闭打印机，等待几分钟，再开启打印机
V_BLSU_ERROR_002i2=如果此错误再次出现，请联系当地经销商

V_LSU_ERROR_001=黑色LSU错误001
V_LSU_ERROR_001i1=未收到线同步信号。关闭打印机，等待几分钟，再开启打印机
V_LSU_ERROR_001i2=如果此错误再次出现，请联系当地经销商

V_LSU_ERROR_002=黑色LSU错误002
V_LSU_ERROR_002i1=未收到ready信号。关闭打印机，等待几分钟，再开启打印机
V_LSU_ERROR_002i2=如果此错误再次出现，请联系当地经销商
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
;V_GENERAL_ERROR=General error
V_GENERAL_ERRORc2=错误 No.:%s
;V_GENERAL_ERRORc2=Error No.:%s
V_GENERAL_ERRORi1=关闭打印机，等待几分钟，再开启打印机
;V_GENERAL_ERRORi1=Turn off the printer. Wait a few minutes, and then turn on the printer.
V_GENERAL_ERRORi2=如果此错误再次出现，请联系当地经销商
;V_GENERAL_ERRORi2=If this error occurs again, contact your dealer.
V_PRT_INTERRUPT=打印中断
;V_PRT_INTERRUPT=Printing interrupted
V_PRT_INTERRUPTi1=关闭打印机，检查所有电缆的连接，并重新开启打印机
;V_PRT_INTERRUPTi1=Turn off the printer and check all cable connections. Then turn on the printer.
V_PRT_INTERRUPTi2=请单击“取消”按钮，取消打印任务
;V_PRT_INTERRUPTi2=Click Cancel Printing to cancel the print job.
V_ERR_OTHER_PC=打印从另一台计算机发送的数据时出现错误
;V_ERR_OTHER_PC=Error occurred while printing data from another computer
V_ERR_OTHER_PCi1=请等待直到错误清除
;V_ERR_OTHER_PCi1=Please wait until the error is cleared.
V_OTHER_PC_PRINT=正在打印不同的文件
;V_OTHER_PC_PRINT=Printing the different document
V_OTHER_PC_PRINTi1=请等待直到打印完成
;V_OTHER_PC_PRINTi1=Please wait until printing is finished.
V_ERR_OTHER_PORT=打印从另一个端口发送的数据时出现错误
;V_ERR_OTHER_PORT=Error occurred while printing data from another port
V_ERR_OTHER_PORTi1=请等待直到错误清除
;V_ERR_OTHER_PORTi1=Please wait until the error is cleared.
V_UNKNOWN_ERROR=未知错误
;V_UNKNOWN_ERROR=Unknown error
V_UNKNOWN_ERRORi1=请检查打印机
;V_UNKNOWN_ERRORi1=Check the printer.
V_COMM_ERROR=通讯错误
;V_COMM_ERROR=Communication error
V_COMM_ERRORi1=请检查所有的电缆连接并确定打印机已打开
;V_COMM_ERRORi1=Check all cable connections and make sure the printer is on.
V_S_CONFIRM_ERR=状态确认错误
;V_S_CONFIRM_ERR=Status confirmation error
V_S_CONFIRM_ERRi1=确认所有的电缆连接正确，并且确认打印机已打开
;V_S_CONFIRM_ERRi1=Check all cable connections and make sure the printer is on.
V_S_CONFIRM_ERRi2=当一个打印任务进行了很长时间时会出现此消息，此消息会在打印完成后消失。
;V_S_CONFIRM_ERRi2=This message can appear when a print job takes a long time to process. This message clears when printing finishes.
V_S_CONFIRM_ERRi3=检查打印机状态，确认打印没有因其他错误停止
;V_S_CONFIRM_ERRi3=Check the printer status to make sure printing has not stopped due to another error.
V_DIFF_DEVICE=非列表中设备
;V_DIFF_DEVICE=Different device from specified
V_DIFF_DEVICEi1=尝试连接列表中没有的设备，请检查驱动程序和设备
;V_DIFF_DEVICEi1=Attempting to connect to a different device from that specified in the driver. Check the driver and the device.

V_SEARCHING=搜索中...
;V_SEARCHING=Searching
V_SEARCHINGi1=请等待...
;V_SEARCHINGi1=Please wait.
V_DRUM_END=硒鼓已到使用寿命
;V_DRUM_END=Drum end of life
V_DRUM_ENDi1=打开顶盖并更换硒鼓
;V_DRUM_ENDi1=Open the top cover, then replace the drum unit.
V_INCORRECT_MEDI=纸张类型不正确
;V_INCORRECT_MEDI=Incorrect media type
V_INCORRECT_MEDIi1=打印机驱动中所选的纸张类型与实际装入的纸张类型不符
;V_INCORRECT_MEDIi1=The media type selected in the printer driver does not match the media type that is loaded.
V_INCORRECT_MEDIi2=请单击“继续”按钮，继续打印
;V_INCORRECT_MEDIi2=Click Continue to resume printing.
V_INCORRECT_MEDIi3=请单击“取消”按钮，取消打印任务
;V_INCORRECT_MEDIi3=Click Cancel Printing to cancel the print job.
V_FATAL_ERROR=严重错误
;V_FATAL_ERROR=Fatal error
V_FATAL_ERRORc2=错误 No.:%s
;V_FATAL_ERRORc2=Error No.:%s
V_FATAL_ERRORi1=关闭打印机，请等待几分钟，然后打开打印机
;V_FATAL_ERRORi1=Turn off the printer. Wait a few minutes, and then turn on the printer.
V_FATAL_ERRORi2=如果此错误再次出现，请联系当地经销商
;V_FATAL_ERRORi2=If this error occurs again, contact your dealer.
V_CST_N_PAPER=送纸错误
;V_CST_N_PAPER=Misfeed
V_CST_N_PAPERi1=请检查纸仓中的纸
;V_CST_N_PAPERi1=Check the paper in cassette .
V_CST_N_PAPERi2=打开并关闭顶盖
;V_CST_N_PAPERi2=Open and close the cover.
V_MAN_N_PAPER=无纸
;V_MAN_N_PAPER=No Paper
V_MAN_N_PAPERi1=纸盒支持A4、B5（JIS）和C16K三种纸型
V_MAN_N_PAPERi2=打印其他纸型请选择手动进纸方式并在手动进纸口放入纸张
;V_MAN_N_PAPERi1=Supply the paper in manual tray.
V_AUTO_N_PAPER=送纸错误
;V_AUTO_N_PAPER=Misfeed
V_AUTO_N_PAPERi1=请检查纸仓或手动进纸口的纸
;V_AUTO_N_PAPERi1=Check the paper in cassette or manual tray.
V_AUTO_N_PAPERi2=打开并关闭顶盖
;V_AUTO_N_PAPERi2=Open and close the cover.
V_PRINTER_BUSY=打印机正在工作中
;V_PRINTER_BUSY=Printer is busy.
V_PRINTER_BUSYi1=请等待...
;V_PRINTER_BUSYi1=Please wait.
V_TEST_MODE=测试模式
;V_TEST_MODE=Test mode
V_TEST_MODEi1=请等待直到测试模式结束
;V_TEST_MODEi1=Please wait until the test mode is cleared.
V_TEST_MODE_ERR=测试模式错误
;V_TEST_MODE_ERR=Test mode error
V_TEST_MODE_ERRi1=关闭打印机，等待几分钟后再开启打印机
;V_TEST_MODE_ERRi1=Turn off the printer. Wait a few minutes, and then turn on the printer.
V_OPC_N_END=硒鼓即将用完
;V_OPC_N_END=Process Cartridge Unit near end of service life
V_OPC_N_ENDi1=更换一个新硒鼓
;V_OPC_N_ENDi1=Prepare a new Process Cartridge Unit.
V_TONER_N_END=墨盒即将用完
;V_TONER_N_END=Toner Kit near end of service life
V_TONER_N_ENDi1=更换一个新墨盒
;V_TONER_N_ENDi1=Prepare a new Toner Kit.
V_PRINT_FAILURE=打印失败
;V_PRINT_FAILURE=Print Failure
V_PRINT_FAILUREi1=内存不足一页数据未能存储，导致打印失败
;V_PRINT_FAILUREi1=Printing was not successful since a data for one page was not saved due to an insufficient memory.
V_PRINT_FAILUREi2=请点击“关闭”按钮，继续打印下一页
;V_PRINT_FAILUREi2=Click Close to resume printing the next page.
V_INSTALL_TONER=请安装新硒鼓
;V_INSTALL_TONER=Install New Toner Cartridge
V_INSTALL_TONERi1=请等待...
;V_INSTALL_TONERi1=Please wait.
V_ENDOFMESSAGE=结束信息
;V_ENDOFMESSAGE=End of Message
V_ENDOFMESSAGEi1=退出
;V_ENDOFMESSAGEi1=Quit.

V_FINGER_OK=指纹操作成功
V_FINGER_FAIL=指纹操作失败
V_FINGER_NEEDSWEEP=请录入指纹
V_FINGER_ERRORIDENTIFY=该指纹不存在
V_FINGER_TEMPLATEEMPTY=选中的指纹不存在
V_FINGER_TEMPLATENOTEMPTY=选中的指纹不为空
V_FINGER_ALLTEMPLATEEMPTY=无存储指纹
V_FINGER_EMPTYIDNOEXIST=指纹存储已满
V_FINGER_DUPLICATIONID=该指纹已存在
V_FINGER_BADQUALITY=指纹图像质量不好
V_FINGER_TIMEOUT=指纹操作超时
V_FINGER_FPCANCEL=取消指纹操作
V_FINGER_INVALIDTEMPNO=选中的指纹不存在
V_FINGER_IDENTIFYSUCCESS=识别指纹成功
V_FINGER_REGISTERSUCCESS=注册指纹成功
V_FINGER_DELETESINGLESUCCESS=删除单个指纹成功
V_FINGER_DELETEALLSUCCESS=删除所有指纹成功
V_FINGER_NEEDRELEASE=请离开手指
V_FINGER_UARTERROR=指纹模块通讯错误
V_FINGER_IDENTIFYSUCCESSi1=

	 	
 	
[PI_MSG]	 	
;	 	
; status sheet	 	
;	 	
SS100mfg=二代打印机
;SS100mfg=Mercury
SS100=打印机信息
;SS100=Printer Information
SS101=打印机名
;SS101=Printer Name
SS102=标题
;SS102=Title
SS103=打印机设置
;SS103=Printer Setting
SS104=睡眠模式
;SS104=Sleep Mode
SS105=纸仓纸张尺寸
;SS105=Cassette Paper size
SS106=墨粉溢出错误
;SS106=Toner Out Error
SS107=总页数
;SS107=Total Pages
SS108=预置存储空间
;SS108=Installed Memory
SS109=通讯模式
;SS109=Communication Mode
SS110=高速
;SS110=High Speed
SS111=全速
;SS111=Full Speed
SS112=墨粉
;SS112=Toner
SS113=零件编号
;SS113=Part Number
SS114=硒鼓
;SS114=Process Cartridge
SS115=零件编号
;SS115=Part Number
SS116=立即需要
;SS116=Needed Soon
SS117=光
;SS117=Lights
SS117a=Paper Out, Paper Jam, Cover Open, and other errors.
;SS117a=Paper Out, Paper Jam, Cover Open, and other errors.
SS117b=参阅状态监视器详细资料
;SS117b=Check Status Monitor 3 for details.
SS117c=墨粉溢出或其他错误
;SS117c=Toner Out and other errors.
SS117d=参阅状态监视器详细资料
;SS117d=Check Status Monitor 3 for details.
SS117e=正在预热、接收数据
;SS117e=Warming Up, Receiving Data.
SS117f=耗材接近保养寿命
;SS117f=Consumables Near End of Service Life and other warnings.
SS117g=参阅状态监视器详细资料
;SS117g=Check Status Monitor 3 for details.

SS117h=其他光式样
;SS117h=Other light patterns:
SS117i=请您参阅打印机手册或状态监视器详细资料
;SS117i=See your printer's documentation or Status Monitor 3 for details.
SS118=信息
;SS118=Information
SS118a=安装了伪劣的硒鼓，使用伪劣硒鼓会影响打印质量
;SS118a=Non-genuine cartridge installed. Using a non-genuine cartridge may affect print quality.
SS118b=推荐使用光电原装硒鼓
;SS118b=Genuine Mercury cartridge recommended.
SS119=Controller Firmware Date
;SS119=控制器固件日期
SS120=Jam Counter
;SS120=Jam Counter
SS121=墨粉更换计数器
;SS121=Counter of changing of toner
SS122=劣质墨粉更换计数器
;SS122=Counter of changing of non-genuine toner
SS123=机器固件版本
;SS123=Engine Firmware Version
SS124=USB ID
SS125=耗材
;SS125=Consumables
SS130=天津光电集团
;SS130=PRIX CORPORATION
SS131=分钟
;SS131=Min
SS132=页
;SS132=Pages
SS133=MB
;SS133=MB
	 	
[DI_MSG]	 	
;	 	
; Setting Information	 	
;	 	
SI200mfg=二代打印机
;SI200mfg=Mercury
SI200=驱动程序信息
;SI200=Driver Information
SI201=布局
;SI201=Layout
SI202=定向
;SI202=Orientation
SI203=肖像
;SI203=Portrait
SI204=风景
;SI204=Landscape
SI205=打印顺序
;SI205=Page Order
SI206=从前到后
;SI206=Front to Back
SI207=从后到前
;SI207=Back to Front
SI208=每张打印页数
;SI208=Pages Per Sheet
SI209=页
;SI209=pages
SI210=打印结构
;SI210=Print the Frame
SI211=打印顺序
;SI211=Print Order
SI212=纸张/质量
;SI212=Paper/Quality
SI213=纸张来源
;SI213=Paper Source
SI214=纸张类型
;SI214=Media
SI215=高级
;SI215=Advanced
SI216=纸张/输出
;SI216=Paper/Output
SI217=纸张尺寸
;SI217=Paper Size
SI218=份数
;SI218=Copy Count
SI219=比较
;SI219=Collated
SI220=图形
;SI220=Graphic
SI221=打印分辨率
;SI221=Print Quality
SI222=文档选项
;SI222=Document Options
SI223=高级打印功能
;SI223=Advanced printing features
SI224=半色调
;SI224=Halftoning
SI225=明亮度
;SI225=Brightness
SI226=剩余墨粉量
;SI226=Toner Save
SI227=缩放选项
;SI227=Zoom Options
SI228=输出纸张
;SI228=Output Paper
SI229=缩放到
;SI229=Zoom To
SI230=缩放比例
;SI230=Zoom Ratio
SI231=位置
;SI231=Location
SI232=180度旋转
;SI232=Rotate by 180
SI233=可选设置
;SI233=Optional Settings
SI234=扩展设置
;SI234=Extended Settings
SI235=边距
;SI235=Offset
SI236=顶边距
;SI236=Top Offset
SI237=左边距
;SI237=Left Offset
SI238=跳过空白页
;SI238=Skip Blank Page
SI239=忽视选择的纸张尺寸
;SI239=Ignore the selected paper size
SI240=使用应用软件中指定的设置
;SI240=Uses the collate settings specified in the application
SI241=忽视内存溢出错误
;SI241=Avoid Insufficient Memroy Error
SI242=自动继续
;SI242=Auto Continue
SI243=监视打印状态
;SI243=Monitor the printing status
SI244=扩展的可打印区域
;SI244=Extended Printable Area
SI245=从打印服务器添加纸张尺寸
;SI245=Add the paper size provided by the print server
SI251=其他设置
;SI251=Other Options
SI252=海报打印
;SI252=Poster Printing
SI253=双面打印
;SI253=Double-Sided Printing
SI254=信纸头
;SI254=Letterhead
SI254a=布置
;SI254a=Placement
SI254b=文本
;SI254b=Text
SI254c=字体
;SI254c=Font
SI254d=大小
;SI254d=Size
SI254e=下划线
;SI254e=Underline
SI254f=加粗
;SI254f=Bold
SI254g=斜体
;SI254g=Italic
SI254h=失败
;SI254h=Strikeout
SI255=水印
;SI255=Watermark
SI255a=布置
;SI255a=Placement
SI255b=文本
;SI255b=Text
SI255c=字体
;SI255c=Font
SI255d=尺寸
;SI255d=Size
SI255e=颜色
;SI255e=Color
SI255f=强度
;SI255f=Intensity
SI255g=下划线
;SI255g=Underline
SI255h=加粗
;SI255h=Bold
SI255i=斜体
;SI255i=Italic
SI255j=边距
;SI255j=Offset
SI255k=角度
;SI255k=Angle
SI256=点数
;SI256=Points	 	
[ITEM]	 	
;-----< >-----	 	
iv700=用户定义尺寸...
;-----< >-----	 	
iv701=Off
iv702=On
iv703=每天一次
;-----< >-----	 	
iv706=Disable
iv707=Enable
;-----< Paper Size >-----	 	
iv711=A4 210 x 297 mm
iv712=A3 297 x 420 mm
iv713=A5 148 x 210 mm
iv714=B4 257 x 364 mm
iv715=B5 182 x 257 mm
iv716=LT 8.5 x 11 in
iv717=HLT 5.5 x 8.5 in
iv718=LGL 8.5 x 14 in
iv719=GLT 8 x 10.5 in
iv720=GLG 8.5 x 13 in
iv721=B 11 x 17 in
iv722=EXE 7.25 x 10.5 in
iv723=F4 210 x 330 mm
iv724=C16K 195 x 270 mm
;--- for World Wide Version ---	 	
iv725=MON 3.875 x 7.5 in
iv726=C10 4.125 x 9.5 in
iv727=DL 110 x 220 mm
iv728=C5 162 x 229 mm
iv729=C6 114 x 162 mm
iv730=IB5 176 x 250 mm
;--- for Japanese Version ---	 	
iv731=J O Postcard 100 x 148 mm
iv732=J W Postcard 148 x 200 mm
iv733=J 4-sided Postcard 200 x 296 mm
iv734=Youkei #0 120 x 135 mm
iv735=Youkei #4 105 x 135 mm
iv736=Youkei #6 98 x 190 mm
iv737=Choukei #3 120 x 235 mm
iv738=Kakukei #3 216 x 277 mm
;--- Common Paper ---	 	
iv739=A3F 311.2 x 457.2 mm
iv740=A3Wide 328 x 453 mm
iv741=FREE
iv742=FREE
iv743=FREE
iv744=FREE
iv745=FREE
iv746=FREE
iv747=FREE
iv748=FREE
iv749=FREE
iv750=FREE
iv751=FREE
iv752=FREE
iv753=FREE
iv754=FREE
iv755=FREE
iv756=FREE
iv757=FREE
iv758=FREE
iv759=User Defined Size
iv760=User Defined Size (Min)
iv761=User Defined Size (Max)
;-----< Paper Size (short) >-----	 	
iv711s=A4
iv712s=A3
iv713s=A5
iv714s=B4
iv715s=B5 (JIS)
iv716s=Letter
iv717s=Half Letter
iv718s=Legal
iv719s=Govt-Letter
iv720s=Govt-Legal
iv721s=B
iv722s=Executive
iv723s=F4
iv724s=C16K
;--- for World Wide Version ---	 	
iv725s=Envelope Monarch
iv726s=Envelope #10
iv727s=Envelope DL
iv728s=Envelope C5
iv729s=Envelope C6
iv730s=ISO B5
;--- for Japanese Version ---	 	
iv731s=J O Postcard
iv732s=J W Postcard
iv733s=J 4-sided Postcard
iv734s=Youkei #0
iv735s=Youkei #4
iv736s=Youkei #6
iv737s=Choukei #3
iv738s=Kakukei #3
;--- Common Paper ---	 	
iv739s=A3F
iv740s=A3 Wide
iv741s=FREE
iv742s=FREE
iv743s=FREE
iv744s=FREE
iv745s=FREE
iv746s=FREE
iv747s=FREE
iv748s=FREE
iv749s=FREE
iv750s=FREE
iv751s=FREE
iv752s=FREE
iv753s=FREE
iv754s=FREE
iv755s=FREE
iv756s=FREE
iv757s=FREE
iv758s=USER
iv759s=USER(Min)
iv760s=USER(Max)
;-----< Paper Source >-----	 	
iv761=Auto
iv762=Cassette
iv763=Manual Tray
;-----< Paper Type >-----	 	
iv771=Plain
iv772=Thick-Wide
iv773=Thick-Narrow
;-----< >-----	 	
iv781=1
iv782=2
iv783=4
iv784=6
iv785=9
iv786=16
;-----< Resolution >-----	 	
iv791=600x600 dpi
iv792=300x300 dpi
iv793=1200x600 dpi
iv794=1200x1200 dpi
;-----< Dithering >-----	 	
iv795=None
iv796=Smooth
iv797=Normal
iv798=Sharp
;-----< Brightness >-----	 	
iv801=Lighter
iv802=较浅
iv803=正常
iv804=较深
iv805=Darker
;-----< Zoom Location >-----	 	
iv811=Upper Left
iv812=Center
;-----< >-----	 	
iv821=Off
iv822=5 min
iv823=15 min
iv824=30 min
iv825=60 min
iv826=120 min
iv827=180 min
iv828=240 min
;-----< >-----	 	
iv831=A4
iv832=信纸
;-----< >-----	 	
iv833=Continue
iv834=Stop
;-----< >-----	 	
iv835=Reset
iv836=Set
;	 	
; ---------- End of File ----------	 	
;	 	
