Protocol Settings - SNMP
This page allows you to configure the settings for SNMP.

Community Name (Read Only)
Enter the community name used for read-only access. You can enter a maximum of 31 bytes. The default is "public".
The password is displayed in 5 asterisks (*), regardless of whether it has already been set or not.
To enter a password, delete all the asterisks and then enter the password.
If the text box is left blank, the original setting will remain valid.

Community Name (Read/Write)
Enter the community names for read-write access. You can enter a maximum of 31 bytes.
The password is displayed in 5 asterisks (*), regardless of whether it has already been set or not.
To enter a password, delete all the asterisks and then enter the password.
If the text box is left blank, the original setting will remain valid.

Community Name (Trap Notification)
Enter the community name used for traps. You can enter a maximum of 31 bytes. The default is SNMP_trap.
The password is displayed in 5 asterisks (*), regardless of whether it has already been set or not.
To enter a password, delete all the asterisks and then enter the password.
If the text box is left blank, the original setting will remain valid.

Trap Notification (IP) 1-3
Notifies trap occurrences if the [Notify] check box is selected. If the check box is selected, enter the IP address and IP socket in the "aaa.bbb.ccc.ddd:eeeee" format. The "aaa", "bbb", and "ccc" must be the numbers between 0 and 255. However, "aaa" cannot be 127 or any number between 224 and 254. The "eeeee" (IP socket) must be any number between 0 and 65535.
If the check box is not selected, trap occurrences will not be notified, and the IP address you entered will reset to the default (0.0.0.0:0) when saved. The [Notify] check box is not selected by default.

Authentication Error Trap
Select the [Notify] check box to notify authentication error traps.

[Apply] button
[Undo] button