Create CSR

Overview
  This print server creates a CSR (Certificate Signing Request) to be issued by a certificate from a CA (Certificate Authority).
  After the CA issues a certificate, install the certificate in the page "Install Certificate."
  NOTE:
  When this printer creates a new certificate the old certificate is deleted.
  Install the certificate issued with the latest CSR for this printer.
Common Name
  Input common name for certificate(Required).
  The length of common name is less than 64 bytes.
  Enter an identifier such as an IP address, host name or domain name to use when accessing to this printer through SSL/TLS communication.
  The host name is displayed by default.
Organization
  Enter your organization, corporation or company (optional).
  The length of organization is less than 64 bytes.
Organization Unit
  Enter your department or division (optional).
  The length of organization unit is less than 64 bytes.
City/Locality
  Enter the city in which your organization is located (optional).
  The length of city/locality is less than 64 bytes.
State/Province
  Enter the state or province in which your organization is located (optional).
  The length of state/province is less than 64 bytes.
Country/Region
  Enter the country or region in which your organization is located (optional).
  The country should be an ISO 3166 country code composed of two characters.
Configure extended partition
SubjectAltName
Auto (Register IPv4)
  Register IPv4
Manual
  You must specify the type and value (e.g. DNS:www.brother.co.jp). Other supported types include email, URI, RID, IP, OtherName.
  The length of characters that you can input is up to 256 bytes for UTF8.
Public Key Algorithm
  Select Public key length.
  It is recommended that you select the default setting because it provides the strongest level of security. The other security settings are only recommended when the device does not support the strongest level of security.
  RSA(2048bit) : RSA 2048 bit key kength (default)
  RSA(1024bit) : RSA 1024 bit key length
Digest Algorithm
  Select Digest Algorithm for signature.
  It is recommended that you select the default setting because it provides the strongest level of security. The other security settings are only recommended when the device does not support the strongest level of security.
  SHA256 : SHA256 Digest Algorithm (default)
  SHA1 : SHA1 Digest Algorithm